(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DSC2033FI2-F0044"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DSC2033FI2-F0044"
				(at 35.56 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DSC2033FI2-F0044"
				(at 35.56 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/DSC2033%20Datasheet%20MKQBPD12042609-2.pdf"
				(at 35.56 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Level shifter"
				(at 35.56 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DSC2033FI2-F0044"
				(at 35.56 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 35.56 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DSC2033FI2-F0044_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "Enable")
					(number "1")
				)
				(pin no_connect line
					(at 19.05 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "")
					(number "2")
				)
				(pin no_connect line
					(at 19.05 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "")
					(number "3")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "FS0")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "FS1")
					(number "6")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "FS2")
					(number "7")
				)
				(pin output line
					(at 21.59 0 180)
					(length 2.54)
					(name "Output1+")
					(number "8")
				)
				(pin output line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "Output1-")
					(number "9")
				)
				(pin output line
					(at 21.59 -7.62 180)
					(length 2.54)
					(name "Output2-")
					(number "10")
				)
				(pin output line
					(at 21.59 -5.08 180)
					(length 2.54)
					(name "Output2+")
					(number "11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD2")
					(number "12")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "13")
				)
			)
			(embedded_fonts no)
		)
)
