(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DSC557-0343FI1"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DSC557-0343FI1"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DSC557-0343FI1"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/TCG/ProductDocuments/DataSheets/DSC557-03-04-05-Multiple-Output-MEMS-PCIe-Gen1-2-3-4-Clock-Generators-DS20006691.pdf"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Two output PCIe Clock Generator"
				(at 45.72 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DSC557-0343FI1"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Val" "100 MHz"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, IC, CLOCK, PCIE"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DSC557-0343FI1_0_1")
			(symbol "DSC557-0343FI1_1_1"
				(text "LVDS"
					(at 12.7 -2.54 0)
				)
				(text "HCSL"
					(at 12.7 -10.16 0)
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "OE")
					(number "1")
				)
				(pin no_connect line
					(at 11.43 -15.24 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin no_connect line
					(at 12.7 -15.24 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "3")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin no_connect line
					(at 13.97 -15.24 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 15.24 -15.24 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin no_connect line
					(at 16.51 -15.24 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin output line
					(at 26.67 -8.89 180)
					(length 2.54)
					(name "CLK1+")
					(number "8")
				)
				(pin output line
					(at 26.67 -11.43 180)
					(length 2.54)
					(name "CLK1-")
					(number "9")
				)
				(pin output line
					(at 26.67 -3.81 180)
					(length 2.54)
					(name "CLK0-")
					(number "10")
				)
				(pin output line
					(at 26.67 -1.27 180)
					(length 2.54)
					(name "CLK0+")
					(number "11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD1")
					(number "12")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD0")
					(number "13")
				)
				(pin no_connect line
					(at 17.78 -15.24 90)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 2.54)
					(name "EPAD")
					(number "15")
				)
			)
			(embedded_fonts no)
		)
)
