(footprint "VQFN-14-1EP_3.2x2.5mm_P0.5mm_Layout4x3"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -2.4 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "VQFN-14-1EP_3.2x2.5mm_P0.5mm_Layout4x3"
		(at 0 3.1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -1.746 5.099 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -1.746 6.299 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -1.746 7.499 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -1.3 -0.762 90)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -1.3 -0.25 90)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -1.3 0.25 90)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -1.3 0.75 90)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -0.5 1.65)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 0 1.65)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 0.5 1.65)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 1.3 0.75 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 1.3 0.25 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at 1.3 -0.25 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at 1.3 -0.75 270)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at 0.5 -1.65 180)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at 0 -1.65 180)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -0.5 -1.65 180)
		(size 0.3 0.7)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd roundrect
		(at 0.003 0 90)
		(size 2.1 1.4)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0)
		(chamfer_ratio 0.2)
		(chamfer top_right)
	)
	(embedded_fonts no)
	(model "antmicro_dsc557_0344fi0t.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
