(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "DW1000-I-TR13"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 63.5 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "DW1000-I-TR13"
				(at 63.5 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "DW1000-I-TR13"
				(at 63.5 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.decawave.com/sites/default/files/resources/DW1000-Datasheet-V2.12.pdf"
				(at 63.5 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF transceiver IC"
				(at 63.5 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "DecaWave"
				(at 63.5 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "DW1000-I-TR13"
				(at 63.5 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 63.5 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 63.5 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "DW1000-I-TR13_1_1"
				(pin no_connect line
					(at 48.26 -73.66 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "1")
				)
				(pin no_connect line
					(at 48.26 -76.2 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "2")
				)
				(pin input line
					(at 50.8 -63.5 180)
					(length 2.54)
					(name "EXTCLK/XTAL1")
					(number "3")
				)
				(pin input line
					(at 50.8 -71.12 180)
					(length 2.54)
					(name "XTAL2")
					(number "4")
				)
				(pin bidirectional line
					(at 50.8 -58.42 180)
					(length 2.54)
					(name "VREF")
					(number "5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDMS")
					(number "6")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDIF")
					(number "7")
				)
				(pin bidirectional line
					(at 50.8 -48.26 180)
					(length 2.54)
					(name "CLKTUNE")
					(number "8")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDDCLK")
					(number "9")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDDSYN")
					(number "10")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDDVCO")
					(number "11")
				)
				(pin bidirectional line
					(at 50.8 -53.34 180)
					(length 2.54)
					(name "VCOTUNE")
					(number "12")
				)
				(pin no_connect line
					(at 48.26 -78.74 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin no_connect line
					(at 48.26 -81.28 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VDDLNA")
					(number "15")
				)
				(pin bidirectional line
					(at 50.8 0 180)
					(length 2.54)
					(name "RF_P")
					(number "16")
				)
				(pin bidirectional line
					(at 50.8 -5.08 180)
					(length 2.54)
					(name "RF_N")
					(number "17")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VDDPA1")
					(number "18")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VDDPA2")
					(number "19")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "VDDREG")
					(number "20")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 2.54)
					(name "EXTON")
					(number "21")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 2.54)
					(name "FORCEON")
					(number "22")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 2.54)
					(name "WAKEUP")
					(number "23")
				)
				(pin input line
					(at 0 -83.82 0)
					(length 2.54)
					(name "~{SPICS}")
					(number "24")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 2.54)
					(name "VDDAON")
					(number "25")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "VDDLDOD")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "~{RST}")
					(number "27")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 2.54)
					(name "VDDIOA")
					(number "28")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 2.54)
					(name "SYNC/GPIO7")
					(number "29")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 2.54)
					(name "GPIO6/EXTRXE/SPIPHA")
					(number "30")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 2.54)
					(name "VDDIO")
					(number "31")
				)
				(pin power_in line
					(at 50.8 -86.36 180)
					(length 2.54)
					(name "VSSIO")
					(number "32")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 2.54)
					(name "GPIO5/EXTTXE/SPIPOL")
					(number "33")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 2.54)
					(name "GPIO4/EXTPA")
					(number "34")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 2.54)
					(name "GPIO3/TXLED")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 2.54)
					(name "GPIO2/RXLED")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 2.54)
					(name "GPIO1/SFDLED")
					(number "37")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 2.54)
					(name "GPIO0/RXOKLED")
					(number "38")
				)
				(pin input line
					(at 0 -88.9 0)
					(length 2.54)
					(name "SPIMOSI")
					(number "39")
				)
				(pin output line
					(at 0 -86.36 0)
					(length 2.54)
					(name "SPIMISO")
					(number "40")
				)
				(pin input line
					(at 0 -81.28 0)
					(length 2.54)
					(name "SPICLK")
					(number "41")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 2.54)
					(hide yes)
					(name "VDDIO")
					(number "42")
				)
				(pin passive line
					(at 50.8 -86.36 180)
					(length 2.54)
					(hide yes)
					(name "VSSIO")
					(number "43")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 2.54)
					(name "VDDDIG")
					(number "44")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 2.54)
					(name "IRQ/GPIO8")
					(number "45")
				)
				(pin input line
					(at 50.8 -83.82 180)
					(length 2.54)
					(name "TESTMODE")
					(number "46")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 2.54)
					(name "VDDBATT")
					(number "47")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 2.54)
					(name "VDDLDOA")
					(number "48")
				)
				(pin power_in line
					(at 50.8 -88.9 180)
					(length 2.54)
					(name "GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
