(footprint "BGA-169-120_7x7mm_Layout13x13_P0.5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.9 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-169-120_7x7mm_Layout13x13_P0.5mm"
		(at 0 4.7 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -3.505 7.299 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -3.505 8.499 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -3.505 9.698 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -3 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -2.5 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -2 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -1.5 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -1 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd circle
		(at -0.5 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd circle
		(at 0 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 0.498 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 0.998 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at 1.499 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 1.999 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at 2.499 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd circle
		(at 2.999 -3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -3 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -2.5 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -2 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -1.5 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -1 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -0.5 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at 0 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 0.498 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 0.998 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 1.499 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at 1.999 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at 2.499 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at 2.999 -2.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -3 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -2.5 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -2 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -1.5 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -1 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C6" smd circle
		(at -0.5 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C7" smd circle
		(at 0 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 0.498 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at 0.998 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at 1.499 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at 1.999 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at 2.499 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C13" smd circle
		(at 2.999 -2)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -3 -1.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -2.5 -1.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -2 -1.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at 1.999 -1.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at 2.499 -1.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at 2.999 -1.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -3 -1)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -2.5 -1)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -2 -1)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at 1.999 -1)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E12" smd circle
		(at 2.499 -1)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E13" smd circle
		(at 2.999 -1)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -3 -0.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -2.5 -0.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -2 -0.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at 1.999 -0.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F12" smd circle
		(at 2.499 -0.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F13" smd circle
		(at 2.999 -0.5)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -3 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -2.5 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -2 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at 1.999 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at 2.499 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G13" smd circle
		(at 2.999 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -3 0.498)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -2.5 0.498)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -2 0.498)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 1.999 0.498)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at 2.499 0.498)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at 2.999 0.498)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -3 0.998)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -2.5 0.998)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -2 0.998)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at 1.999 0.998)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at 2.499 0.998)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at 2.999 0.998)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -3 1.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -2.5 1.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -2 1.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at 1.999 1.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at 2.499 1.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K13" smd circle
		(at 2.999 1.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd circle
		(at -3 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -2.5 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L3" smd circle
		(at -2 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -1.5 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -1 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L6" smd circle
		(at -0.5 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L7" smd circle
		(at 0 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at 0.498 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at 0.998 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L10" smd circle
		(at 1.499 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L11" smd circle
		(at 1.999 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L12" smd circle
		(at 2.499 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L13" smd circle
		(at 2.999 1.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd circle
		(at -3 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -2.5 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M3" smd circle
		(at -2 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -1.5 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M5" smd circle
		(at -1 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M6" smd circle
		(at -0.5 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M7" smd circle
		(at 0 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at 0.498 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at 0.998 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M10" smd circle
		(at 1.499 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M11" smd circle
		(at 1.999 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M12" smd circle
		(at 2.499 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M13" smd circle
		(at 2.999 2.499)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -3 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -2.5 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -2 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -1.5 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N5" smd circle
		(at -1 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N6" smd circle
		(at -0.5 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N7" smd circle
		(at 0 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at 0.498 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at 0.998 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N10" smd circle
		(at 1.499 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N11" smd circle
		(at 1.999 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N12" smd circle
		(at 2.499 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N13" smd circle
		(at 2.999 2.999)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_efm32gg12b410f1024gl120_ar.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
