(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EFM32GG12B410F1024_BGA"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EFM32GG12B410F1024_BGA"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EFM32GG12B410F1024_BGA"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/368/efm32gg12_datasheet-1548213.pdf"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, EFM32 Family EFM32GG Series Microcontrollers, ARM Cortex-M4, 32 bit, 72 MHz, 1 MB"
				(at 43.18 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EFM32GG12B410F1024GL120-AR"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Silicon Labs"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "ARM, MCU, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "BGA120_SIL"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EFM32GG12B410F1024_BGA_1_1"
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VREGI")
					(number "A11")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VREGO")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PA15")
					(number "B1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VBUS")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PA1")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PA0")
					(number "C2")
				)
				(pin power_in line
					(at 0 -78.74 0)
					(length 3.81)
					(name "VSS")
					(number "C5")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "IOVDD1")
					(number "C6")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "C8")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "IOVDD0")
					(number "C9")
				)
				(pin bidirectional line
					(at 24.13 -76.2 180)
					(length 3.81)
					(name "PC14")
					(number "C12")
				)
				(pin bidirectional line
					(at 24.13 -78.74 180)
					(length 3.81)
					(name "PC15")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PA3")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PA2")
					(number "D2")
				)
				(pin bidirectional line
					(at 24.13 -38.1 180)
					(length 3.81)
					(name "PB15")
					(number "D3")
				)
				(pin bidirectional line
					(at 24.13 -71.12 180)
					(length 3.81)
					(name "PC12")
					(number "D12")
				)
				(pin bidirectional line
					(at 24.13 -73.66 180)
					(length 3.81)
					(name "PC13")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PA6")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PA5")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PA4")
					(number "E3")
				)
				(pin bidirectional line
					(at 24.13 -66.04 180)
					(length 3.81)
					(name "PC10")
					(number "E12")
				)
				(pin bidirectional line
					(at 24.13 -68.58 180)
					(length 3.81)
					(name "PC11")
					(number "E13")
				)
				(pin bidirectional line
					(at 24.13 0 180)
					(length 3.81)
					(name "PB0")
					(number "F1")
				)
				(pin bidirectional line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "PB1")
					(number "F2")
				)
				(pin bidirectional line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "PB2")
					(number "F3")
				)
				(pin bidirectional line
					(at 24.13 -60.96 180)
					(length 3.81)
					(name "PC8")
					(number "F12")
				)
				(pin bidirectional line
					(at 24.13 -63.5 180)
					(length 3.81)
					(name "PC9")
					(number "F13")
				)
				(pin bidirectional line
					(at 24.13 -7.62 180)
					(length 3.81)
					(name "PB3")
					(number "G1")
				)
				(pin bidirectional line
					(at 24.13 -10.16 180)
					(length 3.81)
					(name "PB4")
					(number "G2")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "IOVDD2")
					(number "G3")
				)
				(pin bidirectional line
					(at 24.13 -12.7 180)
					(length 3.81)
					(name "PB5")
					(number "H1")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 3.81)
					(name "PB6")
					(number "H2")
				)
				(pin bidirectional line
					(at 24.13 -58.42 180)
					(length 3.81)
					(name "PC7")
					(number "H13")
				)
				(pin bidirectional line
					(at 24.13 -55.88 180)
					(length 3.81)
					(name "PC6")
					(number "J12")
				)
				(pin bidirectional line
					(at 24.13 -40.64 180)
					(length 3.81)
					(name "PC0")
					(number "K1")
				)
				(pin bidirectional line
					(at 24.13 -50.8 180)
					(length 3.81)
					(name "PC1")
					(number "K2")
				)
				(pin bidirectional line
					(at 24.13 -43.18 180)
					(length 3.81)
					(name "PC2")
					(number "L1")
				)
				(pin bidirectional line
					(at 24.13 -45.72 180)
					(length 3.81)
					(name "PC3")
					(number "L2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PA7")
					(number "L3")
				)
				(pin bidirectional line
					(at 24.13 -22.86 180)
					(length 3.81)
					(name "PB9")
					(number "L8")
				)
				(pin bidirectional line
					(at 24.13 -25.4 180)
					(length 3.81)
					(name "PB10")
					(number "L9")
				)
				(pin bidirectional line
					(at 24.13 -17.78 180)
					(length 3.81)
					(name "PB7")
					(number "M1")
				)
				(pin bidirectional line
					(at 24.13 -48.26 180)
					(length 3.81)
					(name "PC4")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PA8")
					(number "M3")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PA10")
					(number "M4")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PA13")
					(number "M5")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PA14")
					(number "M6")
				)
				(pin bidirectional line
					(at 24.13 -20.32 180)
					(length 3.81)
					(name "PB8")
					(number "N1")
				)
				(pin bidirectional line
					(at 24.13 -53.34 180)
					(length 3.81)
					(name "PC5")
					(number "N2")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PA9")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PA11")
					(number "N4")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PA12")
					(number "N5")
				)
				(pin bidirectional line
					(at 24.13 -27.94 180)
					(length 3.81)
					(name "PB11")
					(number "N6")
				)
				(pin bidirectional line
					(at 24.13 -30.48 180)
					(length 3.81)
					(name "PB12")
					(number "N7")
				)
				(pin bidirectional line
					(at 24.13 -33.02 180)
					(length 3.81)
					(name "PB13")
					(number "N9")
				)
				(pin bidirectional line
					(at 24.13 -35.56 180)
					(length 3.81)
					(name "PB14")
					(number "N10")
				)
			)
			(symbol "EFM32GG12B410F1024_BGA_2_1"
				(pin bidirectional line
					(at 24.13 -38.1 180)
					(length 3.81)
					(name "PE15")
					(number "A1")
				)
				(pin bidirectional line
					(at 24.13 -35.56 180)
					(length 3.81)
					(name "PE14")
					(number "A2")
				)
				(pin bidirectional line
					(at 24.13 -30.48 180)
					(length 3.81)
					(name "PE12")
					(number "A3")
				)
				(pin bidirectional line
					(at 24.13 -22.86 180)
					(length 3.81)
					(name "PE9")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PD11")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PD9")
					(number "A6")
				)
				(pin bidirectional line
					(at 24.13 -58.42 180)
					(length 3.81)
					(name "PF7")
					(number "A7")
				)
				(pin bidirectional line
					(at 24.13 -53.34 180)
					(length 3.81)
					(name "PF5")
					(number "A8")
				)
				(pin bidirectional line
					(at 24.13 -50.8 180)
					(length 3.81)
					(name "PF4")
					(number "A9")
				)
				(pin bidirectional line
					(at 24.13 -45.72 180)
					(length 3.81)
					(name "PF2")
					(number "A10")
				)
				(pin bidirectional line
					(at 24.13 -68.58 180)
					(length 3.81)
					(name "PF11")
					(number "A13")
				)
				(pin bidirectional line
					(at 24.13 -33.02 180)
					(length 3.81)
					(name "PE13")
					(number "B2")
				)
				(pin bidirectional line
					(at 24.13 -27.94 180)
					(length 3.81)
					(name "PE11")
					(number "B3")
				)
				(pin bidirectional line
					(at 24.13 -20.32 180)
					(length 3.81)
					(name "PE8")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PD12")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PD10")
					(number "B6")
				)
				(pin bidirectional line
					(at 24.13 -60.96 180)
					(length 3.81)
					(name "PF8")
					(number "B7")
				)
				(pin bidirectional line
					(at 24.13 -55.88 180)
					(length 3.81)
					(name "PF6")
					(number "B8")
				)
				(pin bidirectional line
					(at 24.13 -48.26 180)
					(length 3.81)
					(name "PF3")
					(number "B9")
				)
				(pin bidirectional line
					(at 24.13 -43.18 180)
					(length 3.81)
					(name "PF1")
					(number "B10")
				)
				(pin bidirectional line
					(at 24.13 -71.12 180)
					(length 3.81)
					(name "PF12")
					(number "B11")
				)
				(pin bidirectional line
					(at 24.13 -66.04 180)
					(length 3.81)
					(name "PF10")
					(number "B13")
				)
				(pin bidirectional line
					(at 24.13 -25.4 180)
					(length 3.81)
					(name "PE10")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PD13")
					(number "C4")
				)
				(pin bidirectional line
					(at 24.13 -63.5 180)
					(length 3.81)
					(name "PF9")
					(number "C7")
				)
				(pin bidirectional line
					(at 24.13 -40.64 180)
					(length 3.81)
					(name "PF0")
					(number "C10")
				)
				(pin bidirectional line
					(at 24.13 -10.16 180)
					(length 3.81)
					(name "PE4")
					(number "C11")
				)
				(pin bidirectional line
					(at 24.13 -12.7 180)
					(length 3.81)
					(name "PE5")
					(number "D11")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 3.81)
					(name "PE6")
					(number "E11")
				)
				(pin bidirectional line
					(at 24.13 -17.78 180)
					(length 3.81)
					(name "PE7")
					(number "F11")
				)
				(pin bidirectional line
					(at 24.13 0 180)
					(length 3.81)
					(name "PE0")
					(number "G11")
				)
				(pin bidirectional line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "PE1")
					(number "G12")
				)
				(pin bidirectional line
					(at 24.13 -7.62 180)
					(length 3.81)
					(name "PE3")
					(number "G13")
				)
				(pin power_in line
					(at 0 -71.12 0)
					(length 3.81)
					(name "VSS")
					(number "H3")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "DVDD")
					(number "H11")
				)
				(pin bidirectional line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "PE2")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PD14")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PD15")
					(number "J2")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "IOVDD0")
					(number "J11")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DECOUPLE")
					(number "J13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "IOVDD0")
					(number "K3")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K11")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K12")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PD8")
					(number "K13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "IOVDD0")
					(number "L4")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L5")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "L6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "IOVDD0")
					(number "L7")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PD0")
					(number "L10")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PD1")
					(number "L11")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PD4")
					(number "L12")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PD7")
					(number "L13")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "RESETn")
					(number "M7")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDD")
					(number "M9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "AVDD")
					(number "M10")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M11")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PD3")
					(number "M12")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PD6")
					(number "M13")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDD")
					(number "N11")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PD2")
					(number "N12")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PD5")
					(number "N13")
				)
			)
			(embedded_fonts no)
		)
)
