(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EFM8SB10F2G-A-QFN20"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EFM8SB10F2G-A-QFN20"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EFM8SB10F2G-A-QFN20"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/3/340/1/efm8sb1-datasheet.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "8bit CIP-51 Microcontroller, 25MHz, 2 kB Flash, 20-Pin QFN"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Silicon Labs"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EFM8SB10F2G-A-QFN20"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EFM8SB10F2G-A-QFN20_1_1"
				(pin bidirectional line
					(at 22.86 -6.35 180)
					(length 2.54)
					(name "P0.1")
					(number "1")
					(alternate "AGND" passive line)
					(alternate "INT0.1" input line)
					(alternate "INT1.1" input line)
				)
				(pin bidirectional line
					(at 22.86 -3.81 180)
					(length 2.54)
					(name "P0.0")
					(number "2")
					(alternate "CS0.0" input line)
					(alternate "VREF" passive line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "4")
				)
				(pin input line
					(at 22.86 -1.27 180)
					(length 2.54)
					(name "~{RSTB}")
					(number "5")
					(alternate "C2CK" input line)
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "P2.7")
					(number "6")
					(alternate "C2D" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 2.54)
					(name "P1.7")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 2.54)
					(name "P1.6")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 2.54)
					(name "P1.5")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 2.54)
					(name "P1.3")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "P1.2")
					(number "11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "GND")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 2.54)
					(name "P1.1")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 2.54)
					(name "P1.0")
					(number "14")
				)
				(pin bidirectional line
					(at 22.86 -21.59 180)
					(length 2.54)
					(name "P0.7")
					(number "15")
				)
				(pin bidirectional line
					(at 22.86 -19.05 180)
					(length 2.54)
					(name "P0.6")
					(number "16")
				)
				(pin bidirectional line
					(at 22.86 -16.51 180)
					(length 2.54)
					(name "P0.5")
					(number "17")
				)
				(pin bidirectional line
					(at 22.86 -13.97 180)
					(length 2.54)
					(name "P0.4")
					(number "18")
				)
				(pin bidirectional line
					(at 22.86 -11.43 180)
					(length 2.54)
					(name "P0.3")
					(number "19")
				)
				(pin bidirectional line
					(at 22.86 -8.89 180)
					(length 2.54)
					(name "P0.2")
					(number "20")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "21")
				)
			)
			(embedded_fonts no)
		)
)
