(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EIC7700X"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 93.218 -3.302 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EIC7700X"
				(at 93.218 -8.382 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EIC7700X"
				(at 93.218 -10.922 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.sifive.com/document-file/eic7700x-datasheet"
				(at 93.218 -13.462 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SoC with a Quad-Core SiFive P550 64-bit Out-of-Order CPU cluster, 32GB PLDDR5 RAM, 19.95 TOPS NPU"
				(at 93.218 -26.162 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "ESWIN"
				(at 93.218 -18.542 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EIC7700X"
				(at 93.218 -5.842 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 93.218 -21.082 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 93.218 -23.622 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, BGA, SOC, MICROPROCESSOR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EIC7700X_1_1"
				(pin power_in line
					(at 0 -60.96 0)
					(length 5.08)
					(name "VSS")
					(number "A1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "A34")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA6")
				)
				(pin power_in line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "VDDIO18")
					(number "AA7")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AA8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA10")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD_CPU")
					(number "AA11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AA12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA20")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDD_SOC")
					(number "AA21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AA22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA24")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AA25")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AA26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AA32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB6")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AB7")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AB8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AB11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AB12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AB14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB15")
				)
				(pin power_in line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "VDD18_POR")
					(number "AB16")
				)
				(pin power_in line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "AVDDHV_PLL")
					(number "AB17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AB19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB20")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AB21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AB22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB24")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AB25")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AB26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC8")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AC9")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AC10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AC13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AC14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC16")
				)
				(pin passive line
					(at 45.72 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "AVDDHV_PLL")
					(number "AC17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC18")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AC19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC20")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AC21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "AC22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC31")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD8")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AD9")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AD10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AD13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AD14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD15")
				)
				(pin power_in line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "VPH_PCIE")
					(number "AD16")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(hide yes)
					(name "VPH_PCIE")
					(number "AD17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD23")
				)
				(pin power_in line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "VPH_CSI01")
					(number "AD24")
				)
				(pin power_in line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "VPH_CSI23")
					(number "AD25")
				)
				(pin power_in line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "VPH_CSI45")
					(number "AD26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD31")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AD32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE6")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AE7")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AE8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AE11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AE12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AE14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE15")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VP_PCIE")
					(number "AE16")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(hide yes)
					(name "VP_PCIE")
					(number "AE17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE18")
				)
				(pin power_in line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "VPH_HDMI")
					(number "AE19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE20")
				)
				(pin power_in line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "VPH_DSI")
					(number "AE21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE22")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VP_CSI01")
					(number "AE23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE24")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 5.08)
					(name "VP_CSI23")
					(number "AE25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE26")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "VP_CSI45")
					(number "AE27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE33")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AE34")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF6")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AF7")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AF8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AF11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AF12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF14")
				)
				(pin power_in line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "VDDIO_OTP")
					(number "AF15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF18")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 5.08)
					(name "VP_HDMI")
					(number "AF19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF20")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VP_DSI")
					(number "AF21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "VP_CSI01")
					(number "AF23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF24")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "VP_CSI23")
					(number "AF25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF26")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(hide yes)
					(name "VP_CSI45")
					(number "AF27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AF32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG6")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AG7")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AG8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AG11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AG12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AG32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH6")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AH7")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "AH8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH10")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AH11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD_CPU")
					(number "AH12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AH32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AJ32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AK3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AK6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AK9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AK12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AK20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AK29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AK32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AL16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AL18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AL20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AL32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM31")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AM32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AN1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AN9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AN11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AN14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AN20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AN34")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AP1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AP2")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AP9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AP11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AP14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AP20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AP34")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "B1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E31")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E33")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G7")
				)
				(pin power_in line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "VPH_SATA")
					(number "G8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G24")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 5.08)
					(name "VAA_VDD2H_LPDDR0")
					(number "G25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H9")
				)
				(pin power_in line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "VDDIO33_USB")
					(number "H10")
				)
				(pin passive line
					(at 45.72 -50.8 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO33_USB")
					(number "H11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H21")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "VDD2H_LPDDR")
					(number "H22")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VDD2H_LPDDR")
					(number "H23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H24")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VDD2H_LPDDR")
					(number "H25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H26")
				)
				(pin power_in line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "VSSA_PVT_DDR")
					(number "H28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J6")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 5.08)
					(name "VP_SATA")
					(number "J7")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 5.08)
					(name "VPTX_SATA")
					(number "J8")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 5.08)
					(name "VP_USB0")
					(number "J9")
				)
				(pin power_in line
					(at 0 -48.26 0)
					(length 5.08)
					(name "VPTX_USB0")
					(number "J10")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 5.08)
					(name "VP_USB1")
					(number "J11")
				)
				(pin power_in line
					(at 45.72 0 180)
					(length 5.08)
					(name "VPTX_USB1")
					(number "J12")
				)
				(pin power_in line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "VDDIO_EMMCSD")
					(number "J13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J14")
				)
				(pin power_in line
					(at 45.72 -53.34 180)
					(length 5.08)
					(name "VDDIO33_EMMCSD")
					(number "J15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J16")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "J17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J20")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VDDQ_LPDDR")
					(number "J21")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "J22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J23")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "J24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J27")
				)
				(pin power_in line
					(at 45.72 -35.56 180)
					(length 5.08)
					(name "VDD18_PVT_DDR")
					(number "J28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K9")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 5.08)
					(name "DVDD_USB0")
					(number "K10")
				)
				(pin power_in line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "DVDD_USB1")
					(number "K11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K12")
				)
				(pin passive line
					(at 45.72 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO_EMMCSD")
					(number "K13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K14")
				)
				(pin passive line
					(at 45.72 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO33_EMMCSD")
					(number "K15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K16")
				)
				(pin passive line
					(at 45.72 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18")
					(number "K17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K21")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "K22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K23")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "K24")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "K25")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "K26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K32")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "L4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "L5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "L7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "L8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDD_NPU")
					(number "L11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "L12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "L15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "L16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "L18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L19")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VDD_LPDDR")
					(number "L20")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "L21")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "L22")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "L23")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "L24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "L25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L27")
				)
				(pin passive line
					(at 45.72 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "AVDDHV_PLL")
					(number "L28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "M7")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "M8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "M11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "M12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "M15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "M16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "M18")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "M25")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "M26")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "M27")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VDD2H_LPDDR")
					(number "M28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M32")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "N4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "N5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "N9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "N10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "N13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "N14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N16")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "N17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "N25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N27")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VAA_VDD2H_LPDDR1")
					(number "N29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N31")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N32")
				)
				(pin power_in line
					(at 45.72 -45.72 180)
					(length 5.08)
					(name "VDDIO33_RGMII0")
					(number "P6")
				)
				(pin passive line
					(at 45.72 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO33_RGMII0")
					(number "P7")
				)
				(pin power_in line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "VDDIO18_RGMII")
					(number "P8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "P10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "P13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "P14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P16")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P19")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P22")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "P23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "P25")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "P26")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "P27")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VDD2H_LPDDR")
					(number "P28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R7")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18_RGMII")
					(number "R8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "R11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "R12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "R15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "R16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R19")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R22")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "R23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "R25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T3")
				)
				(pin power_in line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "VDDIO33_RGMII1")
					(number "T6")
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO33_RGMII1")
					(number "T7")
				)
				(pin passive line
					(at 45.72 -25.4 180)
					(length 5.08)
					(hide yes)
					(name "VDDIO18_RGMII")
					(number "T8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T10")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "T11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "T12")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T13")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T14")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "T15")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "T16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T19")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "T25")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "T26")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "T27")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VDD2H_LPDDR")
					(number "T28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T32")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "U4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "U5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "U9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "U10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "U13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "U14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U16")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U19")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U20")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "U22")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U23")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U24")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(hide yes)
					(name "VDD_LPDDR")
					(number "U25")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ_LPDDR")
					(number "U26")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "U32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V32")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "W4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "W5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W6")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "W7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "W9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "W10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "W13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "W14")
				)
				(pin power_in line
					(at 45.72 -60.96 180)
					(length 5.08)
					(name "VSSA_PVT_SOC")
					(number "W15")
				)
				(pin power_in line
					(at 45.72 -38.1 180)
					(length 5.08)
					(name "VDD18_PVT_SOC")
					(number "W16")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W19")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W22")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W23")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W26")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "W27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W30")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W32")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y6")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y7")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "Y9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "Y10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "Y13")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD_NPU")
					(number "Y14")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y16")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y17")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y19")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y20")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y21")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y22")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y23")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y24")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y25")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y26")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDD_SOC")
					(number "Y27")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y29")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y32")
				)
			)
			(symbol "EIC7700X_2_1"
				(pin input line
					(at 35.56 0 180)
					(length 5.08)
					(name "JTAG0_TCK")
					(number "AF1")
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "JTAG0_TDI")
					(number "AF2")
				)
				(pin output line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "JTAG0_TDO")
					(number "AG2")
				)
				(pin input line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "JTAG1_TCK")
					(number "AG4")
				)
				(pin input line
					(at 35.56 -12.7 180)
					(length 5.08)
					(name "JTAG1_TDI")
					(number "AG5")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "JTAG0_TMS")
					(number "AH1")
				)
				(pin input line
					(at 35.56 -30.48 180)
					(length 5.08)
					(name "JTAG2_TRST")
					(number "AH2")
				)
				(pin input line
					(at 35.56 -17.78 180)
					(length 5.08)
					(name "JTAG1_TMS")
					(number "AH4")
				)
				(pin output line
					(at 35.56 -15.24 180)
					(length 5.08)
					(name "JTAG1_TDO")
					(number "AH5")
				)
				(pin output line
					(at 35.56 -25.4 180)
					(length 5.08)
					(name "JTAG2_TDO")
					(number "AJ1")
				)
				(pin input line
					(at 35.56 -20.32 180)
					(length 5.08)
					(name "JTAG2_TCK")
					(number "AJ2")
				)
				(pin input line
					(at 35.56 -22.86 180)
					(length 5.08)
					(name "JTAG2_TDI")
					(number "AJ3")
				)
				(pin input line
					(at 35.56 -27.94 180)
					(length 5.08)
					(name "JTAG2_TMS")
					(number "AJ4")
				)
				(pin bidirectional line
					(at 35.56 -33.02 180)
					(length 5.08)
					(name "GPIO95")
					(number "AK2")
				)
				(pin bidirectional line
					(at 35.56 -35.56 180)
					(length 5.08)
					(name "GPIO34")
					(number "AL3")
				)
				(pin bidirectional line
					(at 35.56 -38.1 180)
					(length 5.08)
					(name "GPIO29")
					(number "AM2")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "RST_OUT_N")
					(number "AN2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "POR_SEL")
					(number "AN3")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "XOUT_24M")
					(number "AN10")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "KEY_RESET_N")
					(number "AP3")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "XIN_24M")
					(number "AP10")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "BOOT_SEL0")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "BOOT_SEL1")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "BOOT_SEL2")
					(number "F11")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "BOOT_SEL3")
					(number "F12")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MODE_SET0")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "CHIP_MODE")
					(number "G11")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MODE_SET1")
					(number "G12")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MODE_SET2")
					(number "G13")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MODE_SET3")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "S_MODE")
					(number "G15")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "LPDDR_REF_CLK")
					(number "H27")
				)
			)
			(symbol "EIC7700X_3_1"
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ13")
					(number "A12")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ12")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ15")
					(number "A14")
				)
				(pin output line
					(at 0 -185.42 0)
					(length 5.08)
					(name "C0_LPDDRA_CA2")
					(number "A15")
				)
				(pin output line
					(at 0 -114.3 0)
					(length 5.08)
					(name "C0_LPDDRA_LP4CKE0_LP5CS0")
					(number "A16")
				)
				(pin output line
					(at 0 -190.5 0)
					(length 5.08)
					(name "C0_LPDDRA_CA0")
					(number "A17")
				)
				(pin bidirectional line
					(at 0 -165.1 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ0")
					(number "A18")
				)
				(pin bidirectional line
					(at 0 -160.02 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ2")
					(number "A19")
				)
				(pin bidirectional line
					(at 0 -154.94 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ4")
					(number "A20")
				)
				(pin bidirectional line
					(at 0 -149.86 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ6")
					(number "A21")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ8")
					(number "A22")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ10")
					(number "A23")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ12")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ14")
					(number "A25")
				)
				(pin output line
					(at 0 -93.98 0)
					(length 5.08)
					(name "C0_LPDDRB_CA0")
					(number "A26")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "C0_LPDDRB_LP4CKE1_LP5CS1")
					(number "A27")
				)
				(pin output line
					(at 0 -88.9 0)
					(length 5.08)
					(name "C0_LPDDRB_CA2")
					(number "A28")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ0")
					(number "A29")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ2")
					(number "A30")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ4")
					(number "A31")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ5")
					(number "A32")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ7")
					(number "A33")
				)
				(pin output line
					(at 69.85 -73.66 180)
					(length 5.08)
					(name "C1_LPDDRB_DMI0")
					(number "AA31")
				)
				(pin bidirectional line
					(at 69.85 -66.04 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ1")
					(number "AA33")
				)
				(pin bidirectional line
					(at 69.85 -68.58 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ0")
					(number "AA34")
				)
				(pin bidirectional line
					(at 69.85 -27.94 180)
					(length 5.08)
					(name "C1_LPDDRB_DQS0_C")
					(number "AB30")
				)
				(pin bidirectional line
					(at 69.85 -25.4 180)
					(length 5.08)
					(name "C1_LPDDRB_DQS0_T")
					(number "AB31")
				)
				(pin bidirectional line
					(at 69.85 -60.96 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ3")
					(number "AB33")
				)
				(pin bidirectional line
					(at 69.85 -63.5 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ2")
					(number "AB34")
				)
				(pin bidirectional line
					(at 69.85 -55.88 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ5")
					(number "AC33")
				)
				(pin bidirectional line
					(at 69.85 -58.42 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ4")
					(number "AC34")
				)
				(pin bidirectional line
					(at 69.85 -50.8 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ7")
					(number "AD33")
				)
				(pin bidirectional line
					(at 69.85 -53.34 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ6")
					(number "AD34")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ10")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -142.24 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ9")
					(number "B12")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ11")
					(number "B13")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ14")
					(number "B14")
				)
				(pin output line
					(at 0 -180.34 0)
					(length 5.08)
					(name "C0_LPDDRA_CA4")
					(number "B15")
				)
				(pin output line
					(at 0 -111.76 0)
					(length 5.08)
					(name "C0_LPDDRA_LP4CKE1_LP5CS1")
					(number "B16")
				)
				(pin output line
					(at 0 -187.96 0)
					(length 5.08)
					(name "C0_LPDDRA_CA1")
					(number "B17")
				)
				(pin bidirectional line
					(at 0 -162.56 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ1")
					(number "B18")
				)
				(pin bidirectional line
					(at 0 -157.48 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ3")
					(number "B19")
				)
				(pin bidirectional line
					(at 0 -152.4 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ5")
					(number "B20")
				)
				(pin bidirectional line
					(at 0 -147.32 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ7")
					(number "B21")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ9")
					(number "B22")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ11")
					(number "B23")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ13")
					(number "B24")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ15")
					(number "B25")
				)
				(pin output line
					(at 0 -91.44 0)
					(length 5.08)
					(name "C0_LPDDRB_CA1")
					(number "B26")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "C0_LPDDRB_LP4CKE0_LP5CS0")
					(number "B27")
				)
				(pin output line
					(at 0 -83.82 0)
					(length 5.08)
					(name "C0_LPDDRB_CA4")
					(number "B28")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ1")
					(number "B29")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ3")
					(number "B30")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "C0_LPDDRB_DQ6")
					(number "B31")
				)
				(pin bidirectional line
					(at 69.85 -144.78 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ8")
					(number "B32")
				)
				(pin bidirectional line
					(at 69.85 -142.24 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ9")
					(number "B33")
				)
				(pin bidirectional line
					(at 0 -144.78 0)
					(length 5.08)
					(name "C0_LPDDRA_DQ8")
					(number "C11")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "C0_LPDDRB_WCK0_T")
					(number "C31")
				)
				(pin bidirectional line
					(at 69.85 -137.16 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ11")
					(number "C33")
				)
				(pin bidirectional line
					(at 69.85 -139.7 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ10")
					(number "C34")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "C0_LPDDRA_DQS1_T")
					(number "D13")
				)
				(pin output line
					(at 0 -96.52 0)
					(length 5.08)
					(name "C0_LPDDRA_WCK1_T")
					(number "D15")
				)
				(pin output line
					(at 0 -177.8 0)
					(length 5.08)
					(name "C0_LPDDRA_CA5")
					(number "D16")
				)
				(pin output line
					(at 0 -172.72 0)
					(length 5.08)
					(name "C0_LPDDRA_CLK_T")
					(number "D17")
				)
				(pin output line
					(at 0 -109.22 0)
					(length 5.08)
					(name "C0_LPDDRA_LP4CS0_LP5CA6")
					(number "D18")
				)
				(pin output line
					(at 0 -101.6 0)
					(length 5.08)
					(name "C0_LPDDRA_WCK0_T")
					(number "D19")
				)
				(pin output line
					(at 0 -170.18 0)
					(length 5.08)
					(name "C0_LPDDRA_DMI0")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "C0_LPDDRA_DQS0_T")
					(number "D21")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "C0_LPDDRB_DQS1_T")
					(number "D23")
				)
				(pin output line
					(at 0 -71.12 0)
					(length 5.08)
					(name "C0_LPDDRB_DMI1")
					(number "D24")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "C0_LPDDRB_WCK1_T")
					(number "D25")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "C0_LPDDRB_LP4CS0_LP5CA6")
					(number "D26")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 5.08)
					(name "C0_LPDDRB_CLK_T")
					(number "D27")
				)
				(pin output line
					(at 0 -81.28 0)
					(length 5.08)
					(name "C0_LPDDRB_CA5")
					(number "D28")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "C0_LPDDRB_DQS0_T")
					(number "D29")
				)
				(pin output line
					(at 0 -73.66 0)
					(length 5.08)
					(name "C0_LPDDRB_DMI0")
					(number "D30")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "C0_LPDDRB_WCK0_C")
					(number "D31")
				)
				(pin bidirectional line
					(at 69.85 -119.38 180)
					(length 5.08)
					(name "C1_LPDDRA_DQS1_C")
					(number "D32")
				)
				(pin bidirectional line
					(at 69.85 -116.84 180)
					(length 5.08)
					(name "C1_LPDDRA_DQS1_T")
					(number "D33")
				)
				(pin bidirectional line
					(at 69.85 -134.62 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ12")
					(number "D34")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "C0_LPDDRA_DQS1_C")
					(number "E13")
				)
				(pin output line
					(at 0 -167.64 0)
					(length 5.08)
					(name "C0_LPDDRA_DMI1")
					(number "E14")
				)
				(pin output line
					(at 0 -99.06 0)
					(length 5.08)
					(name "C0_LPDDRA_WCK1_C")
					(number "E15")
				)
				(pin output line
					(at 0 -175.26 0)
					(length 5.08)
					(name "C0_LPDDRA_CLK_C")
					(number "E17")
				)
				(pin output line
					(at 0 -104.14 0)
					(length 5.08)
					(name "C0_LPDDRA_WCK0_C")
					(number "E19")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "C0_LPDDRA_DQS0_C")
					(number "E21")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "C0_LPDDRB_DQS1_C")
					(number "E23")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "C0_LPDDRB_WCK1_C")
					(number "E25")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 5.08)
					(name "C0_LPDDRB_CLK_C")
					(number "E27")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "C0_LPDDRB_DQS0_C")
					(number "E29")
				)
				(pin output line
					(at 69.85 -167.64 180)
					(length 5.08)
					(name "C1_LPDDRA_DMI1")
					(number "E32")
				)
				(pin bidirectional line
					(at 69.85 -132.08 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ13")
					(number "E34")
				)
				(pin output line
					(at 0 -182.88 0)
					(length 5.08)
					(name "C0_LPDDRA_CA3")
					(number "F16")
				)
				(pin output line
					(at 0 -106.68 0)
					(length 5.08)
					(name "C0_LPDDRA_LP4CS1")
					(number "F18")
				)
				(pin bidirectional line
					(at 0 -193.04 0)
					(length 5.08)
					(name "C0_LPDDR_ZN")
					(number "F22")
				)
				(pin output line
					(at 0 -195.58 0)
					(length 5.08)
					(name "C0_LPDDR_RESET_N")
					(number "F24")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "C0_LPDDRB_LP4CS1")
					(number "F26")
				)
				(pin output line
					(at 0 -86.36 0)
					(length 5.08)
					(name "C0_LPDDRB_CA3")
					(number "F28")
				)
				(pin output line
					(at 69.85 -99.06 180)
					(length 5.08)
					(name "C1_LPDDRA_WCK1_C")
					(number "F31")
				)
				(pin output line
					(at 69.85 -96.52 180)
					(length 5.08)
					(name "C1_LPDDRA_WCK1_T")
					(number "F32")
				)
				(pin bidirectional line
					(at 69.85 -127 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ15")
					(number "F33")
				)
				(pin bidirectional line
					(at 69.85 -129.54 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ14")
					(number "F34")
				)
				(pin output line
					(at 0 -200.66 0)
					(length 5.08)
					(name "C0_LPDDR_ATO")
					(number "G22")
				)
				(pin bidirectional line
					(at 0 -198.12 0)
					(length 5.08)
					(name "C0_LPDDR_DTO")
					(number "G23")
				)
				(pin output line
					(at 69.85 -182.88 180)
					(length 5.08)
					(name "C1_LPDDRA_CA3")
					(number "G29")
				)
				(pin output line
					(at 69.85 -177.8 180)
					(length 5.08)
					(name "C1_LPDDRA_CA5")
					(number "G31")
				)
				(pin output line
					(at 69.85 -180.34 180)
					(length 5.08)
					(name "C1_LPDDRA_CA4")
					(number "G33")
				)
				(pin output line
					(at 69.85 -185.42 180)
					(length 5.08)
					(name "C1_LPDDRA_CA2")
					(number "G34")
				)
				(pin output line
					(at 69.85 -175.26 180)
					(length 5.08)
					(name "C1_LPDDRA_CLK_C")
					(number "H30")
				)
				(pin output line
					(at 69.85 -172.72 180)
					(length 5.08)
					(name "C1_LPDDRA_CLK_T")
					(number "H31")
				)
				(pin output line
					(at 69.85 -111.76 180)
					(length 5.08)
					(name "C1_LPDDRA_LP4CKE1_LP5CS1")
					(number "H33")
				)
				(pin output line
					(at 69.85 -114.3 180)
					(length 5.08)
					(name "C1_LPDDRA_LP4CKE0_LP5CS0")
					(number "H34")
				)
				(pin output line
					(at 69.85 -106.68 180)
					(length 5.08)
					(name "C1_LPDDRA_LP4CS1")
					(number "J29")
				)
				(pin output line
					(at 69.85 -109.22 180)
					(length 5.08)
					(name "C1_LPDDRA_LP4CS0_LP5CA6")
					(number "J31")
				)
				(pin output line
					(at 69.85 -187.96 180)
					(length 5.08)
					(name "C1_LPDDRA_CA1")
					(number "J33")
				)
				(pin output line
					(at 69.85 -190.5 180)
					(length 5.08)
					(name "C1_LPDDRA_CA0")
					(number "J34")
				)
				(pin output line
					(at 69.85 -104.14 180)
					(length 5.08)
					(name "C1_LPDDRA_WCK0_C")
					(number "K30")
				)
				(pin output line
					(at 69.85 -101.6 180)
					(length 5.08)
					(name "C1_LPDDRA_WCK0_T")
					(number "K31")
				)
				(pin bidirectional line
					(at 69.85 -162.56 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ1")
					(number "K33")
				)
				(pin bidirectional line
					(at 69.85 -165.1 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ0")
					(number "K34")
				)
				(pin output line
					(at 69.85 -200.66 180)
					(length 5.08)
					(name "C1_LPDDR_ATO")
					(number "L29")
				)
				(pin output line
					(at 69.85 -170.18 180)
					(length 5.08)
					(name "C1_LPDDRA_DMI0")
					(number "L31")
				)
				(pin bidirectional line
					(at 69.85 -157.48 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ3")
					(number "L33")
				)
				(pin bidirectional line
					(at 69.85 -160.02 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ2")
					(number "L34")
				)
				(pin bidirectional line
					(at 69.85 -124.46 180)
					(length 5.08)
					(name "C1_LPDDRA_DQS0_C")
					(number "M30")
				)
				(pin bidirectional line
					(at 69.85 -121.92 180)
					(length 5.08)
					(name "C1_LPDDRA_DQS0_T")
					(number "M31")
				)
				(pin bidirectional line
					(at 69.85 -152.4 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ5")
					(number "M33")
				)
				(pin bidirectional line
					(at 69.85 -154.94 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ4")
					(number "M34")
				)
				(pin bidirectional line
					(at 69.85 -193.04 180)
					(length 5.08)
					(name "C1_LPDDR_ZN")
					(number "N28")
				)
				(pin bidirectional line
					(at 69.85 -147.32 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ7")
					(number "N33")
				)
				(pin bidirectional line
					(at 69.85 -149.86 180)
					(length 5.08)
					(name "C1_LPDDRA_DQ6")
					(number "N34")
				)
				(pin bidirectional line
					(at 69.85 -22.86 180)
					(length 5.08)
					(name "C1_LPDDRB_DQS1_C")
					(number "P30")
				)
				(pin bidirectional line
					(at 69.85 -20.32 180)
					(length 5.08)
					(name "C1_LPDDRB_DQS1_T")
					(number "P31")
				)
				(pin bidirectional line
					(at 69.85 -45.72 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ9")
					(number "P33")
				)
				(pin bidirectional line
					(at 69.85 -48.26 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ8")
					(number "P34")
				)
				(pin output line
					(at 69.85 -195.58 180)
					(length 5.08)
					(name "C1_LPDDR_RESET_N")
					(number "R28")
				)
				(pin bidirectional line
					(at 69.85 -198.12 180)
					(length 5.08)
					(name "C1_LPDDR_DTO")
					(number "R29")
				)
				(pin output line
					(at 69.85 -71.12 180)
					(length 5.08)
					(name "C1_LPDDRB_DMI1")
					(number "R31")
				)
				(pin bidirectional line
					(at 69.85 -40.64 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ11")
					(number "R33")
				)
				(pin bidirectional line
					(at 69.85 -43.18 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ10")
					(number "R34")
				)
				(pin output line
					(at 69.85 -2.54 180)
					(length 5.08)
					(name "C1_LPDDRB_WCK1_C")
					(number "T30")
				)
				(pin output line
					(at 69.85 0 180)
					(length 5.08)
					(name "C1_LPDDRB_WCK1_T")
					(number "T31")
				)
				(pin bidirectional line
					(at 69.85 -35.56 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ13")
					(number "T33")
				)
				(pin bidirectional line
					(at 69.85 -38.1 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ12")
					(number "T34")
				)
				(pin output line
					(at 69.85 -10.16 180)
					(length 5.08)
					(name "C1_LPDDRB_LP4CS1")
					(number "U29")
				)
				(pin output line
					(at 69.85 -12.7 180)
					(length 5.08)
					(name "C1_LPDDRB_LP4CS0_LP5CA6")
					(number "U31")
				)
				(pin bidirectional line
					(at 69.85 -30.48 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ15")
					(number "U33")
				)
				(pin bidirectional line
					(at 69.85 -33.02 180)
					(length 5.08)
					(name "C1_LPDDRB_DQ14")
					(number "U34")
				)
				(pin output line
					(at 69.85 -78.74 180)
					(length 5.08)
					(name "C1_LPDDRB_CLK_C")
					(number "V30")
				)
				(pin output line
					(at 69.85 -76.2 180)
					(length 5.08)
					(name "C1_LPDDRB_CLK_T")
					(number "V31")
				)
				(pin output line
					(at 69.85 -91.44 180)
					(length 5.08)
					(name "C1_LPDDRB_CA1")
					(number "V33")
				)
				(pin output line
					(at 69.85 -93.98 180)
					(length 5.08)
					(name "C1_LPDDRB_CA0")
					(number "V34")
				)
				(pin output line
					(at 69.85 -86.36 180)
					(length 5.08)
					(name "C1_LPDDRB_CA3")
					(number "W29")
				)
				(pin output line
					(at 69.85 -81.28 180)
					(length 5.08)
					(name "C1_LPDDRB_CA5")
					(number "W31")
				)
				(pin output line
					(at 69.85 -17.78 180)
					(length 5.08)
					(name "C1_LPDDRB_LP4CKE0_LP5CS0")
					(number "W33")
				)
				(pin output line
					(at 69.85 -15.24 180)
					(length 5.08)
					(name "C1_LPDDRB_LP4CKE1_LP5CS1")
					(number "W34")
				)
				(pin output line
					(at 69.85 -7.62 180)
					(length 5.08)
					(name "C1_LPDDRB_WCK0_C")
					(number "Y30")
				)
				(pin output line
					(at 69.85 -5.08 180)
					(length 5.08)
					(name "C1_LPDDRB_WCK0_T")
					(number "Y31")
				)
				(pin output line
					(at 69.85 -83.82 180)
					(length 5.08)
					(name "C1_LPDDRB_CA4")
					(number "Y33")
				)
				(pin output line
					(at 69.85 -88.9 180)
					(length 5.08)
					(name "C1_LPDDRB_CA2")
					(number "Y34")
				)
			)
			(symbol "EIC7700X_4_1"
				(pin input line
					(at 43.18 -73.66 180)
					(length 5.08)
					(name "MIPI_CSI5_D0N")
					(number "AE30")
				)
				(pin input line
					(at 43.18 -71.12 180)
					(length 5.08)
					(name "MIPI_CSI5_D0P")
					(number "AE31")
				)
				(pin input line
					(at 43.18 -78.74 180)
					(length 5.08)
					(name "MIPI_CSI5_CKN")
					(number "AF30")
				)
				(pin input line
					(at 43.18 -76.2 180)
					(length 5.08)
					(name "MIPI_CSI5_CKP")
					(number "AF31")
				)
				(pin input line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "MIPI_CSI4_D1N")
					(number "AF33")
				)
				(pin input line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "MIPI_CSI4_D1P")
					(number "AF34")
				)
				(pin output line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "MIPI_CSI3_ATB")
					(number "AG28")
				)
				(pin input line
					(at 43.18 -68.58 180)
					(length 5.08)
					(name "MIPI_CSI5_D1N")
					(number "AG30")
				)
				(pin input line
					(at 43.18 -66.04 180)
					(length 5.08)
					(name "MIPI_CSI5_D1P")
					(number "AG31")
				)
				(pin input line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "MIPI_CSI4_CKN")
					(number "AG33")
				)
				(pin input line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "MIPI_CSI4_CKP")
					(number "AG34")
				)
				(pin output line
					(at 0 -81.28 0)
					(length 5.08)
					(name "MIPI_CSI2_ATB")
					(number "AH28")
				)
				(pin output line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "MIPI_CSI4_ATB")
					(number "AH30")
				)
				(pin output line
					(at 43.18 -81.28 180)
					(length 5.08)
					(name "MIPI_CSI5_ATB")
					(number "AH31")
				)
				(pin input line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "MIPI_CSI4_D0N")
					(number "AH33")
				)
				(pin input line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "MIPI_CSI4_D0P")
					(number "AH34")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MIPI_CSI0_XHS")
					(number "AJ11")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MIPI_CSI0_MCLK")
					(number "AJ12")
				)
				(pin bidirectional line
					(at 43.18 -115.57 180)
					(length 5.08)
					(name "HDMI_CEC")
					(number "AJ21")
				)
				(pin output line
					(at 0 -53.34 0)
					(length 5.08)
					(name "MIPI_CSI1_ATB")
					(number "AJ28")
				)
				(pin passive line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "MIPI_CSI4_REXT")
					(number "AJ30")
				)
				(pin passive line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "MIPI_CSI5_REXT")
					(number "AJ31")
				)
				(pin input line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "MIPI_CSI3_D0N")
					(number "AJ33")
				)
				(pin input line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "MIPI_CSI3_D0P")
					(number "AJ34")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "MIPI_CSI0_XVS")
					(number "AK10")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MIPI_CSI1_XVS")
					(number "AK11")
				)
				(pin output line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "MIPI_CSI5_XHS")
					(number "AK13")
				)
				(pin output line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "MIPI_CSI5_XVS")
					(number "AK14")
				)
				(pin bidirectional line
					(at 43.18 -105.41 180)
					(length 5.08)
					(name "HDMI_SDA")
					(number "AK21")
				)
				(pin input line
					(at 0 -102.87 0)
					(length 5.08)
					(name "MIPI_DSI_D0P")
					(number "AK22")
				)
				(pin input line
					(at 0 -100.33 0)
					(length 5.08)
					(name "MIPI_DSI_D1N")
					(number "AK23")
				)
				(pin input line
					(at 0 -110.49 0)
					(length 5.08)
					(name "MIPI_DSI_CKN")
					(number "AK24")
				)
				(pin input line
					(at 0 -92.71 0)
					(length 5.08)
					(name "MIPI_DSI_D2P")
					(number "AK25")
				)
				(pin input line
					(at 0 -90.17 0)
					(length 5.08)
					(name "MIPI_DSI_D3N")
					(number "AK26")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MIPI_CSI0_ATB")
					(number "AK28")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "MIPI_CSI2_REXT")
					(number "AK30")
				)
				(pin passive line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "MIPI_CSI3_REXT")
					(number "AK31")
				)
				(pin input line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "MIPI_CSI3_CKN")
					(number "AK33")
				)
				(pin input line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "MIPI_CSI3_CKP")
					(number "AK34")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MIPI_CSI1_XHS")
					(number "AL11")
				)
				(pin output line
					(at 43.18 0 180)
					(length 5.08)
					(name "MIPI_CSI3_XVS")
					(number "AL12")
				)
				(pin output line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "MIPI_CSI3_XHS")
					(number "AL13")
				)
				(pin output line
					(at 43.18 -63.5 180)
					(length 5.08)
					(name "MIPI_CSI5_MCLK")
					(number "AL14")
				)
				(pin output line
					(at 43.18 -107.95 180)
					(length 5.08)
					(name "HDMI_SCL")
					(number "AL21")
				)
				(pin input line
					(at 0 -105.41 0)
					(length 5.08)
					(name "MIPI_DSI_D0N")
					(number "AL22")
				)
				(pin input line
					(at 0 -97.79 0)
					(length 5.08)
					(name "MIPI_DSI_D1P")
					(number "AL23")
				)
				(pin input line
					(at 0 -107.95 0)
					(length 5.08)
					(name "MIPI_DSI_CKP")
					(number "AL24")
				)
				(pin input line
					(at 0 -95.25 0)
					(length 5.08)
					(name "MIPI_DSI_D2N")
					(number "AL25")
				)
				(pin input line
					(at 0 -87.63 0)
					(length 5.08)
					(name "MIPI_DSI_D3P")
					(number "AL26")
				)
				(pin output line
					(at 0 -113.03 0)
					(length 5.08)
					(name "MIPI_DSI_ATB")
					(number "AL28")
				)
				(pin passive line
					(at 0 -85.09 0)
					(length 5.08)
					(name "MIPI_DSI_REXT")
					(number "AL29")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "MIPI_CSI0_REXT")
					(number "AL30")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "MIPI_CSI1_REXT")
					(number "AL31")
				)
				(pin input line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "MIPI_CSI3_D1N")
					(number "AL33")
				)
				(pin input line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "MIPI_CSI3_D1P")
					(number "AL34")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 5.08)
					(name "MIPI_CSI1_MCLK")
					(number "AM11")
				)
				(pin output line
					(at 0 -63.5 0)
					(length 5.08)
					(name "MIPI_CSI2_MCLK")
					(number "AM12")
				)
				(pin output line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "MIPI_CSI3_MCLK")
					(number "AM13")
				)
				(pin output line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "MIPI_CSI4_MCLK")
					(number "AM14")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 5.08)
					(name "MIPI_CSI2_D1P")
					(number "AM33")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 5.08)
					(name "MIPI_CSI2_D1N")
					(number "AM34")
				)
				(pin output line
					(at 0 -55.88 0)
					(length 5.08)
					(name "MIPI_CSI2_XVS")
					(number "AN12")
				)
				(pin output line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "MIPI_CSI4_XHS")
					(number "AN13")
				)
				(pin output line
					(at 43.18 -85.09 180)
					(length 5.08)
					(name "HDMI_TXCKP")
					(number "AN21")
				)
				(pin output line
					(at 43.18 -100.33 180)
					(length 5.08)
					(name "HDMI_TX0P")
					(number "AN22")
				)
				(pin output line
					(at 43.18 -95.25 180)
					(length 5.08)
					(name "HDMI_TX1P")
					(number "AN23")
				)
				(pin output line
					(at 43.18 -90.17 180)
					(length 5.08)
					(name "HDMI_TX2P")
					(number "AN24")
				)
				(pin input line
					(at 43.18 -113.03 180)
					(length 5.08)
					(name "HDMI_HPD")
					(number "AN25")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MIPI_CSI0_D0N")
					(number "AN26")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MIPI_CSI0_CKN")
					(number "AN27")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "MIPI_CSI0_D1N")
					(number "AN28")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MIPI_CSI1_D1N")
					(number "AN29")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "MIPI_CSI1_CKP")
					(number "AN30")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MIPI_CSI1_D0N")
					(number "AN31")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 5.08)
					(name "MIPI_CSI2_D0N")
					(number "AN32")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 5.08)
					(name "MIPI_CSI2_CKN")
					(number "AN33")
				)
				(pin output line
					(at 0 -58.42 0)
					(length 5.08)
					(name "MIPI_CSI2_XHS")
					(number "AP12")
				)
				(pin output line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "MIPI_CSI4_XVS")
					(number "AP13")
				)
				(pin output line
					(at 43.18 -87.63 180)
					(length 5.08)
					(name "HDMI_TXCKN")
					(number "AP21")
				)
				(pin output line
					(at 43.18 -102.87 180)
					(length 5.08)
					(name "HDMI_TX0N")
					(number "AP22")
				)
				(pin output line
					(at 43.18 -97.79 180)
					(length 5.08)
					(name "HDMI_TX1N")
					(number "AP23")
				)
				(pin output line
					(at 43.18 -92.71 180)
					(length 5.08)
					(name "HDMI_TX2N")
					(number "AP24")
				)
				(pin passive line
					(at 43.18 -110.49 180)
					(length 5.08)
					(name "HDMI_REXT")
					(number "AP25")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MIPI_CSI0_D0P")
					(number "AP26")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "MIPI_CSI0_CKP")
					(number "AP27")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MIPI_CSI0_D1P")
					(number "AP28")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "MIPI_CSI1_D1P")
					(number "AP29")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "MIPI_CSI1_CKN")
					(number "AP30")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "MIPI_CSI1_D0P")
					(number "AP31")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 5.08)
					(name "MIPI_CSI2_D0P")
					(number "AP32")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 5.08)
					(name "MIPI_CSI2_CKP")
					(number "AP33")
				)
			)
			(symbol "EIC7700X_5_1"
				(pin bidirectional line
					(at 36.83 -10.16 180)
					(length 5.08)
					(name "SDIO0_D2")
					(number "A2")
				)
				(pin output line
					(at 36.83 -2.54 180)
					(length 5.08)
					(name "SDIO0_CMD")
					(number "A3")
				)
				(pin bidirectional line
					(at 36.83 -5.08 180)
					(length 5.08)
					(name "SDIO0_D0")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "EMMC_D7")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "EMMC_D6")
					(number "A6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "EMMC_D5")
					(number "A7")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "EMMC_CLK")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "EMMC_D0")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "EMMC_D2")
					(number "A10")
				)
				(pin bidirectional line
					(at 36.83 -12.7 180)
					(length 5.08)
					(name "SDIO0_D3")
					(number "B2")
				)
				(pin output line
					(at 36.83 0 180)
					(length 5.08)
					(name "SDIO0_CLK")
					(number "B3")
				)
				(pin bidirectional line
					(at 36.83 -7.62 180)
					(length 5.08)
					(name "SDIO0_D1")
					(number "B4")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 5.08)
					(name "EMMC_RSTN_OUT")
					(number "B5")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "EMMC_DS")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "EMMC_D4")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "EMMC_D3")
					(number "B8")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "EMMC_CMD")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "EMMC_D1")
					(number "B10")
				)
				(pin bidirectional line
					(at 36.83 -25.4 180)
					(length 5.08)
					(name "SDIO1_D2")
					(number "D7")
				)
				(pin output line
					(at 36.83 -17.78 180)
					(length 5.08)
					(name "SDIO1_CMD")
					(number "D8")
				)
				(pin bidirectional line
					(at 36.83 -20.32 180)
					(length 5.08)
					(name "SDIO1_D0")
					(number "D9")
				)
				(pin bidirectional line
					(at 36.83 -27.94 180)
					(length 5.08)
					(name "SDIO1_D3")
					(number "E7")
				)
				(pin output line
					(at 36.83 -15.24 180)
					(length 5.08)
					(name "SDIO1_CLK")
					(number "E8")
				)
				(pin bidirectional line
					(at 36.83 -22.86 180)
					(length 5.08)
					(name "SDIO1_D1")
					(number "E9")
				)
			)
			(symbol "EIC7700X_6_1"
				(pin bidirectional line
					(at 40.64 -48.26 180)
					(length 5.08)
					(name "PCIE_CLKREQ_N")
					(number "AH14")
				)
				(pin bidirectional line
					(at 40.64 0 180)
					(length 5.08)
					(name "PCIE_WAKE_N")
					(number "AH17")
				)
				(pin passive line
					(at 40.64 -43.18 180)
					(length 5.08)
					(name "PCIE_REXT")
					(number "AH19")
				)
				(pin output line
					(at 40.64 -45.72 180)
					(length 5.08)
					(name "PCIE_PERST_N")
					(number "AJ14")
				)
				(pin input line
					(at 40.64 -38.1 180)
					(length 5.08)
					(name "PCIE_RX0P")
					(number "AJ16")
				)
				(pin input line
					(at 40.64 -27.94 180)
					(length 5.08)
					(name "PCIE_RX2P")
					(number "AJ18")
				)
				(pin input line
					(at 40.64 -40.64 180)
					(length 5.08)
					(name "PCIE_RX0N")
					(number "AK16")
				)
				(pin input line
					(at 40.64 -33.02 180)
					(length 5.08)
					(name "PCIE_RX1P")
					(number "AK17")
				)
				(pin input line
					(at 40.64 -30.48 180)
					(length 5.08)
					(name "PCIE_RX2N")
					(number "AK18")
				)
				(pin input line
					(at 40.64 -22.86 180)
					(length 5.08)
					(name "PCIE_RX3P")
					(number "AK19")
				)
				(pin input line
					(at 40.64 -35.56 180)
					(length 5.08)
					(name "PCIE_RX1N")
					(number "AL17")
				)
				(pin input line
					(at 40.64 -25.4 180)
					(length 5.08)
					(name "PCIE_RX3N")
					(number "AL19")
				)
				(pin output line
					(at 40.64 -17.78 180)
					(length 5.08)
					(name "PCIE_TX0P")
					(number "AM16")
				)
				(pin output line
					(at 40.64 -7.62 180)
					(length 5.08)
					(name "PCIE_TX2P")
					(number "AM18")
				)
				(pin input line
					(at 40.64 -53.34 180)
					(length 5.08)
					(name "PCIE_CLKN")
					(number "AN15")
				)
				(pin output line
					(at 40.64 -20.32 180)
					(length 5.08)
					(name "PCIE_TX0N")
					(number "AN16")
				)
				(pin output line
					(at 40.64 -12.7 180)
					(length 5.08)
					(name "PCIE_TX1P")
					(number "AN17")
				)
				(pin output line
					(at 40.64 -10.16 180)
					(length 5.08)
					(name "PCIE_TX2N")
					(number "AN18")
				)
				(pin output line
					(at 40.64 -2.54 180)
					(length 5.08)
					(name "PCIE_TX3P")
					(number "AN19")
				)
				(pin input line
					(at 40.64 -50.8 180)
					(length 5.08)
					(name "PCIE_CLKP")
					(number "AP15")
				)
				(pin output line
					(at 40.64 -15.24 180)
					(length 5.08)
					(name "PCIE_TX1N")
					(number "AP17")
				)
				(pin output line
					(at 40.64 -5.08 180)
					(length 5.08)
					(name "PCIE_TX3N")
					(number "AP19")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "USB1_DM")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "USB1_DP")
					(number "C2")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 5.08)
					(name "USB1_ID")
					(number "C4")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 5.08)
					(name "USB1_SSTX_M")
					(number "D1")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 5.08)
					(name "USB1_SSTX_P")
					(number "D2")
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "USB1_VBUS")
					(number "D4")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "USB1_REXT")
					(number "D5")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "USB0_REXT")
					(number "D6")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "USB1_SSRX_M")
					(number "E2")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "USB1_SSRX_P")
					(number "E3")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "USB0_ID")
					(number "E5")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "USB0_VBUS")
					(number "E6")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "USB0_DM")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "USB0_DP")
					(number "F2")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 5.08)
					(name "USB0_SSTX_M")
					(number "F4")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "USB0_SSTX_P")
					(number "F5")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 5.08)
					(name "SATA_REXT")
					(number "F7")
				)
				(pin output line
					(at 0 -52.07 0)
					(length 5.08)
					(name "SATA_TXP")
					(number "G2")
				)
				(pin output line
					(at 0 -54.61 0)
					(length 5.08)
					(name "SATA_TXM")
					(number "G3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "USB0_SSRX_M")
					(number "G5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "USB0_SSRX_P")
					(number "G6")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 5.08)
					(name "SATA_RXM")
					(number "H1")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 5.08)
					(name "SATA_RXP")
					(number "H2")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "USB1_PWREN")
					(number "H5")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "USB0_PWREN")
					(number "H6")
				)
			)
			(symbol "EIC7700X_7_1"
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "RGMII0_CLK_125")
					(number "H4")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "RGMII0_INTB")
					(number "J2")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "RGMII0_RXD0")
					(number "J3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "RGMII0_RXDV")
					(number "J4")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "RGMII0_RXCLK")
					(number "J5")
				)
				(pin output line
					(at 0 -12.7 0)
					(length 5.08)
					(name "RGMII0_TXCLK")
					(number "K1")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "RGMII0_TXEN")
					(number "K2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "RGMII0_RXD1")
					(number "K3")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "RGMII0_RXD2")
					(number "K4")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "RGMII0_RXD3")
					(number "K5")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "RGMII0_TXD0")
					(number "L1")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "RGMII0_TXD1")
					(number "L2")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "RGMII0_TXD2")
					(number "M1")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "RGMII0_TXD3")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "RGMII0_MDIO")
					(number "N1")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "RGMII0_MDC")
					(number "N2")
				)
				(pin input line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "RGMII1_CLK_125")
					(number "P1")
				)
				(pin input line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "RGMII1_INTB")
					(number "P2")
				)
				(pin input line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "RGMII1_RXCLK")
					(number "P3")
				)
				(pin input line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "RGMII1_RXDV")
					(number "P4")
				)
				(pin input line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "RGMII1_RXD0")
					(number "P5")
				)
				(pin output line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "RGMII1_TXCLK")
					(number "R1")
				)
				(pin output line
					(at 43.18 0 180)
					(length 5.08)
					(name "RGMII1_TXEN")
					(number "R2")
				)
				(pin input line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "RGMII1_RXD3")
					(number "R3")
				)
				(pin input line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "RGMII1_RXD2")
					(number "R4")
				)
				(pin input line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "RGMII1_RXD1")
					(number "R5")
				)
				(pin output line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "RGMII1_TXD0")
					(number "T1")
				)
				(pin output line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "RGMII1_TXD1")
					(number "T2")
				)
				(pin output line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "RGMII1_MDC")
					(number "T4")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "RGMII1_MDIO")
					(number "T5")
				)
				(pin output line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "RGMII1_TXD2")
					(number "U1")
				)
				(pin output line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "RGMII1_TXD3")
					(number "U2")
				)
			)
			(symbol "EIC7700X_8_1"
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "SPI1_CLK")
					(number "AA1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "SPI1_D0")
					(number "AA2")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "SPI1_D3")
					(number "AB1")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 5.08)
					(name "SPI1_CS1_N")
					(number "AB2")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "SPI1_CS0_N")
					(number "AC1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "SPI1_D2")
					(number "AC2")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "SPI1_D1")
					(number "AC3")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "SPI3_CLK")
					(number "AC4")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "SPI3_CS_N")
					(number "AC5")
				)
				(pin input line
					(at 34.29 0 180)
					(length 5.08)
					(name "FAN_TACH")
					(number "AD1")
				)
				(pin output line
					(at 34.29 -2.54 180)
					(length 5.08)
					(name "FAN_PWM")
					(number "AD2")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "SPI3_DI")
					(number "AD4")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 5.08)
					(name "SPI3_DO")
					(number "AD5")
				)
				(pin bidirectional line
					(at 34.29 -8.89 180)
					(length 5.08)
					(name "GPIO5")
					(number "AG1")
				)
				(pin bidirectional line
					(at 34.29 -11.43 180)
					(length 5.08)
					(name "GPIO11")
					(number "AH3")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SPI2_CS0_N")
					(number "AJ5")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 5.08)
					(name "SPI2_CS1_N")
					(number "AJ6")
				)
				(pin bidirectional line
					(at 34.29 -21.59 180)
					(length 5.08)
					(name "GPIO93")
					(number "AK1")
				)
				(pin bidirectional line
					(at 34.29 -19.05 180)
					(length 5.08)
					(name "GPIO92")
					(number "AK4")
				)
				(pin bidirectional line
					(at 34.29 -13.97 180)
					(length 5.08)
					(name "GPIO27")
					(number "AL1")
				)
				(pin bidirectional line
					(at 34.29 -24.13 180)
					(length 5.08)
					(name "GPIO106")
					(number "AL2")
				)
				(pin bidirectional line
					(at 34.29 -26.67 180)
					(length 5.08)
					(name "GPIO111")
					(number "AL4")
				)
				(pin bidirectional line
					(at 34.29 -16.51 180)
					(length 5.08)
					(name "GPIO28")
					(number "AM1")
				)
				(pin bidirectional line
					(at 34.29 -6.35 180)
					(length 5.08)
					(name "GPIO0")
					(number "AM4")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "SPI0_CLK")
					(number "V1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "SPI0_D0")
					(number "V2")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "SPI0_CS_N")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "SPI0_D2")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "SPI0_D1")
					(number "Y1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "SPI0_D3")
					(number "Y2")
				)
			)
			(symbol "EIC7700X_9_1"
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "I2C10_SCL")
					(number "AE1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "I2C10_SDA")
					(number "AE2")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "I2C1_SCL")
					(number "AE3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "I2C1_SDA")
					(number "AE4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "I2C0_SCL")
					(number "AE5")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "I2C11_SDA")
					(number "AF3")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "I2C11_SCL")
					(number "AF4")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "I2C0_SDA")
					(number "AF5")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 5.08)
					(name "I2S2_BCLK")
					(number "AK5")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "I2C2_SCL")
					(number "AK8")
				)
				(pin output line
					(at 33.02 0 180)
					(length 5.08)
					(name "I2S_MCLK")
					(number "AL5")
				)
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 5.08)
					(name "I2S2_WCLK")
					(number "AL6")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "I2C2_SDA")
					(number "AL8")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "I2C3_SDA")
					(number "AL9")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "I2C5_SDA")
					(number "AL10")
				)
				(pin input line
					(at 33.02 -25.4 180)
					(length 5.08)
					(name "I2S2_SDI")
					(number "AM5")
				)
				(pin output line
					(at 33.02 -27.94 180)
					(length 5.08)
					(name "I2S2_SDO")
					(number "AM6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "I2C3_SCL")
					(number "AM8")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "I2C5_SCL")
					(number "AM9")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 5.08)
					(name "I2S1_WCLK")
					(number "AN4")
				)
				(pin output line
					(at 33.02 -17.78 180)
					(length 5.08)
					(name "I2S1_SDO")
					(number "AN5")
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 5.08)
					(name "I2S0_BCLK")
					(number "AN6")
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 5.08)
					(name "I2S0_WCLK")
					(number "AN7")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "I2C4_SCL")
					(number "AN8")
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 5.08)
					(name "I2S1_BCLK")
					(number "AP4")
				)
				(pin input line
					(at 33.02 -15.24 180)
					(length 5.08)
					(name "I2S1_SDI")
					(number "AP5")
				)
				(pin output line
					(at 33.02 -7.62 180)
					(length 5.08)
					(name "I2S0_SDO")
					(number "AP6")
				)
				(pin input line
					(at 33.02 -5.08 180)
					(length 5.08)
					(name "I2S0_SDI")
					(number "AP7")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "I2C4_SDA")
					(number "AP8")
				)
			)
			(symbol "EIC7700X_10_1"
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "UART1_CTS")
					(number "AA4")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 5.08)
					(name "UART1_TX")
					(number "AA5")
				)
				(pin output line
					(at 0 0 0)
					(length 5.08)
					(name "UART2_TX")
					(number "AB3")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "UART2_RX")
					(number "AB4")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 5.08)
					(name "UART1_RTS")
					(number "AB5")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "UART0_TX")
					(number "Y3")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "UART0_RX")
					(number "Y4")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "UART1_RX")
					(number "Y5")
				)
			)
			(embedded_fonts no)
		)
)
