(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EOS-S3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 66.04 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EOS-S3"
				(at 66.04 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EOS-S3"
				(at 66.04 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/pdfDocs/QuickLogic_EOS-S3_DS.pdf"
				(at 66.04 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SoC FPGA EOS S3 Ultra Low Power MCU + eFPGA"
				(at 66.04 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EOS3FF512-WRN42"
				(at 66.04 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "QuickLogic"
				(at 66.04 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 66.04 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 66.04 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, SOC, IC, FPGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EOS-S3_1_1"
				(text "BANK A"
					(at 19.05 -16.51 900)
				)
				(text "BANK B"
					(at 19.05 -64.77 900)
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "XTAL_I")
					(number "A1")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VDD1")
					(number "A2")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "VDD2")
					(number "A3")
				)
				(pin input line
					(at 52.07 -2.54 180)
					(length 2.54)
					(name "FBIO_14/SW_DP_CLK")
					(number "A4")
				)
				(pin input line
					(at 52.07 -7.62 180)
					(length 2.54)
					(name "FBIO_9")
					(number "A5")
				)
				(pin input line
					(at 52.07 -12.7 180)
					(length 2.54)
					(name "FBIO_6/FCLK")
					(number "A6")
				)
				(pin input line
					(at 52.07 -20.32 180)
					(length 2.54)
					(name "SCL_0")
					(number "A7")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "XTAL_O")
					(number "B1")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "ADC0")
					(number "B2")
				)
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "LDO_VIN")
					(number "B3")
				)
				(pin input line
					(at 52.07 0 180)
					(length 2.54)
					(name "FBIO_15/SW_DP_IO")
					(number "B4")
				)
				(pin input line
					(at 52.07 -5.08 180)
					(length 2.54)
					(name "FBIO_10")
					(number "B5")
				)
				(pin input line
					(at 52.07 -10.16 180)
					(length 2.54)
					(name "FBIO_8")
					(number "B6")
				)
				(pin input line
					(at 52.07 -17.78 180)
					(length 2.54)
					(name "SDA_0")
					(number "B7")
				)
				(pin input line
					(at 52.07 -33.02 180)
					(length 2.54)
					(name "FBIO_19/SPI_SLAVE_MOSI")
					(number "C1")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "AVDD")
					(number "C2")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 2.54)
					(name "AGND")
					(number "C3")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 2.54)
					(name "GND")
					(number "C4")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCCIOA")
					(number "C6")
				)
				(pin input line
					(at 52.07 -15.24 180)
					(length 2.54)
					(name "FBIO3/SENSOR_INT_0")
					(number "C7")
				)
				(pin input line
					(at 52.07 -27.94 180)
					(length 2.54)
					(name "FBIO_17/SPI_SLAVE_MISO")
					(number "D1")
				)
				(pin input line
					(at 52.07 -38.1 180)
					(length 2.54)
					(name "FBIO_24")
					(number "D2")
				)
				(pin input line
					(at 52.07 -40.64 180)
					(length 2.54)
					(name "FBIO_25")
					(number "D3")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "STM")
					(number "D4")
				)
				(pin input line
					(at 52.07 -53.34 180)
					(length 2.54)
					(name "FBIO_34/SPI_MASTER_CLK")
					(number "D5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VCCIOB")
					(number "D6")
				)
				(pin input line
					(at 52.07 -63.5 180)
					(length 2.54)
					(name "FBIO_43/AP_INTERRUPT")
					(number "D7")
				)
				(pin input line
					(at 52.07 -25.4 180)
					(length 2.54)
					(name "FBIO_16/SPI_SLAVE_CLK")
					(number "E1")
				)
				(pin input line
					(at 52.07 -35.56 180)
					(length 2.54)
					(name "FBIO_23")
					(number "E2")
				)
				(pin input line
					(at 52.07 -45.72 180)
					(length 2.54)
					(name "FBIO_29")
					(number "E3")
				)
				(pin input line
					(at 52.07 -50.8 180)
					(length 2.54)
					(name "FBIO_31")
					(number "E4")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "FSOURCE")
					(number "E5")
				)
				(pin input line
					(at 52.07 -58.42 180)
					(length 2.54)
					(name "FBIO_38/SPI_MASTER_MOSI")
					(number "E6")
				)
				(pin input line
					(at 52.07 -66.04 180)
					(length 2.54)
					(name "FBIO_44/SW_DP_IO")
					(number "E7")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "SYS_RSTn")
					(number "F1")
				)
				(pin input line
					(at 52.07 -30.48 180)
					(length 2.54)
					(name "FBIO_20/SPI_SLAVE_SSn")
					(number "F2")
				)
				(pin input line
					(at 52.07 -43.18 180)
					(length 2.54)
					(name "FBIO_28")
					(number "F3")
				)
				(pin input line
					(at 52.07 -48.26 180)
					(length 2.54)
					(name "FBIO_30")
					(number "F4")
				)
				(pin input line
					(at 52.07 -55.88 180)
					(length 2.54)
					(name "FBIO_36/SPI_MASTER_MISO")
					(number "F5")
				)
				(pin input line
					(at 52.07 -60.96 180)
					(length 2.54)
					(name "FBIO_39/SPI_MASTER_SSn1")
					(number "F6")
				)
				(pin input line
					(at 52.07 -68.58 180)
					(length 2.54)
					(name "FBIO_45/SW_DP_CLK")
					(number "F7")
				)
			)
			(embedded_fonts no)
		)
)
