(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EOSAI-S-PUN64"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 91.44 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EOSAI-S-PUN64"
				(at 91.44 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EOSAI-S-PUN64"
				(at 91.44 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.quicklogic.com/wp-content/uploads/2020/12/QL-EOS-S3-Ultra-Low-Power-multicore-MCU-Datasheet-2020.pdf"
				(at 91.44 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "MCU + eFPGA SoC"
				(at 91.44 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EOSAI-S-PUN64"
				(at 91.44 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "QuickLogic"
				(at 91.44 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 91.44 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 91.44 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "FPGA, SOC, MCU"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EOSAI-S-PUN64_0_1")
			(symbol "EOSAI-S-PUN64_1_0"
				(text "BANK A"
					(at 27.94 -48.26 900)
				)
				(text "BANK B"
					(at 30.48 -48.26 900)
				)
			)
			(symbol "EOSAI-S-PUN64_1_1"
				(text "ANALOG"
					(at 27.94 -19.05 900)
				)
				(text "POWER"
					(at 30.48 0 0)
				)
				(text "POWER"
					(at 30.48 -93.98 0)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCCIOA")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 2.54)
					(name "FBIO3/SENSOR_INT_0")
					(number "2")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 2.54)
					(name "FBIO4")
					(number "3")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 2.54)
					(name "FBIO_0/SCL_0")
					(number "4")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 2.54)
					(name "FBIO_1/SDA_0")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "FBIO2")
					(number "6")
				)
				(pin bidirectional line
					(at 60.96 -60.96 180)
					(length 2.54)
					(name "FBIO_43/AP_INTERRUPT")
					(number "7")
				)
				(pin bidirectional line
					(at 60.96 -64.77 180)
					(length 2.54)
					(name "FBIO_44/SW_DP_IO")
					(number "8")
				)
				(pin bidirectional line
					(at 60.96 -67.31 180)
					(length 2.54)
					(name "FBIO_45/SW_DP_CLK")
					(number "9")
				)
				(pin bidirectional line
					(at 60.96 -58.42 180)
					(length 2.54)
					(name "FBIO_42")
					(number "10")
				)
				(pin bidirectional line
					(at 60.96 -80.01 180)
					(length 2.54)
					(name "FBIO_39/SPI_HOST_SSn1")
					(number "11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCCIOB")
					(number "12")
				)
				(pin bidirectional line
					(at 60.96 -53.34 180)
					(length 2.54)
					(name "FBIO_40/M_SSn1")
					(number "13")
				)
				(pin bidirectional line
					(at 60.96 -55.88 180)
					(length 2.54)
					(name "FBIO_41")
					(number "14")
				)
				(pin bidirectional line
					(at 60.96 -50.8 180)
					(length 2.54)
					(name "FBIO_37")
					(number "15")
				)
				(pin bidirectional line
					(at 60.96 -77.47 180)
					(length 2.54)
					(name "FBIO_38/SPI_HOST_MOSI")
					(number "16")
				)
				(pin bidirectional line
					(at 60.96 -74.93 180)
					(length 2.54)
					(name "FBIO_36/SPI_HOST_MISO")
					(number "17")
				)
				(pin bidirectional line
					(at 60.96 -48.26 180)
					(length 2.54)
					(name "FBIO_35")
					(number "18")
				)
				(pin passive line
					(at 0 -85.09 0)
					(length 2.54)
					(name "FSOURCE")
					(number "19")
				)
				(pin bidirectional line
					(at 60.96 -72.39 180)
					(length 2.54)
					(name "FBIO_34/SPI_HOST_CLK")
					(number "20")
				)
				(pin bidirectional line
					(at 60.96 -45.72 180)
					(length 2.54)
					(name "FBIO_33")
					(number "21")
				)
				(pin bidirectional line
					(at 60.96 -43.18 180)
					(length 2.54)
					(name "FBIO_32")
					(number "22")
				)
				(pin bidirectional line
					(at 60.96 -40.64 180)
					(length 2.54)
					(name "FBIO_31")
					(number "23")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VCCIOB")
					(number "24")
				)
				(pin bidirectional line
					(at 60.96 -38.1 180)
					(length 2.54)
					(name "FBIO_30")
					(number "25")
				)
				(pin bidirectional line
					(at 60.96 -35.56 180)
					(length 2.54)
					(name "FBIO_29")
					(number "26")
				)
				(pin bidirectional line
					(at 60.96 -33.02 180)
					(length 2.54)
					(name "FBIO_28")
					(number "27")
				)
				(pin bidirectional line
					(at 60.96 -30.48 180)
					(length 2.54)
					(name "FBIO_27")
					(number "28")
				)
				(pin input line
					(at 0 -90.17 0)
					(length 2.54)
					(name "STM")
					(number "29")
				)
				(pin bidirectional line
					(at 60.96 -27.94 180)
					(length 2.54)
					(name "FBIO_26")
					(number "30")
				)
				(pin bidirectional line
					(at 60.96 -25.4 180)
					(length 2.54)
					(name "FBIO_25")
					(number "31")
				)
				(pin bidirectional line
					(at 60.96 -22.86 180)
					(length 2.54)
					(name "FBIO_24")
					(number "32")
				)
				(pin bidirectional line
					(at 60.96 -20.32 180)
					(length 2.54)
					(name "FBIO_23")
					(number "33")
				)
				(pin bidirectional line
					(at 60.96 -17.78 180)
					(length 2.54)
					(name "FBIO_22")
					(number "34")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VCCIOB")
					(number "35")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 2.54)
					(name "FBIO_19/SPI_DEVICE_MOSI")
					(number "36")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 2.54)
					(name "FBIO_20/SPI_DEVICE_SSn")
					(number "37")
				)
				(pin bidirectional line
					(at 60.96 -12.7 180)
					(length 2.54)
					(name "FBIO_18")
					(number "38")
				)
				(pin bidirectional line
					(at 60.96 -15.24 180)
					(length 2.54)
					(name "FBIO_21")
					(number "39")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 2.54)
					(name "FBIO_16/SPI_DEVICE_CLK")
					(number "40")
				)
				(pin input line
					(at 0 -87.63 0)
					(length 2.54)
					(name "SYS_RSTn")
					(number "41")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 2.54)
					(name "FBIO_17/SPI_DEVICE_MISO")
					(number "42")
				)
				(pin power_in line
					(at 0 -97.79 0)
					(length 2.54)
					(name "AGND")
					(number "43")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "XTAL_I")
					(number "44")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "XTAL_O")
					(number "45")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVDD")
					(number "46")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "ADC1")
					(number "47")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "ADC0")
					(number "48")
				)
				(pin power_out line
					(at 60.96 -3.81 180)
					(length 2.54)
					(name "VDD1")
					(number "49")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "LDO_VIN")
					(number "50")
				)
				(pin power_out line
					(at 60.96 -1.27 180)
					(length 2.54)
					(name "VDD2")
					(number "51")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(hide yes)
					(name "LDO_VIN")
					(number "52")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 2.54)
					(name "FBIO_15/SW_DP_IO")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 2.54)
					(name "FBIO_14/SW_DP_CLK")
					(number "54")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 2.54)
					(name "FBIO13")
					(number "55")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 2.54)
					(name "FBIO12")
					(number "56")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 2.54)
					(name "FBIO11")
					(number "57")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VCCIOA")
					(number "58")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 2.54)
					(name "FBIO_10")
					(number "59")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 2.54)
					(name "FBIO_9")
					(number "60")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 2.54)
					(name "FBIO_8")
					(number "61")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 2.54)
					(name "FBIO_6/FCLK")
					(number "62")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 2.54)
					(name "FBIO7")
					(number "63")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 2.54)
					(name "FBIO5/SDA_0_DPU")
					(number "64")
				)
				(pin power_in line
					(at 0 -95.25 0)
					(length 2.54)
					(name "GND")
					(number "65")
				)
			)
			(embedded_fonts no)
		)
)
