(footprint "QFN-32-1EP_5x5mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -3.169 -3.12 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-32-1EP_5x5mm"
		(at -4.939 3.91 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -4.939 5.91 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.939 7.11 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.939 8.31 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.475 -1.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "2" smd rect
		(at -2.475 -1.248 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "3" smd rect
		(at -2.475 -0.749 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "4" smd rect
		(at -2.475 -0.249 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "5" smd rect
		(at -2.475 0.248 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "6" smd rect
		(at -2.475 0.752 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "7" smd rect
		(at -2.475 1.252 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "8" smd rect
		(at -2.475 1.752 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "9" smd rect
		(at -1.768 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "10" smd rect
		(at -1.269 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "11" smd rect
		(at -0.772 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "12" smd rect
		(at -0.272 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "13" smd rect
		(at 0.229 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "14" smd rect
		(at 0.728 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "15" smd rect
		(at 1.23 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "16" smd rect
		(at 1.73 2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "17" smd rect
		(at 2.475 1.752 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "18" smd rect
		(at 2.475 1.252 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "19" smd rect
		(at 2.475 0.752 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "20" smd rect
		(at 2.475 0.248 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "21" smd rect
		(at 2.475 -0.249 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "22" smd rect
		(at 2.475 -0.749 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "23" smd rect
		(at 2.475 -1.248 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "24" smd rect
		(at 2.475 -1.75 270)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "25" smd rect
		(at 1.73 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "26" smd rect
		(at 1.23 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "27" smd rect
		(at 0.728 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "28" smd rect
		(at 0.229 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "29" smd rect
		(at -0.272 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "30" smd rect
		(at -0.772 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "31" smd rect
		(at -1.269 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "32" smd rect
		(at -1.768 -2.475 270)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.07)
	)
	(pad "33" smd rect
		(at 0 0 270)
		(size 3.45 3.45)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_esp32_c3.glb"
		(offset
			(xyz 0.002 -0.001 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -90 0 0)
		)
	)
)
