(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ESP32-C3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 63.5 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ESP32-C3"
				(at 63.5 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ESP32-C3"
				(at 63.5 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3_datasheet_en.pdf"
				(at 63.5 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ultra-Low-Power SoC with RISC-V Single-Core CPU, 2.4 GHz Wi-Fi (802.11b/g/n) and Bluetooth® 5 (LE)"
				(at 63.5 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Espressif Systems"
				(at 63.5 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ESP32-C3"
				(at 63.5 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 63.5 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 63.5 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MCU, MICROPROCESSOR, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ESP32-C3_1_1"
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "LNA_IN")
					(number "1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD3P3")
					(number "2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDD3P3")
					(number "3")
				)
				(pin bidirectional line
					(at 27.94 0 180)
					(length 2.54)
					(name "GPIO0")
					(number "4")
					(alternate "XTAL_32K_P" passive line)
				)
				(pin bidirectional line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "GPIO1")
					(number "5")
					(alternate "XTAL_32K_N" passive line)
				)
				(pin bidirectional line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "GPIO2")
					(number "6")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CHIP_EN")
					(number "7")
				)
				(pin bidirectional line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "GPIO3")
					(number "8")
				)
				(pin bidirectional line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "GPIO4")
					(number "9")
					(alternate "MTMS" passive line)
				)
				(pin bidirectional line
					(at 27.94 -12.7 180)
					(length 2.54)
					(name "GPIO5")
					(number "10")
					(alternate "MTDI" passive line)
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD3P3_RTC")
					(number "11")
				)
				(pin bidirectional line
					(at 27.94 -15.24 180)
					(length 2.54)
					(name "GPIO6")
					(number "12")
					(alternate "MTCK" passive line)
				)
				(pin bidirectional line
					(at 27.94 -17.78 180)
					(length 2.54)
					(name "GPIO7")
					(number "13")
					(alternate "MTDO" passive line)
				)
				(pin bidirectional line
					(at 27.94 -20.32 180)
					(length 2.54)
					(name "GPIO8")
					(number "14")
				)
				(pin bidirectional line
					(at 27.94 -22.86 180)
					(length 2.54)
					(name "GPIO9")
					(number "15")
				)
				(pin bidirectional line
					(at 27.94 -25.4 180)
					(length 2.54)
					(name "GPIO10")
					(number "16")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDD3P3_CPU")
					(number "17")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD_SPI")
					(number "18")
				)
				(pin bidirectional line
					(at 27.94 -27.94 180)
					(length 2.54)
					(name "GPIO12")
					(number "19")
					(alternate "SPIHD" passive line)
				)
				(pin bidirectional line
					(at 27.94 -30.48 180)
					(length 2.54)
					(name "GPIO13")
					(number "20")
					(alternate "SPIWP" passive line)
				)
				(pin bidirectional line
					(at 27.94 -33.02 180)
					(length 2.54)
					(name "GPIO14")
					(number "21")
					(alternate "SPICS0" passive line)
				)
				(pin bidirectional line
					(at 27.94 -35.56 180)
					(length 2.54)
					(name "GPIO15")
					(number "22")
					(alternate "SPICLK" passive line)
				)
				(pin bidirectional line
					(at 27.94 -38.1 180)
					(length 2.54)
					(name "GPIO16")
					(number "23")
					(alternate "SPID" passive line)
				)
				(pin bidirectional line
					(at 27.94 -40.64 180)
					(length 2.54)
					(name "GPIO17")
					(number "24")
					(alternate "SPIQ" passive line)
				)
				(pin bidirectional line
					(at 27.94 -43.18 180)
					(length 2.54)
					(name "GPIO18")
					(number "25")
					(alternate "USB_D-" passive line)
				)
				(pin bidirectional line
					(at 27.94 -45.72 180)
					(length 2.54)
					(name "GPIO19")
					(number "26")
					(alternate "USB_D+" passive line)
				)
				(pin bidirectional line
					(at 27.94 -48.26 180)
					(length 2.54)
					(name "GPIO20")
					(number "27")
					(alternate "U0RXD" passive line)
				)
				(pin bidirectional line
					(at 27.94 -50.8 180)
					(length 2.54)
					(name "GPIO21")
					(number "28")
					(alternate "U0TXD" passive line)
				)
				(pin passive clock
					(at 0 -26.67 0)
					(length 2.54)
					(name "XTAL_N")
					(number "29")
				)
				(pin passive clock
					(at 0 -24.13 0)
					(length 2.54)
					(name "XTAL_P")
					(number "30")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDA")
					(number "31")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDDA")
					(number "32")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "GND")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
