(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ESP32-D0WDQ6-V3"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ESP32-D0WDQ6-V3"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ESP32-D0WDQ6-V3"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/891/Espressif_Systems_01292021_esp32-1991551.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF System on Chip, WiFi, Bluetooth"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Espressif Systems"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ESP32-D0WDQ6-V3"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "RF, SOC, SMT, WIFI, BLUETOOTH"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ESP32-D0WDQ6-V3_1_1"
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDA")
					(number "1")
				)
				(pin passive line
					(at 40.64 0 180)
					(length 2.54)
					(name "LNA_IN")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VDD3P3")
					(number "3")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(hide yes)
					(name "VDD3P3")
					(number "4")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 2.54)
					(name "SENSOR_VP")
					(number "5")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 2.54)
					(name "SENSOR_CAPP")
					(number "6")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 2.54)
					(name "SENSOR_CAPN")
					(number "7")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 2.54)
					(name "SENSOR_VN")
					(number "8")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "CHIP_PU")
					(number "9")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 2.54)
					(name "VDET_1")
					(number "10")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(name "VDET_2")
					(number "11")
				)
				(pin passive line
					(at 0 -41.91 0)
					(length 2.54)
					(name "32K_XP")
					(number "12")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 2.54)
					(name "32K_XN")
					(number "13")
				)
				(pin passive line
					(at 40.64 -45.72 180)
					(length 2.54)
					(name "GPIO25")
					(number "14")
				)
				(pin passive line
					(at 40.64 -48.26 180)
					(length 2.54)
					(name "GPIO26")
					(number "15")
				)
				(pin passive line
					(at 40.64 -21.59 180)
					(length 2.54)
					(name "GPIO27")
					(number "16")
				)
				(pin passive line
					(at 40.64 -19.05 180)
					(length 2.54)
					(name "MTMS")
					(number "17")
				)
				(pin passive line
					(at 40.64 -16.51 180)
					(length 2.54)
					(name "MTDI")
					(number "18")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 2.54)
					(name "VDD3P3_RTC")
					(number "19")
				)
				(pin passive line
					(at 40.64 -13.97 180)
					(length 2.54)
					(name "MTCK")
					(number "20")
				)
				(pin passive line
					(at 40.64 -11.43 180)
					(length 2.54)
					(name "MTDO")
					(number "21")
				)
				(pin passive line
					(at 40.64 -8.89 180)
					(length 2.54)
					(name "GPIO2")
					(number "22")
				)
				(pin passive line
					(at 40.64 -6.35 180)
					(length 2.54)
					(name "GPIO0")
					(number "23")
				)
				(pin passive line
					(at 40.64 -3.81 180)
					(length 2.54)
					(name "GPIO4")
					(number "24")
				)
				(pin passive line
					(at 40.64 -27.94 180)
					(length 2.54)
					(name "GPIO16")
					(number "25")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD_SDIO")
					(number "26")
				)
				(pin passive line
					(at 40.64 -30.48 180)
					(length 2.54)
					(name "GPIO17")
					(number "27")
				)
				(pin passive line
					(at 40.64 -64.77 180)
					(length 2.54)
					(name "SD_DATA_2")
					(number "28")
				)
				(pin passive line
					(at 40.64 -62.23 180)
					(length 2.54)
					(name "SD_DATA_3")
					(number "29")
				)
				(pin passive line
					(at 40.64 -59.69 180)
					(length 2.54)
					(name "SD_CMD")
					(number "30")
				)
				(pin passive line
					(at 40.64 -57.15 180)
					(length 2.54)
					(name "SD_CLK")
					(number "31")
				)
				(pin passive line
					(at 40.64 -54.61 180)
					(length 2.54)
					(name "SD_DATA_0")
					(number "32")
				)
				(pin passive line
					(at 40.64 -52.07 180)
					(length 2.54)
					(name "SD_DATA_1")
					(number "33")
				)
				(pin passive line
					(at 40.64 -25.4 180)
					(length 2.54)
					(name "GPIO5")
					(number "34")
				)
				(pin passive line
					(at 40.64 -33.02 180)
					(length 2.54)
					(name "GPIO18")
					(number "35")
				)
				(pin passive line
					(at 40.64 -43.18 180)
					(length 2.54)
					(name "GPIO23")
					(number "36")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDD3P3_CPU")
					(number "37")
				)
				(pin passive line
					(at 40.64 -35.56 180)
					(length 2.54)
					(name "GPIO19")
					(number "38")
				)
				(pin passive line
					(at 40.64 -40.64 180)
					(length 2.54)
					(name "GPIO22")
					(number "39")
				)
				(pin passive line
					(at 0 -59.69 0)
					(length 2.54)
					(name "U0RXD")
					(number "40")
				)
				(pin passive line
					(at 0 -62.23 0)
					(length 2.54)
					(name "U0TXD")
					(number "41")
				)
				(pin passive line
					(at 40.64 -38.1 180)
					(length 2.54)
					(name "GPIO21")
					(number "42")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDA")
					(number "43")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 2.54)
					(name "XTAL_N")
					(number "44")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "XTAL_P")
					(number "45")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDA")
					(number "46")
				)
				(pin passive line
					(at 0 -54.61 0)
					(length 2.54)
					(name "CAP2")
					(number "47")
				)
				(pin passive line
					(at 0 -57.15 0)
					(length 2.54)
					(name "CAP1")
					(number "48")
				)
				(pin passive line
					(at 0 -64.77 0)
					(length 2.54)
					(name "GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
