(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "EZX710AT2_S_LMR5"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 76.2 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "EZX710AT2_S_LMR5"
				(at 76.2 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "EZX710AT2_S_LMR5"
				(at 76.2 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.google.com/url?sa=t&source=web&rct=j&opi=89978449&url=https://cdrdv2-public.intel.com/596333/596333_X710-TM4_Datasheet_v_2_4.pdf&ved=2ahUKEwiSuv20_sCOAxXVCRAIHdxGO_UQFnoECBEQAQ&usg=AOvVaw1CjGyrGWE8ZvOdw4VBsY6U"
				(at 76.2 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ethernet ICs Intel Ethernet Controller 10 Gigabit X7"
				(at 76.2 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "EZX710AT2 S LMR5"
				(at 76.2 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Intel"
				(at 76.2 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 76.2 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 76.2 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, IC, ETHERNET"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "EZX710AT2_S_LMR5_1_1"
				(text "PCIe"
					(at 21.59 -71.12 900)
				)
				(text "JTAG"
					(at 22.86 -7.112 900)
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PE_CLK_P")
					(number "AA1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PER_0_P")
					(number "AA5")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PER_0_N")
					(number "AA7")
				)
				(pin input line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PER_4_P")
					(number "AA27")
				)
				(pin input line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PER_5_N")
					(number "AA31")
				)
				(pin input line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PER_6_N")
					(number "AA35")
				)
				(pin input line
					(at 0 -132.08 0)
					(length 5.08)
					(name "PER_7_N")
					(number "AA39")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PE_CLK_N")
					(number "AB2")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PER_1_P")
					(number "AB10")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PER_1_N")
					(number "AB12")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PER_2_P")
					(number "AB16")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PER_2_N")
					(number "AB18")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PER_3_P")
					(number "AB22")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PER_3_N")
					(number "AB24")
				)
				(pin input line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PER_4_N")
					(number "AB28")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PET_0_N")
					(number "AC5")
				)
				(pin output line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PET_5_P")
					(number "AC31")
				)
				(pin output line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PET_6_P")
					(number "AC35")
				)
				(pin output line
					(at 0 -121.92 0)
					(length 5.08)
					(name "PET_7_P")
					(number "AC39")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PET_0_P")
					(number "AD4")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PET_1_P")
					(number "AD8")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PET_1_N")
					(number "AD10")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PET_2_P")
					(number "AD14")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PET_2_N")
					(number "AD16")
				)
				(pin output line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PET_3_P")
					(number "AD20")
				)
				(pin output line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PET_3_N")
					(number "AD22")
				)
				(pin output line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PET_4_P")
					(number "AD26")
				)
				(pin output line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PET_4_N")
					(number "AD28")
				)
				(pin output line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PET_5_N")
					(number "AD32")
				)
				(pin output line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PET_6_N")
					(number "AD36")
				)
				(pin output line
					(at 0 -124.46 0)
					(length 5.08)
					(name "PET_7_N")
					(number "AD40")
				)
				(pin open_collector line
					(at 0 -2.54 0)
					(length 5.08)
					(name "~{PE_WAKE}")
					(number "P2")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "~{PE_RST}")
					(number "R1")
				)
				(pin input line
					(at 35.56 -7.62 180)
					(length 5.08)
					(name "JTDI")
					(number "T36")
				)
				(pin open_collector line
					(at 35.56 -10.16 180)
					(length 5.08)
					(name "JTDO")
					(number "T38")
				)
				(pin input line
					(at 35.56 -2.54 180)
					(length 5.08)
					(name "JTCK")
					(number "U37")
				)
				(pin input line
					(at 35.56 0 180)
					(length 5.08)
					(name "~{JRST}")
					(number "V36")
				)
				(pin input line
					(at 35.56 -5.08 180)
					(length 5.08)
					(name "JTMS")
					(number "V38")
				)
				(pin passive line
					(at 35.56 -129.54 180)
					(length 5.08)
					(name "RBIAS")
					(number "Y10")
				)
				(pin passive line
					(at 35.56 -132.08 180)
					(length 5.08)
					(name "RSENSE")
					(number "Y12")
				)
				(pin input line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PER_5_P")
					(number "Y30")
				)
				(pin input line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PER_6_P")
					(number "Y34")
				)
				(pin input line
					(at 0 -129.54 0)
					(length 5.08)
					(name "PER_7_P")
					(number "Y38")
				)
			)
			(symbol "EZX710AT2_S_LMR5_2_1"
				(text "P0 10GBASE-T"
					(at 15.24 -19.05 900)
				)
				(text "LINE INPUT/OUTPUT"
					(at 20.32 -54.61 900)
				)
				(text "P1 10GBASE-T"
					(at 30.48 -19.05 900)
				)
				(pin input line
					(at 0 -58.42 0)
					(length 5.08)
					(name "SER1_RX_N")
					(number "A5")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 5.08)
					(name "SER1_TX_P")
					(number "A9")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "SER0_RX_N")
					(number "A13")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SER0_TX_P")
					(number "A17")
				)
				(pin bidirectional line
					(at 45.72 0 180)
					(length 5.08)
					(name "P1_A_P")
					(number "A23")
				)
				(pin bidirectional line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "P1_B_N")
					(number "A25")
				)
				(pin bidirectional line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "P1_C_P")
					(number "A27")
				)
				(pin bidirectional line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "P1_D_N")
					(number "A29")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "P0_D_P")
					(number "A33")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "P0_C_N")
					(number "A35")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "P0_B_P")
					(number "A37")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "P0_A_N")
					(number "A39")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "SER1_RX_P")
					(number "B6")
				)
				(pin output line
					(at 0 -50.8 0)
					(length 5.08)
					(name "SER1_TX_N")
					(number "B10")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "SER0_RX_P")
					(number "B14")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 5.08)
					(name "SER0_TX_N")
					(number "B18")
				)
				(pin bidirectional line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "P1_A_N")
					(number "B24")
				)
				(pin bidirectional line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "P1_B_P")
					(number "B26")
				)
				(pin bidirectional line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "P1_C_N")
					(number "B28")
				)
				(pin bidirectional line
					(at 45.72 -22.86 180)
					(length 5.08)
					(name "P1_D_P")
					(number "B30")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "P0_D_N")
					(number "B34")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "P0_C_P")
					(number "B36")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "P0_B_N")
					(number "B38")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "P0_A_P")
					(number "B40")
				)
				(pin passive line
					(at 45.72 -55.88 180)
					(length 5.08)
					(name "BIAS_RDAC")
					(number "E39")
				)
				(pin passive line
					(at 45.72 -58.42 180)
					(length 5.08)
					(name "RESCAL_RES_P")
					(number "J37")
				)
			)
			(symbol "EZX710AT2_S_LMR5_3_1"
				(text "P0 SDP"
					(at 16.51 -37.592 900)
				)
				(text "P1 SDP"
					(at 16.51 -50.8 900)
				)
				(text "NC (pull-up)"
					(at 19.812 -23.368 900)
				)
				(text "P3 SDP"
					(at 30.226 -37.846 900)
				)
				(text "P0 LED"
					(at 30.48 -1.778 0)
				)
				(text "P2 LED"
					(at 30.48 -6.858 0)
				)
				(text "P1 LED"
					(at 30.48 -14.732 0)
				)
				(text "P3 LED"
					(at 30.48 -19.558 0)
				)
				(text "P3 SDP"
					(at 30.48 -51.054 900)
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "REFCLKIN_P")
					(number "C1")
					(alternate "XTAL_IN" input line)
				)
				(pin input line
					(at 0 -58.42 0)
					(length 5.08)
					(name "REFCLKIN_N")
					(number "C3")
					(alternate "XTAL_OUT" output line)
				)
				(pin tri_state line
					(at 0 -30.48 0)
					(length 5.08)
					(name "SDP0_0")
					(number "E5")
				)
				(pin passive line
					(at 45.72 -35.56 180)
					(length 5.08)
					(name "SDP2_2")
					(number "E7")
				)
				(pin passive line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "SDP2_0")
					(number "F6")
				)
				(pin tri_state line
					(at 0 -33.02 0)
					(length 5.08)
					(name "SDP0_1")
					(number "G5")
				)
				(pin passive line
					(at 45.72 -38.1 180)
					(length 5.08)
					(name "SDP2_3")
					(number "G7")
				)
				(pin passive line
					(at 45.72 -60.96 180)
					(length 5.08)
					(name "TPIN_5")
					(number "G17")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "SDP1_3")
					(number "H6")
				)
				(pin passive line
					(at 45.72 -63.5 180)
					(length 5.08)
					(name "TPIN_3")
					(number "H20")
				)
				(pin passive line
					(at 45.72 -33.02 180)
					(length 5.08)
					(name "SDP2_1")
					(number "J7")
				)
				(pin tri_state line
					(at 0 -63.5 0)
					(length 5.08)
					(name "OSC_SEL")
					(number "J9")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "MDIO3_SDA3")
					(number "K2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MDC3_SCL3")
					(number "K4")
				)
				(pin tri_state line
					(at 0 -35.56 0)
					(length 5.08)
					(name "SDP0_2")
					(number "K6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "MDIO2_SDA2")
					(number "L1")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "MDC2_SCL2")
					(number "L3")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "SDP0_3")
					(number "L5")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "MDIO1_SDA1")
					(number "M2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "MDC1_SCL1")
					(number "M4")
				)
				(pin passive line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "SDP3_2")
					(number "M6")
				)
				(pin passive line
					(at 45.72 -50.8 180)
					(length 5.08)
					(name "SDP3_3")
					(number "M8")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "MDIO0_SDA0")
					(number "N1")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "MDC0_SCL0")
					(number "N3")
				)
				(pin passive line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "SDP3_0")
					(number "N5")
				)
				(pin passive line
					(at 45.72 -45.72 180)
					(length 5.08)
					(name "SDP3_1")
					(number "N7")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "SDP1_1")
					(number "P4")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "SDP1_2")
					(number "P6")
				)
				(pin passive line
					(at 45.72 -17.78 180)
					(length 5.08)
					(name "LED3_0")
					(number "R3")
				)
				(pin passive line
					(at 45.72 -20.32 180)
					(length 5.08)
					(name "LED3_1")
					(number "R5")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "SDP1_0")
					(number "R7")
				)
				(pin output line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "LED2_0")
					(number "T4")
				)
				(pin output line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "LED2_1")
					(number "T6")
				)
				(pin passive line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "LED1_0")
					(number "U5")
				)
				(pin passive line
					(at 45.72 -15.24 180)
					(length 5.08)
					(name "LED1_1")
					(number "U7")
				)
				(pin output line
					(at 45.72 0 180)
					(length 5.08)
					(name "LED0_0")
					(number "V4")
				)
				(pin output line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "LED0_1")
					(number "V6")
				)
			)
			(symbol "EZX710AT2_S_LMR5_4_1"
				(text "NC-SI"
					(at 22.86 -16.256 900)
				)
				(text "SMBus"
					(at 27.94 -30.988 900)
				)
				(text "Flash"
					(at 27.94 -47.244 900)
				)
				(text "GPIO"
					(at 30.48 -8.636 900)
				)
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "LAN_PWR_GOOD")
					(number "AB42")
				)
				(pin tri_state line
					(at 0 -33.02 0)
					(length 5.08)
					(name "~{DEV_DIS}")
					(number "D2")
				)
				(pin tri_state line
					(at 0 -43.18 0)
					(length 5.08)
					(name "AUX_PWR")
					(number "E1")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "MAIN_PWR_OK")
					(number "E3")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "NCSI_TXD_0")
					(number "F2")
				)
				(pin output line
					(at 0 -2.54 0)
					(length 5.08)
					(name "NCSI_ARB_OUT")
					(number "F4")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "NCSI_TXD_1")
					(number "G1")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "NCSI_ARB_IN")
					(number "G3")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "NCSI_CLK_IN")
					(number "H2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "NCSI_TX_EN")
					(number "H4")
				)
				(pin passive line
					(at 45.72 -10.16 180)
					(length 5.08)
					(name "GPIO_4")
					(number "H8")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "NCSI_RXD_0")
					(number "J1")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 5.08)
					(name "NCSI_RXD_1")
					(number "J3")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "NCSI_CRS_DV")
					(number "J5")
				)
				(pin tri_state line
					(at 45.72 -12.7 180)
					(length 5.08)
					(name "GPIO_5")
					(number "L7")
				)
				(pin tri_state line
					(at 45.72 -43.18 180)
					(length 5.08)
					(name "FLSH_SCK")
					(number "P40")
				)
				(pin tri_state line
					(at 45.72 -45.72 180)
					(length 5.08)
					(name "FLSH_SI")
					(number "P42")
				)
				(pin open_collector line
					(at 45.72 -27.94 180)
					(length 5.08)
					(name "SMBCLK")
					(number "R39")
				)
				(pin tri_state line
					(at 45.72 -40.64 180)
					(length 5.08)
					(name "~{FLSH_CE}")
					(number "R41")
				)
				(pin open_collector line
					(at 45.72 -30.48 180)
					(length 5.08)
					(name "SMBD")
					(number "T40")
				)
				(pin input line
					(at 45.72 -48.26 180)
					(length 5.08)
					(name "FLSH_SO")
					(number "T42")
				)
				(pin tri_state line
					(at 0 -35.56 0)
					(length 5.08)
					(name "~{PCI_DIS}")
					(number "U3")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "POR_BYPASS")
					(number "U39")
				)
				(pin open_collector line
					(at 45.72 -25.4 180)
					(length 5.08)
					(name "~{SMBALRT}")
					(number "U41")
				)
				(pin tri_state line
					(at 45.72 0 180)
					(length 5.08)
					(name "GPIO_0")
					(number "V40")
				)
				(pin passive line
					(at 45.72 -7.62 180)
					(length 5.08)
					(name "GPIO_3")
					(number "V42")
				)
				(pin passive line
					(at 45.72 -2.54 180)
					(length 5.08)
					(name "GPIO_1")
					(number "W41")
				)
				(pin tri_state line
					(at 45.72 -5.08 180)
					(length 5.08)
					(name "GPIO_2")
					(number "Y42")
				)
			)
			(symbol "EZX710AT2_S_LMR5_5_1"
				(pin passive line
					(at 43.18 -86.36 180)
					(length 5.08)
					(name "RSVDJ23_NC")
					(number "J23")
				)
				(pin passive line
					(at 43.18 -88.9 180)
					(length 5.08)
					(name "RSVDJ25_NC")
					(number "J25")
				)
				(pin passive line
					(at 43.18 -83.82 180)
					(length 5.08)
					(name "RSVDK22_NC")
					(number "K22")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 5.08)
					(name "RSVDK24_NC")
					(number "K24")
				)
				(pin passive line
					(at 43.18 -78.74 180)
					(length 5.08)
					(name "RSVDL23_NC")
					(number "L23")
				)
				(pin passive line
					(at 0 -39.37 0)
					(length 5.08)
					(name "RSVDL25_NC")
					(number "L25")
				)
				(pin passive line
					(at 43.18 -81.28 180)
					(length 5.08)
					(name "RSVDL27_NC")
					(number "L27")
				)
				(pin passive line
					(at 43.18 -68.58 180)
					(length 5.08)
					(name "RSVDM22_NC")
					(number "M22")
				)
				(pin passive line
					(at 43.18 -71.12 180)
					(length 5.08)
					(name "RSVDM24_NC")
					(number "M24")
				)
				(pin passive line
					(at 43.18 -73.66 180)
					(length 5.08)
					(name "RSVDM26_NC")
					(number "M26")
				)
				(pin passive line
					(at 43.18 -76.2 180)
					(length 5.08)
					(name "RSVDM28_NC")
					(number "M28")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "RSVDN9_VSS")
					(number "N9")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -60.96 180)
					(length 5.08)
					(name "RSVDN23_NC")
					(number "N23")
				)
				(pin passive line
					(at 43.18 -63.5 180)
					(length 5.08)
					(name "RSVDN25_NC")
					(number "N25")
				)
				(pin passive line
					(at 43.18 -66.04 180)
					(length 5.08)
					(name "RSVDN27_NC")
					(number "N27")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 5.08)
					(name "RSVDP8_VSS")
					(number "P8")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "RSVDP22_VSS")
					(number "P22")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "RSVDP24_NC")
					(number "P24")
				)
				(pin passive line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "RSVDP26_NC")
					(number "P26")
				)
				(pin passive line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "RSVDP28_NC")
					(number "P28")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 5.08)
					(name "RSVDR9_NC")
					(number "R9")
				)
				(pin passive line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "RSVDR23_NC")
					(number "R23")
				)
				(pin passive line
					(at 43.18 -48.26 180)
					(length 5.08)
					(name "RSVDR25_NC")
					(number "R25")
				)
				(pin passive line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "RSVDR27_NC")
					(number "R27")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "RSVDT22_NC")
					(number "T22")
				)
				(pin passive line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "RSVDT24_NC")
					(number "T24")
				)
				(pin passive line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "RSVDT26_NC")
					(number "T26")
				)
				(pin passive line
					(at 43.18 -43.18 180)
					(length 5.08)
					(name "RSVDT28_NC")
					(number "T28")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 5.08)
					(name "RSVDU9_NC")
					(number "U9")
				)
				(pin passive line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "RSVDU23_NC")
					(number "U23")
				)
				(pin passive line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "RSVDU25_NC")
					(number "U25")
				)
				(pin passive line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "RSVDU27_NC")
					(number "U27")
				)
				(pin passive line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "RSVDU29_NC")
					(number "U29")
				)
				(pin passive line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "RSVDV22_NC")
					(number "V22")
				)
				(pin passive line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "RSVDV24_NC")
					(number "V24")
				)
				(pin passive line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "RSVDV26_NC")
					(number "V26")
				)
				(pin passive line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "RSVDV28_NC")
					(number "V28")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "RSVDW1_VSS")
					(number "W1")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "RSVDW5_VSS")
					(number "W5")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "DEBUG_W7")
					(number "W7")
				)
				(pin passive line
					(at 43.18 -91.44 180)
					(length 5.08)
					(name "RSVDW23_NC")
					(number "W23")
				)
				(pin passive line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "RSVDW25_NC")
					(number "W25")
				)
				(pin passive line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "RSVDW27_NC")
					(number "W27")
				)
				(pin passive line
					(at 43.18 0 180)
					(length 5.08)
					(name "DEBUG_Y16")
					(number "Y16")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "RSVDY18_VSS")
					(number "Y18")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "DEBUG_Y20")
					(number "Y20")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "RSVDY22_VSS")
					(number "Y22")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "RSVDY24_VSS")
					(number "Y24")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
			)
			(symbol "EZX710AT2_S_LMR5_6_1"
				(text "MDIO"
					(at 22.86 -33.02 900)
				)
				(text "RST"
					(at 22.86 -58.928 900)
				)
				(text "JTAG"
					(at 22.86 -72.39 900)
				)
				(text "XTAL IN"
					(at 25.4 -7.366 900)
				)
				(text "XTAL PTP"
					(at 25.4 -18.288 900)
				)
				(text "SYNCE / IEEE1588"
					(at 31.75 -34.29 900)
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "REFCLK_SEL")
					(number "D4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "XTAL_BYPASS")
					(number "D10")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "~{RESET}")
					(number "D12")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 5.08)
					(name "RSVDD14")
					(number "D14")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PHY_TMS")
					(number "D16")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 5.08)
					(name "~{PHY_TRST}")
					(number "D18")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "XTAL_P")
					(number "D42")
				)
				(pin output line
					(at 55.88 -35.56 180)
					(length 5.08)
					(name "SYNCE_LOCK_1")
					(number "E9")
				)
				(pin output line
					(at 55.88 -38.1 180)
					(length 5.08)
					(name "SYNCE_LOCK_2")
					(number "E11")
				)
				(pin output line
					(at 55.88 -27.94 180)
					(length 5.08)
					(name "SYNCE_CLKOUT_3")
					(number "E13")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PHY_TDI")
					(number "E15")
				)
				(pin input line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PHY_TCK")
					(number "E17")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "XTAL_N")
					(number "E41")
				)
				(pin output line
					(at 55.88 -33.02 180)
					(length 5.08)
					(name "SYNCE_LOCK_0")
					(number "F8")
				)
				(pin output line
					(at 55.88 -22.86 180)
					(length 5.08)
					(name "SYNCE_CLKOUT_1")
					(number "F10")
				)
				(pin output line
					(at 55.88 -40.64 180)
					(length 5.08)
					(name "SYNCE_LOCK_3")
					(number "F12")
				)
				(pin passive line
					(at 55.88 -2.54 180)
					(length 5.08)
					(name "P1_INT_MLC")
					(number "F14")
				)
				(pin open_collector line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PHY_TDO")
					(number "F16")
				)
				(pin output line
					(at 55.88 -20.32 180)
					(length 5.08)
					(name "SYNCE_CLKOUT_0")
					(number "G9")
				)
				(pin output line
					(at 55.88 -25.4 180)
					(length 5.08)
					(name "SYNCE_CLKOUT_2")
					(number "G11")
				)
				(pin passive line
					(at 55.88 -86.36 180)
					(length 5.08)
					(name "RSVDG13_NC")
					(number "G13")
				)
				(pin passive line
					(at 55.88 -78.74 180)
					(length 5.08)
					(name "RSVDG15_NC")
					(number "G15")
				)
				(pin passive line
					(at 55.88 -12.7 180)
					(length 5.08)
					(name "P1_PTP_SYNC0")
					(number "H10")
				)
				(pin passive line
					(at 55.88 -15.24 180)
					(length 5.08)
					(name "P1_PTP_SYNC1")
					(number "H12")
				)
				(pin passive line
					(at 55.88 -83.82 180)
					(length 5.08)
					(name "RSVDH14_NC")
					(number "H14")
				)
				(pin passive line
					(at 55.88 -76.2 180)
					(length 5.08)
					(name "RSVDH16_NC")
					(number "H16")
				)
				(pin passive line
					(at 55.88 -45.72 180)
					(length 5.08)
					(name "RSVDH40_VSS")
					(number "H40")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "XTAL_PTP_XTAL_N")
					(number "H42")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "RSVD_J11_VSS")
					(number "J11")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "RSVDJ13_VSS")
					(number "J13")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 55.88 -81.28 180)
					(length 5.08)
					(name "RSVDJ15_NC")
					(number "J15")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "RSVDJ17_VSS")
					(number "J17")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "XTAL_PTP_XTAL_P")
					(number "J41")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "RSVDK30_NC")
					(number "K30")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "RSVDK32_NC")
					(number "K32")
				)
				(pin passive line
					(at 55.88 -48.26 180)
					(length 5.08)
					(name "RSVDK40_1P88V")
					(number "K40")
					(alternate "1V88" power_in line)
					(alternate "RSVD" passive line)
				)
				(pin passive line
					(at 55.88 -50.8 180)
					(length 5.08)
					(name "RSVDK42_VSS")
					(number "K42")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "RSVDL33")
					(number "L33")
				)
				(pin passive line
					(at 55.88 -63.5 180)
					(length 5.08)
					(name "RSVDL35_NC")
					(number "L35")
				)
				(pin passive line
					(at 55.88 -58.42 180)
					(length 5.08)
					(name "RSVDL37_VSS")
					(number "L37")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MDC")
					(number "L41")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "RSVDM34_NC")
					(number "M34")
				)
				(pin passive line
					(at 55.88 -66.04 180)
					(length 5.08)
					(name "RSVDM36_NC")
					(number "M36")
				)
				(pin passive line
					(at 55.88 0 180)
					(length 5.08)
					(name "P0_INT_MLC")
					(number "M40")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "MDIO")
					(number "M42")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "RSVDN33_NC")
					(number "N33")
				)
				(pin passive line
					(at 55.88 -68.58 180)
					(length 5.08)
					(name "RSVDN35_NC")
					(number "N35")
				)
				(pin passive line
					(at 55.88 -55.88 180)
					(length 5.08)
					(name "RSVDN37_VSS")
					(number "N37")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 55.88 -7.62 180)
					(length 5.08)
					(name "P0_PTP_SYNC0")
					(number "N39")
				)
				(pin passive line
					(at 55.88 -10.16 180)
					(length 5.08)
					(name "P0_PTP_SYNC1")
					(number "N41")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "RSVDP34_NC")
					(number "P34")
				)
				(pin passive line
					(at 55.88 -71.12 180)
					(length 5.08)
					(name "RSVDP36_NC")
					(number "P36")
				)
				(pin passive line
					(at 55.88 -53.34 180)
					(length 5.08)
					(name "RSVDP38_VSS")
					(number "P38")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "RSVDR33_NC")
					(number "R33")
				)
				(pin passive line
					(at 55.88 -73.66 180)
					(length 5.08)
					(name "RSVDR37_NC")
					(number "R37")
				)
			)
			(symbol "EZX710AT2_S_LMR5_7_1"
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "RSVDA41_NC")
					(number "A41")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "RSVDB42_NC")
					(number "B42")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "RSVDC21_NC")
					(number "C21")
				)
				(pin passive line
					(at 43.18 -50.8 180)
					(length 5.08)
					(name "RSVDD6_VSS")
					(number "D6")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "RSVDD8_1P88V")
					(number "D8")
					(alternate "1V88" power_in line)
					(alternate "RSVD" passive line)
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "RSVDD20_NC")
					(number "D20")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "RSVDD22_VSS")
					(number "D22")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -55.88 180)
					(length 5.08)
					(name "RSVDD32_NC")
					(number "D32")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "RSVDE19_1P88V")
					(number "E19")
					(alternate "1V88" power_in line)
					(alternate "RSVD" passive line)
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "RSVDE21_VSS")
					(number "E21")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "RSVDE23_VSS")
					(number "E23")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "RSVDE25_VSS")
					(number "E25")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "RSVDF18_VSS")
					(number "F18")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "RSVDF20_VSS")
					(number "F20")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "RSVDF22_VSS")
					(number "F22")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -53.34 180)
					(length 5.08)
					(name "RSVDF38_VSS")
					(number "F38")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "RSVDG19_VSS")
					(number "G19")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "RSVDG21_VSS")
					(number "G21")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "RSVDG23_VSS")
					(number "G23")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "RSVH18_VSS")
					(number "H18")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "RSVDH22_VSS")
					(number "H22")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "RSVDH24_VSS")
					(number "H24")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "RSVDJ19_VSS")
					(number "J19")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "RSVDJ21_VSS")
					(number "J21")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -58.42 180)
					(length 5.08)
					(name "RSVDJ39_NC")
					(number "J39")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "RSVDK26_NC")
					(number "K26")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "RSVDK28_NC")
					(number "K28")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "RSVDK34_NC")
					(number "K34")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "RSVDK36_NC")
					(number "K36")
				)
				(pin passive line
					(at 43.18 0 180)
					(length 5.08)
					(name "RSVDL29_NC")
					(number "L29")
				)
				(pin passive line
					(at 43.18 -45.72 180)
					(length 5.08)
					(name "RSVDL31_VSS")
					(number "L31")
					(alternate "RSVD" passive line)
					(alternate "VSS" power_in line)
				)
				(pin passive line
					(at 43.18 -5.08 180)
					(length 5.08)
					(name "RSVDM30_NC")
					(number "M30")
				)
				(pin passive line
					(at 43.18 -2.54 180)
					(length 5.08)
					(name "RSVDM32_NC")
					(number "M32")
				)
				(pin passive line
					(at 43.18 -10.16 180)
					(length 5.08)
					(name "RSVDN29_NC")
					(number "N29")
				)
				(pin passive line
					(at 43.18 -7.62 180)
					(length 5.08)
					(name "RSVDN31_NC")
					(number "N31")
				)
				(pin passive line
					(at 43.18 -15.24 180)
					(length 5.08)
					(name "RSVDP30_NC")
					(number "P30")
				)
				(pin passive line
					(at 43.18 -12.7 180)
					(length 5.08)
					(name "RSVDP32_NC")
					(number "P32")
				)
				(pin passive line
					(at 43.18 -20.32 180)
					(length 5.08)
					(name "RSVDR29_NC")
					(number "R29")
				)
				(pin passive line
					(at 43.18 -17.78 180)
					(length 5.08)
					(name "RSVDR31_NC")
					(number "R31")
				)
				(pin passive line
					(at 43.18 -25.4 180)
					(length 5.08)
					(name "RSVDT30_NC")
					(number "T30")
				)
				(pin passive line
					(at 43.18 -22.86 180)
					(length 5.08)
					(name "RSVDT32_NC")
					(number "T32")
				)
				(pin passive line
					(at 43.18 -33.02 180)
					(length 5.08)
					(name "RSVDU31_NC")
					(number "U31")
				)
				(pin passive line
					(at 43.18 -30.48 180)
					(length 5.08)
					(name "RSVDU33_NC")
					(number "U33")
				)
				(pin passive line
					(at 43.18 -27.94 180)
					(length 5.08)
					(name "RSVDU35_NC")
					(number "U35")
				)
				(pin passive line
					(at 43.18 -40.64 180)
					(length 5.08)
					(name "RSVDV30_NC")
					(number "V30")
				)
				(pin passive line
					(at 43.18 -38.1 180)
					(length 5.08)
					(name "RSVDV32_NC")
					(number "V32")
				)
				(pin passive line
					(at 43.18 -35.56 180)
					(length 5.08)
					(name "RSVDV34_NC")
					(number "V34")
				)
			)
			(symbol "EZX710AT2_S_LMR5_8_1"
				(text "Power supply"
					(at 19.05 -1.27 0)
				)
				(text "GND"
					(at 30.48 -49.53 900)
				)
				(pin power_in line
					(at 50.8 -40.64 180)
					(length 5.08)
					(name "VSSA")
					(number "A3")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "A7")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "A11")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "A15")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "A19")
				)
				(pin power_in line
					(at 50.8 -43.18 180)
					(length 5.08)
					(name "AVSS")
					(number "A21")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "A31")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA3")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA9")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA11")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA13")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA15")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA17")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA19")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA21")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA23")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA25")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA29")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA33")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA37")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AA41")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB4")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB6")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB8")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB14")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB20")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB26")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB30")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB32")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB34")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB36")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB38")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AB40")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC1")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC3")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC7")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC9")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC11")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC13")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC15")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC17")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC19")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC21")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC23")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC25")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC27")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC29")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC33")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC37")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AC41")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD2")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD6")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD12")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD18")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD24")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD30")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD34")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD38")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "AD42")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "B2")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "B4")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "B8")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "B12")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "B16")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "B20")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "B22")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "B32")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C5")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C7")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C9")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C11")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C13")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C15")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C17")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "C19")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 5.08)
					(name "P1_AVDDL")
					(number "C23")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "P1_AVDDL")
					(number "C25")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "P1_AVDDL")
					(number "C27")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "P1_AVDDL")
					(number "C29")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "C31")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 5.08)
					(name "P0_AVDDL")
					(number "C33")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(hide yes)
					(name "P0_AVDDL")
					(number "C35")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(hide yes)
					(name "P0_AVDDL")
					(number "C37")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(hide yes)
					(name "P0_AVDDL")
					(number "C39")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "C41")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "D24")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "D26")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "D28")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "BIAS_AVDDH")
					(number "D30")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "XGB_AVDDH")
					(number "D34")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "D36")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "D38")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "D40")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 5.08)
					(name "P1_AVDDH")
					(number "E27")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "P1_AVDDH")
					(number "E29")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "E31")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "E33")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "P0_AVDDH")
					(number "E35")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "P0_AVDDH")
					(number "E37")
				)
				(pin power_in line
					(at 50.8 -53.34 180)
					(length 5.08)
					(name "VSS")
					(number "F24")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F26")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F28")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F30")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F32")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F34")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F36")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "F40")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "F42")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDDIO1")
					(number "G25")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "DVDD")
					(number "G27")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DVDD")
					(number "G29")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DVDD")
					(number "G31")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DVDD")
					(number "G33")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "DVDD")
					(number "G35")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDIO1")
					(number "G37")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PLL_VDD")
					(number "G39")
				)
				(pin passive line
					(at 50.8 -43.18 180)
					(length 5.08)
					(hide yes)
					(name "AVSS")
					(number "G41")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "H26")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "H28")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "H30")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "H32")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "H34")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "H36")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "H38")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 5.08)
					(name "XFI_VDD")
					(number "J27")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "XFI_VDD")
					(number "J29")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "XFI_VDD")
					(number "J31")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 5.08)
					(name "XFI_PVDD")
					(number "J33")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "XFI_VDD")
					(number "J35")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "K8")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "K10")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "K12")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "K14")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "K16")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K18")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K20")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "K38")
				)
				(pin power_in line
					(at 50.8 -20.32 180)
					(length 5.08)
					(name "VCC3P3_TX")
					(number "L9")
				)
				(pin power_in line
					(at 50.8 0 180)
					(length 5.08)
					(name "VCCA")
					(number "L11")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "L13")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "L15")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "L17")
				)
				(pin power_in line
					(at 50.8 -5.08 180)
					(length 5.08)
					(name "VCCD")
					(number "L19")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "L21")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 5.08)
					(name "VDDIO2")
					(number "L39")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "M10")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "M12")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "M14")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "M16")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M18")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M20")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VDDP2")
					(number "M38")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "N11")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "N13")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "N15")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "N17")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "N19")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "N21")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P10")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P12")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P14")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P16")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P18")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P20")
				)
				(pin passive line
					(at 50.8 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3")
					(number "R11")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "R13")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "R15")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "R17")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "R19")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "R21")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R35")
				)
				(pin power_in line
					(at 50.8 -25.4 180)
					(length 5.08)
					(name "VCC3P3_SVR")
					(number "T2")
				)
				(pin passive line
					(at 50.8 -10.16 180)
					(length 5.08)
					(name "RSVDT8_VCCD")
					(number "T8")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T10")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T12")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T14")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T16")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T18")
				)
				(pin passive line
					(at 50.8 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T20")
				)
				(pin passive line
					(at 50.8 -15.24 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3")
					(number "T34")
				)
				(pin power_in line
					(at 50.8 -48.26 180)
					(length 5.08)
					(name "VSS_SVR")
					(number "U1")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "U11")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "U13")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "U15")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "U17")
				)
				(pin passive line
					(at 50.8 -5.08 180)
					(length 5.08)
					(hide yes)
					(name "VCCD")
					(number "U19")
				)
				(pin power_in line
					(at 50.8 -15.24 180)
					(length 5.08)
					(name "VCC3P3")
					(number "U21")
				)
				(pin passive line
					(at 50.8 -27.94 180)
					(length 5.08)
					(name "SVR_IND")
					(number "V2")
				)
				(pin passive line
					(at 50.8 -33.02 180)
					(length 5.08)
					(name "RSVDV8_NC")
					(number "V8")
				)
				(pin passive line
					(at 50.8 -35.56 180)
					(length 5.08)
					(name "RSVDV10_NC")
					(number "V10")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "V12")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "V14")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "V16")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "V18")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "V20")
				)
				(pin power_in line
					(at 50.8 -45.72 180)
					(length 5.08)
					(name "RSVDW3_VSS")
					(number "W3")
				)
				(pin power_in line
					(at 50.8 -7.62 180)
					(length 5.08)
					(name "VCCD_A")
					(number "W9")
				)
				(pin power_in line
					(at 50.8 -17.78 180)
					(length 5.08)
					(name "VCC3P3_A")
					(number "W11")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "W13")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "W15")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "W17")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "W19")
				)
				(pin passive line
					(at 50.8 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCA")
					(number "W21")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "W29")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "W31")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "W33")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "W35")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "W37")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "W39")
				)
				(pin power_in line
					(at 50.8 -50.8 180)
					(length 5.08)
					(name "VSS_S")
					(number "Y2")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y4")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y6")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y8")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y14")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y26")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y28")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y32")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y36")
				)
				(pin passive line
					(at 50.8 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSSA")
					(number "Y40")
				)
			)
			(embedded_fonts no)
		)
)
