(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FIN1019MTC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FIN1019MTC"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FIN1019MTC"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FIN1019-D.pdf"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LVDS Driver, LVDS Differential Receiver, -40 °C, 85 °C, 3 V, 3.6 V, TSSOP"
				(at 55.88 -30.48 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FIN1019MTCX"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ON Semiconductor"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, LOGIC, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FIN1019MTC_1_1"
				(text "D"
					(at 8.89 -3.81 0)
				)
				(text "R"
					(at 11.43 -10.16 0)
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DE")
					(number "1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DI")
					(number "2")
				)
				(pin no_connect line
					(at 17.78 -16.51 180)
					(length 2.54)
					(name "NC")
					(number "3")
				)
				(pin output line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RO")
					(number "4")
				)
				(pin no_connect line
					(at 2.54 -2.54 0)
					(length 2.54)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 17.78 -13.97 180)
					(length 2.54)
					(name "NC")
					(number "6")
				)
				(pin power_in line
					(at 0 -16.51 0)
					(length 2.54)
					(name "GND")
					(number "7")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{RE}")
					(number "8")
				)
				(pin input line
					(at 20.32 -11.43 180)
					(length 2.54)
					(name "RI-")
					(number "9")
				)
				(pin input line
					(at 20.32 -8.89 180)
					(length 2.54)
					(name "RI+")
					(number "10")
				)
				(pin output line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "DO-")
					(number "11")
				)
				(pin output line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "DO+")
					(number "12")
				)
				(pin no_connect line
					(at 17.78 0 180)
					(length 2.54)
					(name "NC")
					(number "13")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "14")
				)
			)
			(embedded_fonts no)
		)
)
