(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FM25V02A_DFN"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FM25V02A_DFN"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FM25V02A_DFN"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/3/70/1/Infineon-FM25V02A_256_Kbit_(32K_8)_Serial_(SPI)_F-RAM-DataSheet-v10_00-EN.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FRAM Memory IC 256Kbit SPI 40MHz 8-DFN"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FM25V02A-DG"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Infineon"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, FLASH, SPI, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FM25V02A_DFN_1_1"
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SO")
					(number "2")
					(alternate "O1)" passive line)
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{WP}")
					(number "3")
				)
				(pin power_in line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "V_{SS}")
					(number "4")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "SI")
					(number "5")
					(alternate "O0)" passive line)
				)
				(pin input clock
					(at 0 -12.7 0)
					(length 2.54)
					(name "SCK")
					(number "6")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{HOLD}")
					(number "7")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "V_{DD}")
					(number "8")
				)
				(pin power_in line
					(at 20.32 -10.16 180)
					(length 2.54)
					(name "EP")
					(number "9")
				)
			)
			(embedded_fonts no)
		)
)
