(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "FS32K146UAT0V_LQFP-64"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 60.96 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "FS32K146UAT0V_LQFP-64"
				(at 60.96 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "FS32K146UAT0V_LQFP-64"
				(at 60.96 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/S32K1xx.pdf"
				(at 60.96 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ARM MCU, S32 Family S32K1xx Series Microcontrollers, ARM Cortex-M4F, 32 bit, 112 MHz, 1 MB"
				(at 60.96 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "NXP"
				(at 60.96 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "FS32K146UAT0VLHT"
				(at 60.96 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 60.96 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 60.96 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MCU, ARM, MICROCONTROLLER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "FS32K146UAT0V_LQFP-64_1_1"
				(pin passive line
					(at 34.29 -39.37 180)
					(length 2.54)
					(name "PTD1")
					(number "1")
				)
				(pin passive line
					(at 34.29 -36.83 180)
					(length 2.54)
					(name "PTD0")
					(number "2")
				)
				(pin passive line
					(at 34.29 -91.44 180)
					(length 2.54)
					(name "PTE11")
					(number "3")
				)
				(pin passive line
					(at 34.29 -88.9 180)
					(length 2.54)
					(name "PTE10")
					(number "4")
				)
				(pin passive line
					(at 34.29 -76.2 180)
					(length 2.54)
					(name "PTE5")
					(number "5")
				)
				(pin passive line
					(at 34.29 -73.66 180)
					(length 2.54)
					(name "PTE4")
					(number "6")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDA")
					(number "8")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "VREFH")
					(number "9")
				)
				(pin power_in line
					(at 0 -91.44 0)
					(length 2.54)
					(name "VSS")
					(number "10")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 2.54)
					(name "PTB7")
					(number "11")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 2.54)
					(name "PTB6")
					(number "12")
				)
				(pin passive line
					(at 34.29 -71.12 180)
					(length 2.54)
					(name "PTE3")
					(number "13")
				)
				(pin passive line
					(at 34.29 -59.69 180)
					(length 2.54)
					(name "PTD16")
					(number "14")
				)
				(pin passive line
					(at 34.29 -57.15 180)
					(length 2.54)
					(name "PTD15")
					(number "15")
				)
				(pin passive line
					(at 34.29 -86.36 180)
					(length 2.54)
					(name "PTE9")
					(number "16")
				)
				(pin passive line
					(at 34.29 -83.82 180)
					(length 2.54)
					(name "PTE8")
					(number "17")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 2.54)
					(name "PTB5")
					(number "18")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "PTB4")
					(number "19")
				)
				(pin passive line
					(at 34.29 -7.62 180)
					(length 2.54)
					(name "PTC3")
					(number "20")
				)
				(pin passive line
					(at 34.29 -5.08 180)
					(length 2.54)
					(name "PTC2")
					(number "21")
				)
				(pin passive line
					(at 34.29 -54.61 180)
					(length 2.54)
					(name "PTD7")
					(number "22")
				)
				(pin passive line
					(at 34.29 -52.07 180)
					(length 2.54)
					(name "PTD6")
					(number "23")
				)
				(pin passive line
					(at 34.29 -49.53 180)
					(length 2.54)
					(name "PTD5")
					(number "24")
				)
				(pin passive line
					(at 34.29 -2.54 180)
					(length 2.54)
					(name "PTC1")
					(number "25")
				)
				(pin passive line
					(at 34.29 0 180)
					(length 2.54)
					(name "PTC0")
					(number "26")
				)
				(pin passive line
					(at 34.29 -33.02 180)
					(length 2.54)
					(name "PTC17")
					(number "27")
				)
				(pin passive line
					(at 34.29 -30.48 180)
					(length 2.54)
					(name "PTC16")
					(number "28")
				)
				(pin passive line
					(at 34.29 -27.94 180)
					(length 2.54)
					(name "PTC15")
					(number "29")
				)
				(pin passive line
					(at 34.29 -25.4 180)
					(length 2.54)
					(name "PTC14")
					(number "30")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "PTB3")
					(number "31")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "PTB2")
					(number "32")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(name "PTB1")
					(number "33")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 2.54)
					(name "PTB0")
					(number "34")
				)
				(pin passive line
					(at 34.29 -22.86 180)
					(length 2.54)
					(name "PTC9")
					(number "35")
				)
				(pin passive line
					(at 34.29 -20.32 180)
					(length 2.54)
					(name "PTC8")
					(number "36")
				)
				(pin passive line
					(at 0 -26.67 0)
					(length 2.54)
					(name "PTA7")
					(number "37")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 2.54)
					(name "PTA6")
					(number "38")
				)
				(pin passive line
					(at 34.29 -81.28 180)
					(length 2.54)
					(name "PTE7")
					(number "39")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "40")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "41")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 2.54)
					(name "PTB13")
					(number "42")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 2.54)
					(name "PTB12")
					(number "43")
				)
				(pin passive line
					(at 34.29 -46.99 180)
					(length 2.54)
					(name "PTD4")
					(number "44")
				)
				(pin passive line
					(at 34.29 -44.45 180)
					(length 2.54)
					(name "PTD3")
					(number "45")
				)
				(pin passive line
					(at 34.29 -41.91 180)
					(length 2.54)
					(name "PTD2")
					(number "46")
				)
				(pin passive line
					(at 0 -16.51 0)
					(length 2.54)
					(name "PTA3")
					(number "47")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 2.54)
					(name "PTA2")
					(number "48")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 2.54)
					(name "PTA1")
					(number "49")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 2.54)
					(name "PTA0")
					(number "50")
				)
				(pin passive line
					(at 34.29 -17.78 180)
					(length 2.54)
					(name "PTC7")
					(number "51")
				)
				(pin passive line
					(at 34.29 -15.24 180)
					(length 2.54)
					(name "PTC6")
					(number "52")
				)
				(pin passive line
					(at 34.29 -78.74 180)
					(length 2.54)
					(name "PTE6")
					(number "53")
				)
				(pin passive line
					(at 34.29 -68.58 180)
					(length 2.54)
					(name "PTE2")
					(number "54")
				)
				(pin passive line
					(at 0 -36.83 0)
					(length 2.54)
					(name "PTA13")
					(number "55")
				)
				(pin passive line
					(at 0 -34.29 0)
					(length 2.54)
					(name "PTA12")
					(number "56")
				)
				(pin passive line
					(at 0 -31.75 0)
					(length 2.54)
					(name "PTA11")
					(number "57")
				)
				(pin passive line
					(at 0 -29.21 0)
					(length 2.54)
					(name "PTA10")
					(number "58")
				)
				(pin passive line
					(at 34.29 -66.04 180)
					(length 2.54)
					(name "PTE1")
					(number "59")
				)
				(pin passive line
					(at 34.29 -63.5 180)
					(length 2.54)
					(name "PTE0")
					(number "60")
				)
				(pin passive line
					(at 34.29 -12.7 180)
					(length 2.54)
					(name "PTC5")
					(number "61")
				)
				(pin passive line
					(at 34.29 -10.16 180)
					(length 2.54)
					(name "PTC4")
					(number "62")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 2.54)
					(name "PTA5")
					(number "63")
				)
				(pin passive line
					(at 0 -19.05 0)
					(length 2.54)
					(name "PTA4")
					(number "64")
				)
			)
			(embedded_fonts no)
		)
)
