(footprint "WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3.1 0)
		(layer "F.SilkS")
	)
	(property "Value" "WSON-8-1EP_6x5mm_P1.27mm_EP3.4x4mm"
		(at 0 4 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -4.35 6.85 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -4.35 8.05 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.35 9.25 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3 -1.905 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3 -0.635 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3 0.635 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3 1.905 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at 3 1.905 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at 3 0.635 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at 3 -0.635 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at 3 -1.905 90)
		(size 0.5 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at 0 0)
		(size 3.4 4)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_gd25q16cwigr.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
