(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "GR716"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 57.15 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "GR716A"
				(at 57.15 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "GR716"
				(at 57.15 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.gaisler.com/doc/gr716/gr716-ds-um-3-2.pdf"
				(at 57.15 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Fault-tolerant LEON3 SPARC V8 processor"
				(at 57.15 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GR716A"
				(at 57.15 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Frontgrade"
				(at 57.15 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 57.15 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 57.15 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, MCU"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "GR716_1_1"
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VDD_CORE")
					(number "1")
				)
				(pin power_in line
					(at 30.48 0 180)
					(length 3.81)
					(name "VDD_LDO")
					(number "2")
				)
				(pin power_in line
					(at 0 -24.13 0)
					(length 3.81)
					(name "GND")
					(number "3")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VDD_IO")
					(number "4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "13")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD_CORE")
					(number "15")
				)
				(pin power_in line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "VDDA_ADC")
					(number "19")
				)
				(pin power_in line
					(at 30.48 -24.13 180)
					(length 3.81)
					(name "VSSA_ADC")
					(number "20")
				)
				(pin power_in line
					(at 30.48 -7.62 180)
					(length 3.81)
					(name "VDDA_REF")
					(number "29")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VREFBUF")
					(number "30")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VREF")
					(number "31")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(name "RREF")
					(number "32")
				)
				(pin power_in line
					(at 30.48 -19.05 180)
					(length 3.81)
					(name "VSSA_REF")
					(number "33")
				)
				(pin power_in line
					(at 30.48 -21.59 180)
					(length 3.81)
					(name "VSSA_DAC")
					(number "38")
				)
				(pin power_in line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "VDDA_DAC")
					(number "39")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDD_LVDS")
					(number "40")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "41")
				)
				(pin power_in line
					(at 30.48 -10.16 180)
					(length 3.81)
					(name "VDDA_PLL")
					(number "55")
				)
				(pin power_in line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "VSSA_PLL")
					(number "56")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD_CORE")
					(number "61")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "62")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "63")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "74")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "75")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD_CORE")
					(number "76")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "87")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "88")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD_CORE")
					(number "89")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "101")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "102")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD_CORE")
					(number "103")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "115")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "116")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD_CORE")
					(number "117")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VDD_IO")
					(number "129")
				)
				(pin passive line
					(at 0 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "130")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(hide yes)
					(name "VDD_LDO")
					(number "131")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VDD_CORE")
					(number "132")
				)
			)
			(symbol "GR716_2_1"
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "DUART_RX")
					(number "7")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "DUART_TX")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 3.81)
					(name "SPIM_SEL")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 3.81)
					(name "SPIM_SCK")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 3.81)
					(name "SPIM_MOSI")
					(number "11")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 3.81)
					(name "SPIM_MISO")
					(number "12")
				)
				(pin output line
					(at 34.29 -16.51 180)
					(length 3.81)
					(name "LVDS_TX0_P")
					(number "42")
				)
				(pin output line
					(at 34.29 -19.05 180)
					(length 3.81)
					(name "LVDS_TX0_N")
					(number "43")
				)
				(pin output line
					(at 34.29 -21.59 180)
					(length 3.81)
					(name "LVDS_TX1_P")
					(number "44")
				)
				(pin output line
					(at 34.29 -24.13 180)
					(length 3.81)
					(name "LVDS_TX1_N")
					(number "45")
				)
				(pin output line
					(at 34.29 -26.67 180)
					(length 3.81)
					(name "LVDS_TX2_P")
					(number "46")
				)
				(pin output line
					(at 34.29 -29.21 180)
					(length 3.81)
					(name "LVDS_TX2_N")
					(number "47")
				)
				(pin input line
					(at 34.29 0 180)
					(length 3.81)
					(name "LVDS_RX0_P")
					(number "48")
				)
				(pin input line
					(at 34.29 -2.54 180)
					(length 3.81)
					(name "LVDS_RX0_N")
					(number "49")
				)
				(pin input line
					(at 34.29 -5.08 180)
					(length 3.81)
					(name "LVDS_RX1_P")
					(number "50")
				)
				(pin input line
					(at 34.29 -7.62 180)
					(length 3.81)
					(name "LVDS_RX1_N")
					(number "51")
				)
				(pin input line
					(at 34.29 -10.16 180)
					(length 3.81)
					(name "LVDS_RX2_P")
					(number "52")
				)
				(pin input line
					(at 34.29 -12.7 180)
					(length 3.81)
					(name "LVDS_RX2_N")
					(number "53")
				)
			)
			(symbol "GR716_3_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "GPIO_37")
					(number "21")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "GPIO_38")
					(number "22")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "GPIO_39")
					(number "23")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "GPIO_40")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "GPIO_41")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "GPIO_42")
					(number "26")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "GPIO_43")
					(number "27")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "GPIO_44")
					(number "28")
				)
				(pin bidirectional line
					(at 27.94 0 180)
					(length 3.81)
					(name "GPIO_45")
					(number "34")
				)
				(pin bidirectional line
					(at 27.94 -2.54 180)
					(length 3.81)
					(name "GPIO_46")
					(number "35")
				)
				(pin bidirectional line
					(at 27.94 -5.08 180)
					(length 3.81)
					(name "GPIO_47")
					(number "36")
				)
				(pin bidirectional line
					(at 27.94 -7.62 180)
					(length 3.81)
					(name "GPIO_48")
					(number "37")
				)
			)
			(symbol "GR716_4_1"
				(pin bidirectional line
					(at 33.02 -30.48 180)
					(length 3.81)
					(name "GPIO_49")
					(number "64")
				)
				(pin bidirectional line
					(at 33.02 -33.02 180)
					(length 3.81)
					(name "GPIO_50")
					(number "65")
				)
				(pin bidirectional line
					(at 33.02 -35.56 180)
					(length 3.81)
					(name "GPIO_51")
					(number "66")
				)
				(pin bidirectional line
					(at 33.02 -38.1 180)
					(length 3.81)
					(name "GPIO_52")
					(number "67")
				)
				(pin bidirectional line
					(at 33.02 -40.64 180)
					(length 3.81)
					(name "GPIO_53")
					(number "68")
				)
				(pin bidirectional line
					(at 33.02 -43.18 180)
					(length 3.81)
					(name "GPIO_54")
					(number "69")
				)
				(pin bidirectional line
					(at 33.02 -45.72 180)
					(length 3.81)
					(name "GPIO_55")
					(number "70")
				)
				(pin bidirectional line
					(at 33.02 -48.26 180)
					(length 3.81)
					(name "GPIO_56")
					(number "71")
				)
				(pin bidirectional line
					(at 33.02 -50.8 180)
					(length 3.81)
					(name "GPIO_57")
					(number "72")
				)
				(pin bidirectional line
					(at 33.02 -53.34 180)
					(length 3.81)
					(name "GPIO_58")
					(number "73")
				)
				(pin bidirectional line
					(at 33.02 -55.88 180)
					(length 3.81)
					(name "GPIO_59")
					(number "77")
				)
				(pin bidirectional line
					(at 33.02 -58.42 180)
					(length 3.81)
					(name "GPIO_60")
					(number "78")
				)
				(pin bidirectional line
					(at 33.02 -60.96 180)
					(length 3.81)
					(name "GPIO_61")
					(number "79")
				)
				(pin bidirectional line
					(at 33.02 -63.5 180)
					(length 3.81)
					(name "GPIO_62")
					(number "80")
				)
				(pin bidirectional line
					(at 33.02 -66.04 180)
					(length 3.81)
					(name "GPIO_63")
					(number "81")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "GPIO_0")
					(number "82")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "GPIO_1")
					(number "83")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "GPIO_2")
					(number "84")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "GPIO_3")
					(number "85")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "GPIO_4")
					(number "86")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "GPIO_5")
					(number "90")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "GPIO_6")
					(number "91")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "GPIO_7")
					(number "92")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "GPIO_8")
					(number "93")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "GPIO_9")
					(number "94")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "GPIO_10")
					(number "95")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "GPIO_11")
					(number "96")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "GPIO_12")
					(number "97")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "GPIO_13")
					(number "98")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "GPIO_14")
					(number "99")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "GPIO_15")
					(number "100")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "GPIO_16")
					(number "104")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "GPIO_17")
					(number "105")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "GPIO_18")
					(number "106")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "GPIO_19")
					(number "107")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "GPIO_20")
					(number "108")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "GPIO_21")
					(number "109")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "GPIO_22")
					(number "110")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "GPIO_23")
					(number "111")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "GPIO_24")
					(number "112")
				)
				(pin bidirectional line
					(at 33.02 0 180)
					(length 3.81)
					(name "GPIO_25")
					(number "113")
				)
				(pin bidirectional line
					(at 33.02 -2.54 180)
					(length 3.81)
					(name "GPIO_26")
					(number "114")
				)
				(pin bidirectional line
					(at 33.02 -5.08 180)
					(length 3.81)
					(name "GPIO_27")
					(number "118")
				)
				(pin bidirectional line
					(at 33.02 -7.62 180)
					(length 3.81)
					(name "GPIO_28")
					(number "119")
				)
				(pin bidirectional line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "GPIO_29")
					(number "120")
				)
				(pin bidirectional line
					(at 33.02 -12.7 180)
					(length 3.81)
					(name "GPIO_30")
					(number "121")
				)
				(pin bidirectional line
					(at 33.02 -15.24 180)
					(length 3.81)
					(name "GPIO_31")
					(number "122")
				)
				(pin bidirectional line
					(at 33.02 -17.78 180)
					(length 3.81)
					(name "GPIO_32")
					(number "123")
				)
				(pin bidirectional line
					(at 33.02 -20.32 180)
					(length 3.81)
					(name "GPIO_33")
					(number "124")
				)
				(pin bidirectional line
					(at 33.02 -22.86 180)
					(length 3.81)
					(name "GPIO_34")
					(number "125")
				)
				(pin bidirectional line
					(at 33.02 -25.4 180)
					(length 3.81)
					(name "GPIO_35")
					(number "126")
				)
				(pin bidirectional line
					(at 33.02 -27.94 180)
					(length 3.81)
					(name "GPIO_36")
					(number "127")
				)
			)
			(symbol "GR716_5_1"
				(pin input line
					(at 30.48 -17.78 180)
					(length 3.81)
					(name "DSU_EN")
					(number "5")
				)
				(pin input line
					(at 30.48 -15.24 180)
					(length 3.81)
					(name "DSU_BREAK")
					(number "6")
				)
				(pin output line
					(at 30.48 -5.08 180)
					(length 3.81)
					(name "RESET_OUT_N")
					(number "16")
				)
				(pin input line
					(at 30.48 -2.54 180)
					(length 3.81)
					(name "RESET_IN_N")
					(number "17")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 3.81)
					(name "C_RST")
					(number "18")
				)
				(pin input clock
					(at 0 -17.78 0)
					(length 3.81)
					(name "SPWCLK")
					(number "54")
				)
				(pin input clock
					(at 0 -15.24 0)
					(length 3.81)
					(name "CLK")
					(number "57")
				)
				(pin output line
					(at 0 0 0)
					(length 3.81)
					(name "XO_OUT")
					(number "58")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "XO_X1")
					(number "59")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 3.81)
					(name "XO_X2")
					(number "60")
				)
				(pin input line
					(at 30.48 -12.7 180)
					(length 3.81)
					(name "TESTEN")
					(number "128")
				)
			)
			(embedded_fonts no)
		)
)
