(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "GS2971A"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "GS2971A"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "GS2971A"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/44000000MD3i/kpmMkrmUWgHlbCOwdLzVohMm1SDPoVH85guEGK.KXTc"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SDI receiver"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GS2971A"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Semtech"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "GS2971A_1_1"
				(pin output line
					(at 0 -3.81 0)
					(length 3.81)
					(name "STAT0")
					(number "A5")
				)
				(pin output line
					(at 0 -6.35 0)
					(length 3.81)
					(name "STAT1")
					(number "A6")
				)
				(pin output line
					(at 0 0 0)
					(length 3.81)
					(name "PCLK")
					(number "A8")
				)
				(pin output line
					(at 26.67 -45.72 180)
					(length 3.81)
					(name "DOUT18")
					(number "A9")
				)
				(pin output line
					(at 26.67 -43.18 180)
					(length 3.81)
					(name "DOUT17")
					(number "A10")
				)
				(pin output line
					(at 0 -8.89 0)
					(length 3.81)
					(name "STAT2")
					(number "B5")
				)
				(pin output line
					(at 0 -11.43 0)
					(length 3.81)
					(name "STAT3")
					(number "B6")
				)
				(pin output line
					(at 26.67 -48.26 180)
					(length 3.81)
					(name "DOUT19")
					(number "B8")
				)
				(pin output line
					(at 26.67 -40.64 180)
					(length 3.81)
					(name "DOUT16")
					(number "B9")
				)
				(pin output line
					(at 26.67 -38.1 180)
					(length 3.81)
					(name "DOUT15")
					(number "B10")
				)
				(pin output line
					(at 0 -13.97 0)
					(length 3.81)
					(name "STAT4")
					(number "C5")
				)
				(pin output line
					(at 0 -16.51 0)
					(length 3.81)
					(name "STAT5")
					(number "C6")
				)
				(pin output line
					(at 26.67 -30.48 180)
					(length 3.81)
					(name "DOUT12")
					(number "C8")
				)
				(pin output line
					(at 26.67 -35.56 180)
					(length 3.81)
					(name "DOUT14")
					(number "C9")
				)
				(pin output line
					(at 26.67 -33.02 180)
					(length 3.81)
					(name "DOUT13")
					(number "C10")
				)
				(pin output line
					(at 26.67 -25.4 180)
					(length 3.81)
					(name "DOUT10")
					(number "E9")
				)
				(pin output line
					(at 26.67 -27.94 180)
					(length 3.81)
					(name "DOUT11")
					(number "E10")
				)
				(pin output line
					(at 26.67 -20.32 180)
					(length 3.81)
					(name "DOUT08")
					(number "F9")
				)
				(pin output line
					(at 26.67 -22.86 180)
					(length 3.81)
					(name "DOUT09")
					(number "F10")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 3.81)
					(name "WCLK")
					(number "H4")
				)
				(pin output line
					(at 26.67 -15.24 180)
					(length 3.81)
					(name "DOUT06")
					(number "H9")
				)
				(pin output line
					(at 26.67 -17.78 180)
					(length 3.81)
					(name "DOUT07")
					(number "H10")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 3.81)
					(name "SDO+")
					(number "J1")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 3.81)
					(name "AOUT_{1/2}")
					(number "J3")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 3.81)
					(name "ACLK")
					(number "J4")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 3.81)
					(name "AOUT_{5/6}")
					(number "J5")
				)
				(pin output line
					(at 26.67 -2.54 180)
					(length 3.81)
					(name "DOUT01")
					(number "J8")
				)
				(pin output line
					(at 26.67 -10.16 180)
					(length 3.81)
					(name "DOUT04")
					(number "J9")
				)
				(pin output line
					(at 26.67 -12.7 180)
					(length 3.81)
					(name "DOUT05")
					(number "J10")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 3.81)
					(name "SDO-")
					(number "K1")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 3.81)
					(name "AOUT_{3/4}")
					(number "K3")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 3.81)
					(name "AMCLK")
					(number "K4")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 3.81)
					(name "AOUT_{7/8}")
					(number "K5")
				)
				(pin output line
					(at 26.67 0 180)
					(length 3.81)
					(name "DOUT0")
					(number "K8")
				)
				(pin output line
					(at 26.67 -5.08 180)
					(length 3.81)
					(name "DOUT02")
					(number "K9")
				)
				(pin output line
					(at 26.67 -7.62 180)
					(length 3.81)
					(name "DOUT03")
					(number "K10")
				)
			)
			(symbol "GS2971A_2_1"
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VBG")
					(number "A1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "LF")
					(number "A2")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "LB_CONT")
					(number "A3")
				)
				(pin no_connect line
					(at 3.81 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "RSV")
					(number "B3")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 3.81)
					(name "SDI+")
					(number "C1")
				)
				(pin input line
					(at 31.75 -20.32 180)
					(length 3.81)
					(name "RESET_TRST")
					(number "C7")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 3.81)
					(name "SDI-")
					(number "D1")
				)
				(pin input line
					(at 31.75 -33.02 180)
					(length 3.81)
					(name "SW_EN")
					(number "D7")
				)
				(pin input line
					(at 31.75 -15.24 180)
					(length 3.81)
					(name "JTAG/~{HOST}")
					(number "D8")
				)
				(pin output line
					(at 31.75 -38.1 180)
					(length 3.81)
					(name "SDOUT_TDO")
					(number "E7")
				)
				(pin input line
					(at 31.75 -25.4 180)
					(length 3.81)
					(name "SDIN_TDI")
					(number "E8")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 3.81)
					(name "AGC+")
					(number "F1")
				)
				(pin no_connect line
					(at 3.81 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "RSV")
					(number "F2")
				)
				(pin input line
					(at 31.75 -10.16 180)
					(length 3.81)
					(name "~{CS}_TMS")
					(number "F7")
				)
				(pin input line
					(at 31.75 -22.86 180)
					(length 3.81)
					(name "SCLK_TCK")
					(number "F8")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(name "AGC-")
					(number "G1")
				)
				(pin input line
					(at 31.75 -17.78 180)
					(length 3.81)
					(name "~{RC_BYP}")
					(number "G3")
				)
				(pin bidirectional line
					(at 31.75 -2.54 180)
					(length 3.81)
					(name "~{SMPTE_BYPASS}")
					(number "G7")
				)
				(pin bidirectional line
					(at 31.75 0 180)
					(length 3.81)
					(name "DVB_ASI")
					(number "G8")
				)
				(pin input line
					(at 31.75 -7.62 180)
					(length 3.81)
					(name "AUDIO_EN/~{DIS}")
					(number "H3")
				)
				(pin input line
					(at 31.75 -35.56 180)
					(length 3.81)
					(name "TIM_861")
					(number "H5")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 3.81)
					(name "XTAL_OUT")
					(number "H6")
				)
				(pin input line
					(at 31.75 -5.08 180)
					(length 3.81)
					(name "20BIT/~{10BIT}")
					(number "H7")
				)
				(pin input line
					(at 31.75 -12.7 180)
					(length 3.81)
					(name "IOPROC_EN/~{DIS}")
					(number "H8")
				)
				(pin input line
					(at 31.75 -27.94 180)
					(length 3.81)
					(name "SDO_EN/DIS")
					(number "J2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "XTAL2")
					(number "J6")
				)
				(pin input line
					(at 31.75 -30.48 180)
					(length 3.81)
					(name "STANDBY")
					(number "K2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "XTAL1")
					(number "K6")
				)
			)
			(symbol "GS2971A_3_1"
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCO_{VDD}")
					(number "A4")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "IO_{VDD}")
					(number "A7")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 3.81)
					(name "A_{VDD}")
					(number "B1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PLL_{VDD}")
					(number "B2")
				)
				(pin power_in line
					(at 26.67 0 180)
					(length 3.81)
					(name "VCO_{GND}")
					(number "B4")
				)
				(pin power_in line
					(at 26.67 -15.24 180)
					(length 3.81)
					(name "IO_{GND}")
					(number "B7")
				)
				(pin power_in line
					(at 26.67 -5.08 180)
					(length 3.81)
					(name "A_{GND}")
					(number "C2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "PLL_{VDD}")
					(number "C3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "PLL_{VDD}")
					(number "C4")
				)
				(pin passive line
					(at 26.67 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "A_{GND}")
					(number "D2")
				)
				(pin passive line
					(at 26.67 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "A_{GND}")
					(number "D3")
				)
				(pin power_in line
					(at 26.67 -2.54 180)
					(length 3.81)
					(name "PLL_{GND}")
					(number "D4")
				)
				(pin power_in line
					(at 26.67 -12.7 180)
					(length 3.81)
					(name "CORE_{GND}")
					(number "D5")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "CORE_{VDD}")
					(number "D6")
				)
				(pin passive line
					(at 26.67 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "IO_{GND}")
					(number "D9")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "IO_{VDD}")
					(number "D10")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "EQ_{VDD}")
					(number "E1")
				)
				(pin power_in line
					(at 26.67 -7.62 180)
					(length 3.81)
					(name "EQ_{GND}")
					(number "E2")
				)
				(pin passive line
					(at 26.67 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "A_{GND}")
					(number "E3")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "PLL_{GND}")
					(number "E4")
				)
				(pin passive line
					(at 26.67 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "CORE_{GND}")
					(number "E5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "CORE_{VDD}")
					(number "E6")
				)
				(pin passive line
					(at 26.67 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "A_{GND}")
					(number "F3")
				)
				(pin passive line
					(at 26.67 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "PLL_{GND}")
					(number "F4")
				)
				(pin passive line
					(at 26.67 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "CORE_{GND}")
					(number "F5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "CORE_{VDD}")
					(number "F6")
				)
				(pin passive line
					(at 26.67 -5.08 180)
					(length 3.81)
					(hide yes)
					(name "A_{GND}")
					(number "G2")
				)
				(pin passive line
					(at 26.67 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "CORE_{GND}")
					(number "G4")
				)
				(pin passive line
					(at 26.67 -12.7 180)
					(length 3.81)
					(hide yes)
					(name "CORE_{GND}")
					(number "G5")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "CORE_{VDD}")
					(number "G6")
				)
				(pin passive line
					(at 26.67 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "IO_{GND}")
					(number "G9")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "IO_{VDD}")
					(number "G10")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "BUFF_{VDD}")
					(number "H1")
				)
				(pin power_in line
					(at 26.67 -10.16 180)
					(length 3.81)
					(name "BUFF_{GND}")
					(number "H2")
				)
				(pin passive line
					(at 26.67 -15.24 180)
					(length 3.81)
					(hide yes)
					(name "IO_{GND}")
					(number "J7")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "IO_{VDD}")
					(number "K7")
				)
			)
			(embedded_fonts no)
		)
)
