(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "GS2988"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "GS2988"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "GS2988"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://semtech.my.salesforce.com/sfc/p/#E0000000JelG/a/44000000MDIY/URmNPYk6YrvngFjCh2n.ZRVsjLb90QOH1YLezdH9vhM"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SDI driver"
				(at 43.18 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GS2988-INE3"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Semtech"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, No-RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "GS2988_0_1")
			(symbol "GS2988_1_1"
				(pin input line
					(at 0 -3.81 0)
					(length 2.54)
					(name "DDI+")
					(number "1")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "DDI-")
					(number "2")
				)
				(pin power_in line
					(at 0 -19.05 0)
					(length 2.54)
					(name "V_{EE}")
					(number "3")
				)
				(pin passive line
					(at 22.86 -13.97 180)
					(length 2.54)
					(name "RSET")
					(number "4")
				)
				(pin no_connect line
					(at 20.32 -16.51 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{DISABLE}")
					(number "6")
				)
				(pin no_connect line
					(at 20.32 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "7")
				)
				(pin no_connect line
					(at 20.32 -19.05 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_{CC}")
					(number "9")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "SD/~{HD}")
					(number "10")
				)
				(pin output line
					(at 22.86 -6.35 180)
					(length 2.54)
					(name "SDO-")
					(number "11")
				)
				(pin output line
					(at 22.86 -3.81 180)
					(length 2.54)
					(name "SDO+")
					(number "12")
				)
				(pin no_connect line
					(at 20.32 -20.32 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin output line
					(at 22.86 -11.43 180)
					(length 2.54)
					(name "~{OSP}")
					(number "14")
				)
				(pin no_connect line
					(at 20.32 -21.59 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "15")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{EQ_EN}")
					(number "16")
				)
				(pin passive line
					(at 0 -21.59 0)
					(length 2.54)
					(name "EP")
					(number "17")
				)
			)
			(embedded_fonts no)
		)
)
