(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "GSV2001"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "GSV2001"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "GSV2001"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.gscoolink.com/en/h-nd-41.html"
				(at 38.1 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "1 In to 2 Out HDMI2.0 Repeater with Audio Extraction/Insertion"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "GSV2001"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "GSCoolink Microelectronics"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, SMT, VIDEO, HDMI"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "GSV2001_1_1"
				(pin output line
					(at 25.4 -49.53 180)
					(length 2.54)
					(name "TXB_CN")
					(number "7")
				)
				(pin output line
					(at 25.4 -46.99 180)
					(length 2.54)
					(name "TXB_CP")
					(number "8")
				)
				(pin output line
					(at 25.4 -34.29 180)
					(length 2.54)
					(name "TXB_0N")
					(number "9")
				)
				(pin output line
					(at 25.4 -31.75 180)
					(length 2.54)
					(name "TXB_0P")
					(number "10")
				)
				(pin output line
					(at 25.4 -39.37 180)
					(length 2.54)
					(name "TXB_1N")
					(number "12")
				)
				(pin output line
					(at 25.4 -36.83 180)
					(length 2.54)
					(name "TXB_1P")
					(number "13")
				)
				(pin output line
					(at 25.4 -44.45 180)
					(length 2.54)
					(name "TXB_2N")
					(number "14")
				)
				(pin output line
					(at 25.4 -41.91 180)
					(length 2.54)
					(name "TXB_2P")
					(number "15")
				)
				(pin input line
					(at 25.4 -58.42 180)
					(length 2.54)
					(name "TXB_HPD")
					(number "17")
				)
				(pin bidirectional line
					(at 25.4 -53.34 180)
					(length 2.54)
					(name "TXB_SDA")
					(number "18")
				)
				(pin bidirectional line
					(at 25.4 -55.88 180)
					(length 2.54)
					(name "TXB_SCL")
					(number "19")
				)
				(pin input line
					(at 25.4 -60.96 180)
					(length 2.54)
					(name "TXB_UTILITY")
					(number "20")
				)
				(pin bidirectional line
					(at 25.4 -21.59 180)
					(length 2.54)
					(name "TXA_SDA")
					(number "21")
				)
				(pin bidirectional line
					(at 25.4 -24.13 180)
					(length 2.54)
					(name "TXA_SCL")
					(number "22")
				)
				(pin input line
					(at 25.4 -26.67 180)
					(length 2.54)
					(name "TXA_HPD")
					(number "23")
				)
				(pin output line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "TXA_CN")
					(number "27")
				)
				(pin output line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "TXA_CP")
					(number "28")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "TXA_0N")
					(number "29")
				)
				(pin output line
					(at 25.4 0 180)
					(length 2.54)
					(name "TXA_0P")
					(number "30")
				)
				(pin output line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "TXA_1N")
					(number "32")
				)
				(pin output line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "TXA_1P")
					(number "33")
				)
				(pin output line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "TXA_2N")
					(number "34")
				)
				(pin output line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "TXA_2P")
					(number "35")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RXA_CN")
					(number "61")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "RXA_CP")
					(number "62")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 2.54)
					(name "RXA_0N")
					(number "63")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "RXA_0P")
					(number "64")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "RXA_1N")
					(number "66")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "RXA_1P")
					(number "67")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "RXA_2N")
					(number "68")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RXA_2P")
					(number "69")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 2.54)
					(name "CEC")
					(number "72")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 2.54)
					(name "RX_HPD")
					(number "73")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 2.54)
					(name "RX_SDA")
					(number "74")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "RX_SCL")
					(number "75")
				)
				(pin power_in line
					(at 0 -29.21 0)
					(length 2.54)
					(name "RX_5V")
					(number "76")
				)
			)
			(symbol "GSV2001_2_1"
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "XTALI")
					(number "3")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "XTALO")
					(number "4")
				)
				(pin bidirectional line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "AUD_D0")
					(number "44")
				)
				(pin bidirectional line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "AUD_D1")
					(number "45")
				)
				(pin bidirectional line
					(at 25.4 -12.7 180)
					(length 2.54)
					(name "AUD_D2")
					(number "46")
				)
				(pin bidirectional line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "AUD_D3")
					(number "47")
				)
				(pin bidirectional line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "AUD_D4")
					(number "48")
				)
				(pin bidirectional line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "AUD_D5")
					(number "49")
				)
				(pin bidirectional line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "AUD_SCLK")
					(number "50")
				)
				(pin bidirectional line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "AUD_MCLK")
					(number "51")
				)
				(pin bidirectional line
					(at 25.4 0 180)
					(length 2.54)
					(name "I2C_SDA")
					(number "52")
				)
				(pin bidirectional line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "I2C_SCL")
					(number "53")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "CSB")
					(number "54")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "RESETB")
					(number "55")
				)
				(pin output line
					(at 0 0 0)
					(length 2.54)
					(name "INT")
					(number "56")
				)
				(pin output line
					(at 0 -5.08 0)
					(length 2.54)
					(name "AVMUTE")
					(number "57")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "REXT400")
					(number "71")
				)
			)
			(symbol "GSV2001_3_1"
				(pin power_in line
					(at 25.4 0 180)
					(length 2.54)
					(name "TVDD")
					(number "1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "MPLL_PVDD")
					(number "2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DVDD")
					(number "5")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TXB_AVDD")
					(number "6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TXB_AVDD")
					(number "11")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TXB_AVDD")
					(number "16")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 2.54)
					(name "TX_PVDD")
					(number "24")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXA_AVDD")
					(number "25")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "TVDD")
					(number "26")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXA_AVDD")
					(number "31")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXA_AVDD")
					(number "36")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DVDD")
					(number "37")
				)
				(pin power_in line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "DVDDIO")
					(number "38")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXA_AVDD")
					(number "39")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXA_AVDD")
					(number "40")
				)
				(pin passive line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "DVDDIO")
					(number "41")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXA_AVDD")
					(number "42")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DVDD")
					(number "43")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DVDD")
					(number "58")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RX_AVDD")
					(number "59")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "TVDD")
					(number "60")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RX_AVDD")
					(number "65")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RX_AVDD")
					(number "70")
				)
				(pin power_in line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "GND")
					(number "77")
				)
			)
			(embedded_fonts no)
		)
)
