(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "H26M64103EMR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 39.37 3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "H26M64103EMR"
				(at 39.37 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "H26M64103EMR"
				(at 39.37 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www1.futureelectronics.com/doc/Kingston/EMMCnnn-IB29-PZ90-v1.0.pdf"
				(at 39.37 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "eMMC 32GB"
				(at 39.37 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "H26M64103EMR"
				(at 39.37 1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "SK Hynix"
				(at 39.37 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 39.37 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 39.37 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MEMORY, BGA"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "H26M64103EMR_1_1"
				(pin bidirectional line
					(at 24.13 -10.16 180)
					(length 3.81)
					(name "DAT0")
					(number "A3")
				)
				(pin bidirectional line
					(at 24.13 -12.7 180)
					(length 3.81)
					(name "DAT1")
					(number "A4")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 3.81)
					(name "DAT2")
					(number "A5")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VSS")
					(number "A6")
				)
				(pin passive line
					(at 3.81 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "A7")
				)
				(pin bidirectional line
					(at 24.13 -17.78 180)
					(length 3.81)
					(name "DAT3")
					(number "B2")
				)
				(pin bidirectional line
					(at 24.13 -20.32 180)
					(length 3.81)
					(name "DAT4")
					(number "B3")
				)
				(pin bidirectional line
					(at 24.13 -22.86 180)
					(length 3.81)
					(name "DAT5")
					(number "B4")
				)
				(pin bidirectional line
					(at 24.13 -25.4 180)
					(length 3.81)
					(name "DAT6")
					(number "B5")
				)
				(pin bidirectional line
					(at 24.13 -27.94 180)
					(length 3.81)
					(name "DAT7")
					(number "B6")
				)
				(pin power_in line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "VDDI")
					(number "C2")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VSSQ")
					(number "C4")
				)
				(pin power_in line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "VCCQ")
					(number "C6")
				)
				(pin passive line
					(at 3.81 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "E5")
				)
				(pin power_in line
					(at 24.13 0 180)
					(length 3.81)
					(name "VCC")
					(number "E6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E7")
				)
				(pin passive line
					(at 3.81 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "E8")
				)
				(pin passive line
					(at 3.81 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "VSF")
					(number "E9")
				)
				(pin passive line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VSF")
					(number "E10")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "F5")
				)
				(pin passive line
					(at 3.81 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "VSF")
					(number "F10")
				)
				(pin passive line
					(at 3.81 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "G3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin passive line
					(at 3.81 -13.97 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "G10")
				)
				(pin output line
					(at 24.13 -7.62 180)
					(length 3.81)
					(name "DS")
					(number "H5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H10")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J5")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "J10")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "~{RST}")
					(number "K5")
				)
				(pin passive line
					(at 3.81 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "K6")
				)
				(pin passive line
					(at 3.81 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "K7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K8")
				)
				(pin passive line
					(at 24.13 0 180)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "K9")
				)
				(pin passive line
					(at 3.81 -16.51 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "K10")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "M4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "CMD")
					(number "M5")
				)
				(pin input clock
					(at 0 -2.54 0)
					(length 3.81)
					(name "CLK")
					(number "M6")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "N2")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "N4")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "N5")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "P3")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "P4")
				)
				(pin passive line
					(at 24.13 -2.54 180)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "P5")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "P6")
				)
				(pin passive line
					(at 3.81 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "P7")
				)
				(pin passive line
					(at 3.81 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "P10")
				)
			)
			(embedded_fonts no)
		)
)
