(footprint "QFN-48-1EP_7x7mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -4.275 0)
		(layer "F.SilkS")
	)
	(property "Value" "QFN-48-1EP_7x7mm"
		(at 0 5.749 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "License: Apache-2.0"
		(at -4.45 7.749 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at -4.45 8.949 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -4.45 10.149 0)
		(layer "F.Fab")
	)
	(pad "" smd roundrect
		(at -1.6 -1.6)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at -1.6 0)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at -1.6 1.6)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at 0 -1.6)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at 0 0)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at 0 1.6)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at 1.6 -1.6)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at 1.6 0)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "" smd roundrect
		(at 1.6 1.6)
		(size 1.4 1.4)
		(layers "F.Paste")
		(roundrect_rratio 0.05)
	)
	(pad "1" smd rect
		(at -3.475 -2.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -3.475 -2.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -3.475 -1.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -3.475 -1.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -3.475 -0.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -3.475 -0.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -3.475 0.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -3.475 0.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -3.475 1.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -3.475 1.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -3.475 2.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -3.475 2.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -2.75 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -2.25 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at -1.75 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at -1.25 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at -0.75 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at -0.25 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 0.25 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 0.75 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 1.25 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 1.75 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 2.25 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 2.75 3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 3.475 2.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 3.475 2.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 3.475 1.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 3.475 1.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 3.475 0.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "30" smd rect
		(at 3.475 0.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "31" smd rect
		(at 3.475 -0.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "32" smd rect
		(at 3.475 -0.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "33" smd rect
		(at 3.475 -1.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "34" smd rect
		(at 3.475 -1.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "35" smd rect
		(at 3.475 -2.25)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "36" smd rect
		(at 3.475 -2.75)
		(size 0.85 0.28)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "37" smd rect
		(at 2.75 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "38" smd rect
		(at 2.25 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "39" smd rect
		(at 1.75 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "40" smd rect
		(at 1.25 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "41" smd rect
		(at 0.75 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "42" smd rect
		(at 0.25 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "43" smd rect
		(at -0.25 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "44" smd rect
		(at -0.75 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "45" smd rect
		(at -1.25 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "46" smd rect
		(at -1.75 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "47" smd rect
		(at -2.25 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "48" smd rect
		(at -2.75 -3.475)
		(size 0.28 0.85)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "49" smd rect
		(at 0 0)
		(size 5.15 5.15)
		(layers "F.Cu" "F.Mask")
	)
	(embedded_fonts no)
	(model "antmicro_ice40up5k_sg48itr50.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
