(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ICE40UP5K-SG48"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 63.5 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ICE40UP5K-SG48"
				(at 63.5 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ICE40UP5K-SG48"
				(at 63.5 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.latticesemi.com/~/media/LatticeSemi/Documents/DataSheets/iCE/iCE40%20UltraPlus%20Family%20Data%20Sheet.pdf?document_id=51968"
				(at 63.5 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "iCE40 UltraPlus™ Field Programmable Gate Array"
				(at 63.5 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ICE40UP5K-SG48ITR50"
				(at 63.5 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lattice Semiconductor"
				(at 63.5 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 63.5 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 63.5 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, FPGA, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ICE40UP5K-SG48_1_1"
				(text "BANK 1"
					(at 24.13 -24.13 900)
				)
				(text "BANK 0"
					(at 33.02 -24.13 900)
				)
				(text "BANK 2"
					(at 33.02 -58.42 900)
				)
				(pin power_in line
					(at 0 -60.96 0)
					(length 2.54)
					(name "VCCIO_2")
					(number "1")
				)
				(pin bidirectional line
					(at 50.8 -58.42 180)
					(length 2.54)
					(name "IOB_6A")
					(number "2")
				)
				(pin bidirectional line
					(at 50.8 -63.5 180)
					(length 2.54)
					(name "IOB_9B")
					(number "3")
				)
				(pin bidirectional line
					(at 50.8 -60.96 180)
					(length 2.54)
					(name "IOB_8A")
					(number "4")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(hide yes)
					(name "VCC")
					(number "5")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "IOB_13B")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "CDONE")
					(number "7")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{CRESET_B}")
					(number "8")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "IOB_16A")
					(number "9")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "IOB_18A")
					(number "10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "IOB_20A")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "IOB_22A")
					(number "12")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "IOB_24A")
					(number "13")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 2.54)
					(name "IOB_32A_SPI_SO")
					(number "14")
				)
				(pin bidirectional clock
					(at 0 -40.64 0)
					(length 2.54)
					(name "IOB_34A_SPI_SCK")
					(number "15")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 2.54)
					(name "IOB_35B_SPI_SS")
					(number "16")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 2.54)
					(name "IOB_33B_SPI_SI")
					(number "17")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "IOB_31B")
					(number "18")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 2.54)
					(name "IOB_29B")
					(number "19")
				)
				(pin bidirectional clock
					(at 0 -25.4 0)
					(length 2.54)
					(name "IOB_25B_G3")
					(number "20")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "IOB_23B")
					(number "21")
				)
				(pin power_in line
					(at 0 -58.42 0)
					(length 2.54)
					(name "SPI_VCCIO_1")
					(number "22")
				)
				(pin bidirectional line
					(at 50.8 -2.54 180)
					(length 2.54)
					(name "IOT_37A")
					(number "23")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 2.54)
					(name "VPP_2V5")
					(number "24")
				)
				(pin bidirectional line
					(at 50.8 0 180)
					(length 2.54)
					(name "IOT_36B")
					(number "25")
				)
				(pin bidirectional line
					(at 50.8 -7.62 180)
					(length 2.54)
					(name "IOT_39A")
					(number "26")
				)
				(pin bidirectional line
					(at 50.8 -5.08 180)
					(length 2.54)
					(name "IOT_38B")
					(number "27")
				)
				(pin bidirectional line
					(at 50.8 -10.16 180)
					(length 2.54)
					(name "IOT_41A")
					(number "28")
				)
				(pin power_in line
					(at 0 -50.8 0)
					(length 2.54)
					(name "VCCPLL")
					(number "29")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "VCC")
					(number "30")
				)
				(pin bidirectional line
					(at 50.8 -12.7 180)
					(length 2.54)
					(name "IOT_42B")
					(number "31")
				)
				(pin bidirectional line
					(at 50.8 -15.24 180)
					(length 2.54)
					(name "IOT_43A")
					(number "32")
				)
				(pin power_in line
					(at 0 -55.88 0)
					(length 2.54)
					(name "VCCIO_0")
					(number "33")
				)
				(pin bidirectional line
					(at 50.8 -17.78 180)
					(length 2.54)
					(name "IOT_44B")
					(number "34")
				)
				(pin bidirectional clock
					(at 50.8 -22.86 180)
					(length 2.54)
					(name "IOT_46B_G0")
					(number "35")
				)
				(pin bidirectional line
					(at 50.8 -25.4 180)
					(length 2.54)
					(name "IOT_48B")
					(number "36")
				)
				(pin bidirectional clock
					(at 50.8 -20.32 180)
					(length 2.54)
					(name "IOT_45A_G1")
					(number "37")
				)
				(pin bidirectional line
					(at 50.8 -30.48 180)
					(length 2.54)
					(name "IOT_50B")
					(number "38")
				)
				(pin bidirectional line
					(at 50.8 -35.56 180)
					(length 2.54)
					(name "RGB0")
					(number "39")
				)
				(pin bidirectional line
					(at 50.8 -38.1 180)
					(length 2.54)
					(name "RGB1")
					(number "40")
				)
				(pin bidirectional line
					(at 50.8 -40.64 180)
					(length 2.54)
					(name "RGB2")
					(number "41")
				)
				(pin bidirectional line
					(at 50.8 -33.02 180)
					(length 2.54)
					(name "IOT_51A")
					(number "42")
				)
				(pin bidirectional line
					(at 50.8 -27.94 180)
					(length 2.54)
					(name "IOT_49A")
					(number "43")
				)
				(pin bidirectional clock
					(at 50.8 -50.8 180)
					(length 2.54)
					(name "IOB_3B_G6")
					(number "44")
				)
				(pin bidirectional line
					(at 50.8 -55.88 180)
					(length 2.54)
					(name "IOB_5B")
					(number "45")
				)
				(pin bidirectional line
					(at 50.8 -45.72 180)
					(length 2.54)
					(name "IOB_0A")
					(number "46")
				)
				(pin bidirectional line
					(at 50.8 -48.26 180)
					(length 2.54)
					(name "IOB_2A")
					(number "47")
				)
				(pin bidirectional line
					(at 50.8 -53.34 180)
					(length 2.54)
					(name "IOB_4A")
					(number "48")
				)
				(pin power_in line
					(at 0 -63.5 0)
					(length 2.54)
					(name "GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
