(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ICM-42670-P"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 38.1 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ICM-42670-P"
				(at 38.1 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ICM-42670-P"
				(at 38.1 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://product.tdk.com/system/files/dam/doc/product/sensor/mortion-inertial/imu/data_sheet/ds-000451-icm-42670-p.pdf"
				(at 38.1 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "6-Axis MotionTracking IMU with I3C, I2C and SPI interface"
				(at 38.1 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "TDK"
				(at 38.1 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ICM-42670-P"
				(at 38.1 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 38.1 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 38.1 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, IMU, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "InvenSense?QFN*3x3mm*P0.4mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ICM-42670-P_1_1"
				(pin output line
					(at 0 -11.43 0)
					(length 2.54)
					(name "SDO")
					(number "1")
					(alternate "AD0" input line)
				)
				(pin passive line
					(at 21.59 -6.35 180)
					(length 2.54)
					(name "RESV")
					(number "2")
				)
				(pin passive line
					(at 21.59 -8.89 180)
					(length 2.54)
					(name "RESV")
					(number "3")
				)
				(pin output line
					(at 21.59 0 180)
					(length 2.54)
					(name "INT1")
					(number "4")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "5")
				)
				(pin power_in line
					(at 21.59 -17.78 180)
					(length 2.54)
					(name "GND")
					(number "6")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "FSYNC")
					(number "7")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
				(pin output line
					(at 21.59 -2.54 180)
					(length 2.54)
					(name "INT2")
					(number "9")
				)
				(pin passive line
					(at 21.59 -11.43 180)
					(length 2.54)
					(name "RESV")
					(number "10")
				)
				(pin passive line
					(at 21.59 -13.97 180)
					(length 2.54)
					(name "RESV")
					(number "11")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "CS")
					(number "12")
				)
				(pin input line
					(at 0 -6.35 0)
					(length 2.54)
					(name "SCL")
					(number "13")
					(alternate "SCLK" passive line)
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 2.54)
					(name "SDA")
					(number "14")
					(alternate "SDI" input line)
					(alternate "SDIO" bidirectional line)
				)
			)
			(embedded_fonts no)
		)
)
