(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IP4856CX25_CZ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IP4856CX25_CZ"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IP4856CX25_CZ"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/IP4856CX25_C.pdf"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Level shifter"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IP4856CX25/CZ"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Nexperia"
				(at 35.56 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IP4856CX25_CZ_1_1"
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 2.54)
					(name "DATA2_H")
					(number "A1")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DIR_CMD")
					(number "A2")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DIR_0")
					(number "A3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VSUPPLY")
					(number "A4")
				)
				(pin bidirectional line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "DATA2_SD")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 2.54)
					(name "DATA3_H")
					(number "B1")
				)
				(pin input line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "SEL")
					(number "B2")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VCCA")
					(number "B3")
				)
				(pin passive line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "VLDO")
					(number "B4")
				)
				(pin bidirectional line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "DATA3_SD")
					(number "B5")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "CLK_IN")
					(number "C1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "ENABLE")
					(number "C2")
				)
				(pin power_in line
					(at 0 -52.07 0)
					(length 2.54)
					(name "GND")
					(number "C3")
				)
				(pin input line
					(at 25.4 0 180)
					(length 2.54)
					(name "VSD_REF")
					(number "C4")
				)
				(pin output line
					(at 25.4 -36.83 180)
					(length 2.54)
					(name "CLK_SD")
					(number "C5")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DATA0_H")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 2.54)
					(name "CMD_H")
					(number "D2")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 2.54)
					(name "CD")
					(number "D3")
				)
				(pin bidirectional line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "CMD_SD")
					(number "D4")
				)
				(pin bidirectional line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "DATA0_SD")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DATA1_H")
					(number "E1")
				)
				(pin output line
					(at 0 -40.64 0)
					(length 2.54)
					(name "CLK_FB")
					(number "E2")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DIR_1_3")
					(number "E3")
				)
				(pin output line
					(at 0 -48.26 0)
					(length 2.54)
					(name "WP")
					(number "E4")
				)
				(pin bidirectional line
					(at 25.4 -20.32 180)
					(length 2.54)
					(name "DATA1_SD")
					(number "E5")
				)
			)
			(embedded_fonts no)
		)
)
