(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IS25LP01GJ-RMLE"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 45.72 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IS25LP01GJ-RMLE"
				(at 45.72 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IS25LP01GJ-RMLE"
				(at 45.72 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.issi.com/WW/pdf/25LP-WP01GJ.pdf"
				(at 45.72 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NOR Flash 1Gb QPI/QSPI, 16-pin SOP 300Mil, RoHS"
				(at 45.72 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "ISSI"
				(at 45.72 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IS25LP01GJ-RMLE-TY"
				(at 45.72 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 45.72 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 45.72 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MEMORY, FLASH, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IS25LP01GJ-RMLE_1_1"
				(pin input line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "~{HOLD}")
					(number "1")
					(alternate "IO3" bidirectional line)
					(alternate "~{RESET}" input line)
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VCC")
					(number "2")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "4")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "5")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{CE}")
					(number "7")
				)
				(pin output line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "SO")
					(number "8")
					(alternate "IO1" bidirectional line)
				)
				(pin input line
					(at 25.4 -5.08 180)
					(length 2.54)
					(name "~{WP}")
					(number "9")
					(alternate "IO2" bidirectional line)
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 2.54)
					(name "GND")
					(number "10")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "11")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "12")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin no_connect line
					(at 22.86 -17.78 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "14")
				)
				(pin input line
					(at 25.4 0 180)
					(length 2.54)
					(name "SI")
					(number "15")
					(alternate "IO0" bidirectional line)
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SCK")
					(number "16")
				)
			)
			(embedded_fonts no)
		)
)
