(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IS25WX064-JHLE"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 33.02 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IS25WX064-JHLE"
				(at 33.02 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IS25WX064-JHLE"
				(at 33.02 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.issi.com/WW/pdf/25LX-WX032-064.pdf"
				(at 33.02 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "NOR Flash 64Mb, Octal Flash, 1.8V, 24-ball TFBGA, RoHS, Automotive Grade A3"
				(at 33.02 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IS25WX064-JHLE"
				(at 33.02 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "ISSI"
				(at 33.02 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 33.02 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 33.02 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MEMORY, FLASH, BGA, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IS25WX064-JHLE_1_1"
				(pin no_connect line
					(at 16.51 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "A2")
				)
				(pin no_connect line
					(at 16.51 -15.24 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "A3")
				)
				(pin input line
					(at 0 0 0)
					(length 2.54)
					(name "~{RESET}")
					(number "A4")
				)
				(pin bidirectional line
					(at 19.05 -5.08 180)
					(length 2.54)
					(name "~{ERR}")
					(number "A5")
				)
				(pin no_connect line
					(at 16.51 -13.97 180)
					(length 2.54)
					(hide yes)
					(name "RFU")
					(number "B1")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "C")
					(number "B2")
				)
				(pin power_in line
					(at 19.05 -30.48 180)
					(length 2.54)
					(name "VSS")
					(number "B3")
				)
				(pin power_in line
					(at 19.05 0 180)
					(length 2.54)
					(name "VCC")
					(number "B4")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "DNU")
					(number "B5")
				)
				(pin power_in line
					(at 19.05 -27.94 180)
					(length 2.54)
					(name "VSSQ")
					(number "C1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "~{S}")
					(number "C2")
				)
				(pin output line
					(at 19.05 -7.62 180)
					(length 2.54)
					(name "DQS")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DQ2/~{W}")
					(number "C4")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 2.54)
					(name "Vpp")
					(number "C5")
				)
				(pin power_in line
					(at 19.05 -2.54 180)
					(length 2.54)
					(name "VCCQ")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DQ1")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "DQ0")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "DQ3")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "DQ4")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "DQ7")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 2.54)
					(name "DQ6")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 2.54)
					(name "DQ5")
					(number "E3")
				)
				(pin passive line
					(at 19.05 -2.54 180)
					(length 2.54)
					(hide yes)
					(name "VCCQ")
					(number "E4")
				)
				(pin passive line
					(at 19.05 -27.94 180)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "E5")
				)
			)
			(embedded_fonts no)
		)
)
