(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IS42S32800G-6BL"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 43.18 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IS42S32800G-6BL"
				(at 43.18 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IS42S32800G-6BL"
				(at 43.18 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.issi.com/WW/pdf/42-45S32800G.pdf"
				(at 43.18 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "DRAM 256M, 3.3V, SDRAM, 8Mx32, 166Mhz, 90 ball BGA (8mmx13mm)"
				(at 43.18 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "ISSI"
				(at 43.18 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IS42S32800G-6BL"
				(at 43.18 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 43.18 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 43.18 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, SDRAM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IS42S32800G-6BL_1_1"
				(pin bidirectional line
					(at 29.21 -66.04 180)
					(length 2.54)
					(name "DQ26")
					(number "A1")
				)
				(pin bidirectional line
					(at 29.21 -60.96 180)
					(length 2.54)
					(name "DQ24")
					(number "A2")
				)
				(pin power_in line
					(at 0 -87.63 0)
					(length 2.54)
					(name "VSS")
					(number "A3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "VDD")
					(number "A7")
				)
				(pin bidirectional line
					(at 29.21 -58.42 180)
					(length 2.54)
					(name "DQ23")
					(number "A8")
				)
				(pin bidirectional line
					(at 29.21 -53.34 180)
					(length 2.54)
					(name "DQ21")
					(number "A9")
				)
				(pin bidirectional line
					(at 29.21 -71.12 180)
					(length 2.54)
					(name "DQ28")
					(number "B1")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDDQ")
					(number "B2")
				)
				(pin power_in line
					(at 0 -90.17 0)
					(length 2.54)
					(name "VSSQ")
					(number "B3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "B7")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "B8")
				)
				(pin bidirectional line
					(at 29.21 -48.26 180)
					(length 2.54)
					(name "DQ19")
					(number "B9")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "C1")
				)
				(pin bidirectional line
					(at 29.21 -68.58 180)
					(length 2.54)
					(name "DQ27")
					(number "C2")
				)
				(pin bidirectional line
					(at 29.21 -63.5 180)
					(length 2.54)
					(name "DQ25")
					(number "C3")
				)
				(pin bidirectional line
					(at 29.21 -55.88 180)
					(length 2.54)
					(name "DQ22")
					(number "C7")
				)
				(pin bidirectional line
					(at 29.21 -50.8 180)
					(length 2.54)
					(name "DQ20")
					(number "C8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "C9")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "D1")
				)
				(pin bidirectional line
					(at 29.21 -73.66 180)
					(length 2.54)
					(name "DQ29")
					(number "D2")
				)
				(pin bidirectional line
					(at 29.21 -76.2 180)
					(length 2.54)
					(name "DQ30")
					(number "D3")
				)
				(pin bidirectional line
					(at 29.21 -43.18 180)
					(length 2.54)
					(name "DQ17")
					(number "D7")
				)
				(pin bidirectional line
					(at 29.21 -45.72 180)
					(length 2.54)
					(name "DQ18")
					(number "D8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "D9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "E1")
				)
				(pin bidirectional line
					(at 29.21 -78.74 180)
					(length 2.54)
					(name "DQ31")
					(number "E2")
				)
				(pin no_connect line
					(at 2.54 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "E3")
				)
				(pin no_connect line
					(at 2.54 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "E7")
				)
				(pin bidirectional line
					(at 29.21 -40.64 180)
					(length 2.54)
					(name "DQ16")
					(number "E8")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "E9")
				)
				(pin passive line
					(at 0 -87.63 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "F1")
				)
				(pin input line
					(at 0 -80.01 0)
					(length 2.54)
					(name "DQM3")
					(number "F2")
				)
				(pin input line
					(at 0 -26.67 0)
					(length 2.54)
					(name "A3")
					(number "F3")
				)
				(pin input line
					(at 0 -24.13 0)
					(length 2.54)
					(name "A2")
					(number "F7")
				)
				(pin input line
					(at 0 -77.47 0)
					(length 2.54)
					(name "DQM2")
					(number "F8")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "F9")
				)
				(pin input line
					(at 0 -29.21 0)
					(length 2.54)
					(name "A4")
					(number "G1")
				)
				(pin input line
					(at 0 -31.75 0)
					(length 2.54)
					(name "A5")
					(number "G2")
				)
				(pin input line
					(at 0 -34.29 0)
					(length 2.54)
					(name "A6")
					(number "G3")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 2.54)
					(name "A10")
					(number "G7")
				)
				(pin input line
					(at 0 -19.05 0)
					(length 2.54)
					(name "A0")
					(number "G8")
				)
				(pin input line
					(at 0 -21.59 0)
					(length 2.54)
					(name "A1")
					(number "G9")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "A7")
					(number "H1")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "A8")
					(number "H2")
				)
				(pin no_connect line
					(at 2.54 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "H3")
				)
				(pin no_connect line
					(at 2.54 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "H7")
				)
				(pin input line
					(at 0 -54.61 0)
					(length 2.54)
					(name "BA1")
					(number "H8")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "A11")
					(number "H9")
				)
				(pin input clock
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLK")
					(number "J1")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "CKE")
					(number "J2")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "A9")
					(number "J3")
				)
				(pin input line
					(at 0 -52.07 0)
					(length 2.54)
					(name "BA0")
					(number "J7")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 2.54)
					(name "~{CS}")
					(number "J8")
				)
				(pin input line
					(at 0 -62.23 0)
					(length 2.54)
					(name "~{RAS}")
					(number "J9")
				)
				(pin input line
					(at 0 -74.93 0)
					(length 2.54)
					(name "DQM1")
					(number "K1")
				)
				(pin no_connect line
					(at 2.54 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "K2")
				)
				(pin no_connect line
					(at 2.54 -83.82 0)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "K3")
				)
				(pin input line
					(at 0 -64.77 0)
					(length 2.54)
					(name "~{CAS}")
					(number "K7")
				)
				(pin input line
					(at 0 -67.31 0)
					(length 2.54)
					(name "~{WE}")
					(number "K8")
				)
				(pin input line
					(at 0 -72.39 0)
					(length 2.54)
					(name "DQM0")
					(number "K9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "L1")
				)
				(pin bidirectional line
					(at 29.21 -20.32 180)
					(length 2.54)
					(name "DQ8")
					(number "L2")
				)
				(pin passive line
					(at 0 -87.63 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "L3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "L7")
				)
				(pin bidirectional line
					(at 29.21 -17.78 180)
					(length 2.54)
					(name "DQ7")
					(number "L8")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "L9")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "M1")
				)
				(pin bidirectional line
					(at 29.21 -25.4 180)
					(length 2.54)
					(name "DQ10")
					(number "M2")
				)
				(pin bidirectional line
					(at 29.21 -22.86 180)
					(length 2.54)
					(name "DQ9")
					(number "M3")
				)
				(pin bidirectional line
					(at 29.21 -15.24 180)
					(length 2.54)
					(name "DQ6")
					(number "M7")
				)
				(pin bidirectional line
					(at 29.21 -12.7 180)
					(length 2.54)
					(name "DQ5")
					(number "M8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "M9")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "N1")
				)
				(pin bidirectional line
					(at 29.21 -30.48 180)
					(length 2.54)
					(name "DQ12")
					(number "N2")
				)
				(pin bidirectional line
					(at 29.21 -35.56 180)
					(length 2.54)
					(name "DQ14")
					(number "N3")
				)
				(pin bidirectional line
					(at 29.21 -2.54 180)
					(length 2.54)
					(name "DQ1")
					(number "N7")
				)
				(pin bidirectional line
					(at 29.21 -7.62 180)
					(length 2.54)
					(name "DQ3")
					(number "N8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "N9")
				)
				(pin bidirectional line
					(at 29.21 -27.94 180)
					(length 2.54)
					(name "DQ11")
					(number "P1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "P2")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "P3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(hide yes)
					(name "VDDQ")
					(number "P7")
				)
				(pin passive line
					(at 0 -90.17 0)
					(length 2.54)
					(hide yes)
					(name "VSSQ")
					(number "P8")
				)
				(pin bidirectional line
					(at 29.21 -10.16 180)
					(length 2.54)
					(name "DQ4")
					(number "P9")
				)
				(pin bidirectional line
					(at 29.21 -33.02 180)
					(length 2.54)
					(name "DQ13")
					(number "R1")
				)
				(pin bidirectional line
					(at 29.21 -38.1 180)
					(length 2.54)
					(name "DQ15")
					(number "R2")
				)
				(pin passive line
					(at 0 -87.63 0)
					(length 2.54)
					(hide yes)
					(name "VSS")
					(number "R3")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "VDD")
					(number "R7")
				)
				(pin bidirectional line
					(at 29.21 0 180)
					(length 2.54)
					(name "DQ0")
					(number "R8")
				)
				(pin bidirectional line
					(at 29.21 -5.08 180)
					(length 2.54)
					(name "DQ2")
					(number "R9")
				)
			)
			(embedded_fonts no)
		)
)
