(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IS61WV5128BLL-10BLI"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -1.27 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IS61WV5128BLL-10BLI"
				(at 50.8 -5.588 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IS61WV5128BLL-10BLI"
				(at 50.8 -17.018 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.issi.com/WW/pdf/61-64WV5128Axx-Bxx.pdf"
				(at 50.8 -19.304 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "512K x 8 HIGH-SPEED ASYNCHRONOUS CMOS STATIC RAM"
				(at 50.8 -21.844 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "ISSI"
				(at 50.8 -14.986 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IS61WV5128BLL-10BLI"
				(at 50.8 -3.302 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -12.446 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -10.414 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IS61WV5128BLL-10BLI_1_1"
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "A0")
					(number "A1")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "A1")
					(number "A2")
				)
				(pin no_connect line
					(at 25.4 -29.21 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A3")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "A3")
					(number "A4")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "A6")
					(number "A5")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "A8")
					(number "A6")
				)
				(pin bidirectional line
					(at 30.48 -15.24 180)
					(length 5.08)
					(name "I/O4")
					(number "B1")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "A2")
					(number "B2")
				)
				(pin input line
					(at 30.48 -40.64 180)
					(length 5.08)
					(name "~{WE}")
					(number "B3")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "A4")
					(number "B4")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "A7")
					(number "B5")
				)
				(pin bidirectional line
					(at 30.48 -5.08 180)
					(length 5.08)
					(name "I/O0")
					(number "B6")
				)
				(pin bidirectional line
					(at 30.48 -17.78 180)
					(length 5.08)
					(name "I/O5")
					(number "C1")
				)
				(pin no_connect line
					(at 25.4 -31.75 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "C3")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "A5")
					(number "C4")
				)
				(pin bidirectional line
					(at 30.48 -7.62 180)
					(length 5.08)
					(name "I/O1")
					(number "C6")
				)
				(pin passive line
					(at 30.48 -45.72 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "D1")
				)
				(pin power_in line
					(at 30.48 0 180)
					(length 5.08)
					(name "VDD")
					(number "D6")
				)
				(pin passive line
					(at 30.48 0 180)
					(length 5.08)
					(hide yes)
					(name "VDD")
					(number "E1")
				)
				(pin power_in line
					(at 30.48 -45.72 180)
					(length 5.08)
					(name "GND")
					(number "E6")
				)
				(pin bidirectional line
					(at 30.48 -20.32 180)
					(length 5.08)
					(name "I/O6")
					(number "F1")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 5.08)
					(name "A18")
					(number "F3")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 5.08)
					(name "A17")
					(number "F4")
				)
				(pin bidirectional line
					(at 30.48 -10.16 180)
					(length 5.08)
					(name "I/O2")
					(number "F6")
				)
				(pin bidirectional line
					(at 30.48 -22.86 180)
					(length 5.08)
					(name "I/O7")
					(number "G1")
				)
				(pin input line
					(at 30.48 -38.1 180)
					(length 5.08)
					(name "~{OE}")
					(number "G2")
				)
				(pin input line
					(at 30.48 -43.18 180)
					(length 5.08)
					(name "~{CE}")
					(number "G3")
				)
				(pin input line
					(at 0 -40.64 0)
					(length 5.08)
					(name "A16")
					(number "G4")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 5.08)
					(name "A15")
					(number "G5")
				)
				(pin bidirectional line
					(at 30.48 -12.7 180)
					(length 5.08)
					(name "I/O3")
					(number "G6")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "A9")
					(number "H1")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "A10")
					(number "H2")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "A11")
					(number "H3")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "A12")
					(number "H4")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "A13")
					(number "H5")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "A14")
					(number "H6")
				)
			)
			(embedded_fonts no)
		)
)
