(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "IS66WVS4M8BLL-104NLI"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "IS66WVS4M8BLL-104NLI"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "IS66WVS4M8BLL-104NLI"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.issi.com/WW/pdf/66-67WVS4M8ALL-BLL.pdf"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "SPI, SRAM 32Mb, SerialRAM, 2.7V-3.6V, 104MHz, 8 pin SOIC 150 mil"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "ISSI"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "IS66WVS4M8BLL-104NLI"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, MEMORY, IC, DRAM, HYPERBUS, HYPERRAM, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "IS66WVS4M8BLL-104NLI_1_1"
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "~{CS}")
					(number "1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "SO/SIO1")
					(number "2")
					(alternate "SIO1" passive line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 2.54)
					(name "SIO2")
					(number "3")
				)
				(pin power_in line
					(at 20.32 -12.7 180)
					(length 2.54)
					(name "VSS")
					(number "4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 2.54)
					(name "SI/SIO0")
					(number "5")
					(alternate "SIO0" passive line)
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "CLK")
					(number "6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 2.54)
					(name "SIO3")
					(number "7")
				)
				(pin power_in line
					(at 20.32 0 180)
					(length 2.54)
					(name "VDD")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
