(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ISL83485IBZ-T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 35.56 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ISL83485IBZ-T"
				(at 35.56 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ISL83485IBZ-T"
				(at 35.56 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.renesas.com/en/document/dst/isl83483-isl83485-isl83488-isl83490-isl83491-datasheet?r=532056"
				(at 35.56 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Transceiver, RS422 & RS485, 3 V to 3.6 V, SOIC-8, -40 °C to 85 °C"
				(at 35.56 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Renesas"
				(at 35.56 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "ISL83485IBZ-T"
				(at 35.56 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 35.56 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 35.56 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, INTERFACE, IC, DRIVER, TRANSCEIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ISL83485IBZ-T_1_1"
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(name "RO")
					(number "1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 2.54)
					(name "~{RE}")
					(number "2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 2.54)
					(name "DE")
					(number "3")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 2.54)
					(name "DI")
					(number "4")
				)
				(pin passive line
					(at 20.32 -7.62 180)
					(length 2.54)
					(name "GND")
					(number "5")
				)
				(pin passive line
					(at 20.32 -5.08 180)
					(length 2.54)
					(name "A")
					(number "6")
					(alternate "Y" passive line)
				)
				(pin passive line
					(at 20.32 -2.54 180)
					(length 2.54)
					(name "B")
					(number "7")
					(alternate "Z" passive line)
				)
				(pin passive line
					(at 20.32 0 180)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
			)
			(embedded_fonts no)
		)
)
