(footprint "JHL6340SLLSQ"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "JHL6340SLLSQ"
		(at 0 6.4 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at 0 7.8 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at 0 10.45 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at 0.05 9 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -5.06 -5.06)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd oval
		(at -4.6 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd oval
		(at -4.14 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd oval
		(at -3.68 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd oval
		(at -3.22 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A6" smd oval
		(at -2.76 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A7" smd oval
		(at -2.3 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd oval
		(at -1.84 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd oval
		(at -1.38 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd oval
		(at -0.92 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd oval
		(at -0.46 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd oval
		(at 0 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A13" smd oval
		(at 0.46 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A14" smd oval
		(at 0.92 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A15" smd oval
		(at 1.38 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A16" smd oval
		(at 1.84 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A17" smd oval
		(at 2.3 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A18" smd oval
		(at 2.76 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A19" smd oval
		(at 3.22 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A20" smd oval
		(at 3.68 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A21" smd oval
		(at 4.14 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A22" smd oval
		(at 4.6 -5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A23" smd circle
		(at 5.06 -5.06)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA1" smd oval
		(at -5.06 4.14 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA2" smd circle
		(at -4.6 4.14)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA22" smd circle
		(at 4.6 4.14)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA23" smd oval
		(at 5.06 4.14 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB1" smd oval
		(at -5.06 4.6 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB2" smd circle
		(at -4.6 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB3" smd circle
		(at -4.14 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB4" smd circle
		(at -3.68 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB5" smd circle
		(at -3.22 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB6" smd circle
		(at -2.76 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB7" smd circle
		(at -2.3 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB8" smd circle
		(at -1.84 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB9" smd circle
		(at -1.38 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB10" smd circle
		(at -0.92 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB11" smd circle
		(at -0.46 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB12" smd circle
		(at 0 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB13" smd circle
		(at 0.46 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB14" smd circle
		(at 0.92 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB15" smd circle
		(at 1.38 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB16" smd circle
		(at 1.84 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB17" smd circle
		(at 2.3 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB18" smd circle
		(at 2.76 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB19" smd circle
		(at 3.22 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB20" smd circle
		(at 3.68 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB21" smd circle
		(at 4.14 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB22" smd circle
		(at 4.6 4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB23" smd oval
		(at 5.06 4.6 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC1" smd circle
		(at -5.06 5.06)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC2" smd oval
		(at -4.6 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC3" smd oval
		(at -4.14 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC4" smd oval
		(at -3.68 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC5" smd oval
		(at -3.22 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC6" smd oval
		(at -2.76 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC7" smd oval
		(at -2.3 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC8" smd oval
		(at -1.84 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC9" smd oval
		(at -1.38 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC10" smd oval
		(at -0.92 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC11" smd oval
		(at -0.46 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC12" smd oval
		(at 0 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC13" smd oval
		(at 0.46 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC14" smd oval
		(at 0.92 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC15" smd oval
		(at 1.38 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC16" smd oval
		(at 1.84 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC17" smd oval
		(at 2.3 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC18" smd oval
		(at 2.76 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC19" smd oval
		(at 3.22 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC20" smd oval
		(at 3.68 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC21" smd oval
		(at 4.14 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC22" smd oval
		(at 4.6 5.06)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AC23" smd circle
		(at 5.06 5.06)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd oval
		(at -5.06 -4.6 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -4.6 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -4.14 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -3.68 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -3.22 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B6" smd circle
		(at -2.76 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B7" smd circle
		(at -2.3 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at -1.84 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at -1.38 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at -0.92 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at -0.46 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at 0 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B13" smd circle
		(at 0.46 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B14" smd circle
		(at 0.92 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B15" smd circle
		(at 1.38 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B16" smd circle
		(at 1.84 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B17" smd circle
		(at 2.3 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B18" smd circle
		(at 2.76 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B19" smd circle
		(at 3.22 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B20" smd circle
		(at 3.68 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B21" smd circle
		(at 4.14 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B22" smd circle
		(at 4.6 -4.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B23" smd oval
		(at 5.06 -4.6 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd oval
		(at -5.06 -4.14 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -4.6 -4.14)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C22" smd circle
		(at 4.6 -4.14)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C23" smd oval
		(at 5.06 -4.14 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd oval
		(at -5.06 -3.68 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -4.6 -3.68)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -3.9 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -3.25 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D6" smd circle
		(at -2.6 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at -1.95 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at -1.3 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at -0.65 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at 0 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D13" smd circle
		(at 0.65 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D15" smd circle
		(at 1.3 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D16" smd circle
		(at 1.95 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D18" smd circle
		(at 2.6 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D19" smd circle
		(at 3.25 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D20" smd circle
		(at 3.9 -3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D22" smd circle
		(at 4.6 -3.68)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D23" smd oval
		(at 5.06 -3.68 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd oval
		(at -5.06 -3.22 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -4.6 -3.22)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -3.9 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -3.25 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E6" smd circle
		(at -2.6 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at -1.95 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at -1.3 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at -0.65 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E12" smd circle
		(at 0 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E13" smd circle
		(at 0.65 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E15" smd circle
		(at 1.3 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E16" smd circle
		(at 1.95 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E18" smd circle
		(at 2.6 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E19" smd circle
		(at 3.25 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E20" smd circle
		(at 3.9 -3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E22" smd circle
		(at 4.6 -3.22)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E23" smd oval
		(at 5.06 -3.22 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd oval
		(at -5.06 -2.76 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -4.6 -2.76)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -3.9 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -3.25 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F6" smd circle
		(at -2.6 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at -1.95 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at -1.3 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at -0.65 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F12" smd circle
		(at 0 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F13" smd circle
		(at 0.65 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F15" smd circle
		(at 1.3 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F16" smd circle
		(at 1.95 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F18" smd circle
		(at 2.6 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F19" smd circle
		(at 3.25 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F20" smd circle
		(at 3.9 -2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F22" smd circle
		(at 4.6 -2.76)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F23" smd oval
		(at 5.06 -2.76 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd oval
		(at -5.06 -2.3 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -4.6 -2.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G22" smd circle
		(at 4.6 -2.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G23" smd oval
		(at 5.06 -2.3 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd oval
		(at -5.06 -1.84 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -4.6 -1.84)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -3.9 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -3.25 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H6" smd circle
		(at -2.6 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at -1.95 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at -1.3 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at -0.65 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at 0 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H13" smd circle
		(at 0.65 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H15" smd circle
		(at 1.3 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H16" smd circle
		(at 1.95 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H18" smd circle
		(at 2.6 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H19" smd circle
		(at 3.25 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H20" smd circle
		(at 3.9 -1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H22" smd circle
		(at 4.6 -1.84)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H23" smd oval
		(at 5.06 -1.84 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd oval
		(at -5.06 -1.38 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -4.6 -1.38)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -3.9 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -3.25 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J6" smd circle
		(at -2.6 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at -1.95 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at -1.3 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at -0.65 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at 0 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J13" smd circle
		(at 0.65 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J15" smd circle
		(at 1.3 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J16" smd circle
		(at 1.95 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J18" smd circle
		(at 2.6 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J19" smd circle
		(at 3.25 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J20" smd circle
		(at 3.9 -1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J22" smd circle
		(at 4.6 -1.38)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J23" smd oval
		(at 5.06 -1.38 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd oval
		(at -5.06 -0.92 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -4.6 -0.92)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K22" smd circle
		(at 4.6 -0.92)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K23" smd oval
		(at 5.06 -0.92 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L1" smd oval
		(at -5.06 -0.46 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L2" smd circle
		(at -4.6 -0.46)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L4" smd circle
		(at -3.9 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L5" smd circle
		(at -3.25 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L6" smd circle
		(at -2.6 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L8" smd circle
		(at -1.95 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L9" smd circle
		(at -1.3 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L11" smd circle
		(at -0.65 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L12" smd circle
		(at 0 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L13" smd circle
		(at 0.65 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L15" smd circle
		(at 1.3 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L16" smd circle
		(at 1.95 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L18" smd circle
		(at 2.6 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L19" smd circle
		(at 3.25 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L20" smd circle
		(at 3.9 -0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L22" smd circle
		(at 4.6 -0.46)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "L23" smd oval
		(at 5.06 -0.46 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M1" smd oval
		(at -5.06 0 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M2" smd circle
		(at -4.6 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M4" smd circle
		(at -3.9 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M5" smd circle
		(at -3.25 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M6" smd circle
		(at -2.6 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M8" smd circle
		(at -1.95 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M9" smd circle
		(at -1.3 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M11" smd circle
		(at -0.65 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M12" smd circle
		(at 0 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M13" smd circle
		(at 0.65 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M15" smd circle
		(at 1.3 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M16" smd circle
		(at 1.95 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M18" smd circle
		(at 2.6 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M19" smd circle
		(at 3.25 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M20" smd circle
		(at 3.9 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M22" smd circle
		(at 4.6 0)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "M23" smd oval
		(at 5.06 0 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd oval
		(at -5.06 0.46 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -4.6 0.46)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -3.9 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N5" smd circle
		(at -3.25 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N6" smd circle
		(at -2.6 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at -1.95 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at -1.3 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N11" smd circle
		(at -0.65 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N12" smd circle
		(at 0 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N13" smd circle
		(at 0.65 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N15" smd circle
		(at 1.3 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N16" smd circle
		(at 1.95 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N18" smd circle
		(at 2.6 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N19" smd circle
		(at 3.25 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N20" smd circle
		(at 3.9 0.65)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N22" smd circle
		(at 4.6 0.46)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N23" smd oval
		(at 5.06 0.46 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd oval
		(at -5.06 0.92 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -4.6 0.92)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P22" smd circle
		(at 4.6 0.92)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P23" smd oval
		(at 5.06 0.92 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd oval
		(at -5.06 1.38 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -4.6 1.38)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R4" smd circle
		(at -3.9 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R5" smd circle
		(at -3.25 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R6" smd circle
		(at -2.6 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R8" smd circle
		(at -1.95 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R9" smd circle
		(at -1.3 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R11" smd circle
		(at -0.65 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R12" smd circle
		(at 0 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R13" smd circle
		(at 0.65 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R15" smd circle
		(at 1.3 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R16" smd circle
		(at 1.95 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R18" smd circle
		(at 2.6 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R19" smd circle
		(at 3.25 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R20" smd circle
		(at 3.9 1.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R22" smd circle
		(at 4.6 1.38)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R23" smd oval
		(at 5.06 1.38 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd oval
		(at -5.06 1.84 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -4.6 1.84)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T4" smd circle
		(at -3.9 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T5" smd circle
		(at -3.25 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T6" smd circle
		(at -2.6 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T8" smd circle
		(at -1.95 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T9" smd circle
		(at -1.3 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T11" smd circle
		(at -0.65 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T12" smd circle
		(at 0 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T13" smd circle
		(at 0.65 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T15" smd circle
		(at 1.3 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T16" smd circle
		(at 1.95 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T18" smd circle
		(at 2.6 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T19" smd circle
		(at 3.25 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T20" smd circle
		(at 3.9 1.95)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T22" smd circle
		(at 4.6 1.84)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T23" smd oval
		(at 5.06 1.84 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd oval
		(at -5.06 2.3 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -4.6 2.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U22" smd circle
		(at 4.6 2.3)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U23" smd oval
		(at 5.06 2.3 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V1" smd oval
		(at -5.06 2.76 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V2" smd circle
		(at -4.6 2.76)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V4" smd circle
		(at -3.9 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V5" smd circle
		(at -3.25 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V6" smd circle
		(at -2.6 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V8" smd circle
		(at -1.95 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V9" smd circle
		(at -1.3 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V11" smd circle
		(at -0.65 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V12" smd circle
		(at 0 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V13" smd circle
		(at 0.65 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V15" smd circle
		(at 1.3 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V16" smd circle
		(at 1.95 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V18" smd circle
		(at 2.6 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V19" smd circle
		(at 3.25 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V20" smd circle
		(at 3.9 2.6)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V22" smd circle
		(at 4.6 2.76)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V23" smd oval
		(at 5.06 2.76 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd oval
		(at -5.06 3.22 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W2" smd circle
		(at -4.6 3.22)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W4" smd circle
		(at -3.9 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W5" smd circle
		(at -3.25 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W6" smd circle
		(at -2.6 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W8" smd circle
		(at -1.95 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W9" smd circle
		(at -1.3 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W11" smd circle
		(at -0.65 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W12" smd circle
		(at 0 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W13" smd circle
		(at 0.65 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W15" smd circle
		(at 1.3 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W16" smd circle
		(at 1.95 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W18" smd circle
		(at 2.6 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W19" smd circle
		(at 3.25 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W20" smd circle
		(at 3.9 3.25)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W22" smd circle
		(at 4.6 3.22)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W23" smd oval
		(at 5.06 3.22 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y1" smd oval
		(at -5.06 3.68 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -4.6 3.68)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y4" smd circle
		(at -3.9 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y5" smd circle
		(at -3.25 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y6" smd circle
		(at -2.6 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y8" smd circle
		(at -1.95 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y9" smd circle
		(at -1.3 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y11" smd circle
		(at -0.65 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y12" smd circle
		(at 0 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y13" smd circle
		(at 0.65 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y15" smd circle
		(at 1.3 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y16" smd circle
		(at 1.95 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y18" smd circle
		(at 2.6 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y19" smd circle
		(at 3.25 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y20" smd circle
		(at 3.9 3.9)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y22" smd circle
		(at 4.6 3.68)
		(size 0.254 0.254)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y23" smd oval
		(at 5.06 3.68 90)
		(size 0.1578 0.3302)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_jhl6340sllsq.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
