(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "JHL6340SLLSQ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 71.12 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "JHL6340SLLSQ"
				(at 71.12 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "JHL6340SLLSQ"
				(at 71.12 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.thunderbolttechnology.net/sites/default/files/18-241_ThunderboltController_Brief_HI.pdf"
				(at 71.12 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Thunderbolt™ 3 Controller, I/O"
				(at 71.12 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Intel"
				(at 71.12 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "JHL6340SLLSQ"
				(at 71.12 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 71.12 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 71.12 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "JHL6340SLLSQ_1_0")
			(symbol "JHL6340SLLSQ_1_1"
				(pin power_in line
					(at 54.61 -55.88 180)
					(length 5.08)
					(name "SVR_VSS")
					(number "A1")
				)
				(pin power_in line
					(at 54.61 0 180)
					(length 5.08)
					(name "VCC3P3_SVR")
					(number "A2")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3_SVR")
					(number "A3")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A6")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "VSS_ANA")
					(number "A10")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A12")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A14")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AA22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AA23")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(name "VSS")
					(number "AB1")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB6")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB10")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB12")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB14")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB22")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AC2")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC6")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC10")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC12")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC14")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC22")
				)
				(pin passive line
					(at 54.61 -55.88 180)
					(length 5.08)
					(hide yes)
					(name "SVR_VSS")
					(number "B1")
				)
				(pin passive line
					(at 54.61 -55.88 180)
					(length 5.08)
					(hide yes)
					(name "SVR_VSS")
					(number "B2")
				)
				(pin passive line
					(at 54.61 0 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3_SVR")
					(number "B3")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B6")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B10")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B12")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B14")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B22")
				)
				(pin power_out line
					(at 54.61 -53.34 180)
					(length 5.08)
					(name "SVR_IND")
					(number "C1")
				)
				(pin passive line
					(at 54.61 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "SVR_IND")
					(number "C2")
				)
				(pin passive line
					(at 54.61 -53.34 180)
					(length 5.08)
					(hide yes)
					(name "SVR_IND")
					(number "D1")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D9")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D11")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D12")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D13")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D15")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D18")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E6")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E9")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E11")
				)
				(pin power_in line
					(at 54.61 -38.1 180)
					(length 5.08)
					(name "VCC0P9_SVR_ANA")
					(number "E12")
				)
				(pin passive line
					(at 54.61 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_ANA")
					(number "E13")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E15")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E23")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F5")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "F6")
				)
				(pin power_in line
					(at 54.61 -2.54 180)
					(length 5.08)
					(name "VCC3P3_SX")
					(number "F8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F9")
				)
				(pin passive line
					(at 54.61 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_ANA")
					(number "F11")
				)
				(pin passive line
					(at 54.61 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_ANA")
					(number "F12")
				)
				(pin passive line
					(at 54.61 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_ANA")
					(number "F13")
				)
				(pin passive line
					(at 54.61 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_ANA")
					(number "F15")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F16")
				)
				(pin power_in line
					(at 54.61 -71.12 180)
					(length 5.08)
					(name "VCC0P9_LVR")
					(number "F18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "G22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "G23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H1")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H2")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H5")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "H8")
				)
				(pin power_in line
					(at 54.61 -5.08 180)
					(length 5.08)
					(name "VCC3P3A")
					(number "H9")
				)
				(pin power_in line
					(at 54.61 -73.66 180)
					(length 5.08)
					(name "VCC0P9_LVR_SENSE")
					(number "H11")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H12")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H13")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H15")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H16")
				)
				(pin passive line
					(at 54.61 -71.12 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_LVR")
					(number "H18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J5")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J8")
				)
				(pin power_in line
					(at 54.61 -40.64 180)
					(length 5.08)
					(name "VCC0P9_SVR_SENSE")
					(number "J9")
				)
				(pin passive line
					(at 54.61 -71.12 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_LVR")
					(number "J11")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J12")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J13")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J15")
				)
				(pin power_in line
					(at 0 -73.66 0)
					(length 5.08)
					(name "VCC3P3_ANA_USB2")
					(number "J16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J19")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "K1")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "K2")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L5")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCC0P9_ANA_DPSRC")
					(number "L6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_DP")
					(number "L8")
				)
				(pin power_in line
					(at 54.61 -35.56 180)
					(length 5.08)
					(name "VCC0P9_SVR")
					(number "L9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCC0P9_DP")
					(number "L11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_DP")
					(number "L12")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L13")
				)
				(pin power_in line
					(at 0 -71.12 0)
					(length 5.08)
					(name "VCC3P3_ANA_PCIE")
					(number "L16")
				)
				(pin power_in line
					(at 0 -22.86 0)
					(length 5.08)
					(name "VCC0P9_ANA_PCIE_2")
					(number "L18")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VCC0P9_ANA_PCIE_1")
					(number "L19")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "M1")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "M2")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "M5")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_ANA_DPSRC")
					(number "M6")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_DP")
					(number "M8")
				)
				(pin passive line
					(at 54.61 -35.56 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "M9")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M11")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M12")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 5.08)
					(name "VCC0P9_PCIE")
					(number "M13")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_PCIE")
					(number "M15")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_PCIE")
					(number "M16")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_ANA_PCIE_2")
					(number "M18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "M19")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "M20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "N5")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N9")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N11")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N12")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N13")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_ANA_PCIE_2")
					(number "N18")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_ANA_PCIE_1")
					(number "N19")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "N20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "N22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "N23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "P1")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "P2")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "R5")
				)
				(pin power_in line
					(at 54.61 -20.32 180)
					(length 5.08)
					(name "VCC3P3_LC")
					(number "R6")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_CIO")
					(number "R8")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_CIO")
					(number "R9")
				)
				(pin power_in line
					(at 0 -53.34 0)
					(length 5.08)
					(name "VCC0P9_CIO")
					(number "R11")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_CIO")
					(number "R12")
				)
				(pin power_in line
					(at 54.61 -17.78 180)
					(length 5.08)
					(name "VCC3P3_S0")
					(number "R13")
				)
				(pin power_in line
					(at 0 -35.56 0)
					(length 5.08)
					(name "VCC0P9_USB")
					(number "R15")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_USB")
					(number "R16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "R18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "R19")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "R20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "R22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "R23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T1")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T2")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T5")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T6")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T8")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_DP")
					(number "T11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_DP")
					(number "T12")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T13")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T15")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T16")
				)
				(pin passive line
					(at 54.61 -81.28 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T18")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "U22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "U23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V5")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V6")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VCC0P9_ANA_DPSNK")
					(number "V11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_ANA_DPSNK")
					(number "V12")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_ANA_DPSNK")
					(number "V13")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V15")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W5")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W6")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W8")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W9")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W20")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W22")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W23")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y9")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y13")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y20")
				)
			)
			(symbol "JHL6340SLLSQ_2_0"
				(text "PCIe Gen3"
					(at 24.13 -17.78 0)
				)
			)
			(symbol "JHL6340SLLSQ_2_1"
				(pin output line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PCIE_CLKREQ_N")
					(number "AC5")
				)
				(pin input line
					(at 55.88 -25.4 180)
					(length 5.08)
					(name "PCIE_TX3_N")
					(number "F22")
				)
				(pin input line
					(at 55.88 -22.86 180)
					(length 5.08)
					(name "PCIE_TX3_P")
					(number "F23")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PCIE_RX3_N")
					(number "H22")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PCIE_RX3_P")
					(number "H23")
				)
				(pin input line
					(at 55.88 -17.78 180)
					(length 5.08)
					(name "PCIE_TX2_N")
					(number "K22")
				)
				(pin input line
					(at 55.88 -15.24 180)
					(length 5.08)
					(name "PCIE_TX2_P")
					(number "K23")
				)
				(pin input line
					(at 55.88 -33.02 180)
					(length 5.08)
					(name "PERST_N")
					(number "L4")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PCIE_RX2_N")
					(number "M22")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PCIE_RX2_P")
					(number "M23")
				)
				(pin input line
					(at 55.88 -38.1 180)
					(length 5.08)
					(name "PCIE_RBIAS")
					(number "N16")
				)
				(pin input line
					(at 55.88 -10.16 180)
					(length 5.08)
					(name "PCIE_TX1_N")
					(number "P22")
				)
				(pin input line
					(at 55.88 -7.62 180)
					(length 5.08)
					(name "PCIE_TX1_P")
					(number "P23")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PCIE_REFCLK_100_IN_N")
					(number "T19")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PCIE_RX1_N")
					(number "T22")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PCIE_RX1_P")
					(number "T23")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PCIE_REFCLK_100_IN_P")
					(number "V19")
				)
				(pin input line
					(at 55.88 -2.54 180)
					(length 5.08)
					(name "PCIE_TX0_N")
					(number "V22")
				)
				(pin input line
					(at 55.88 0 180)
					(length 5.08)
					(name "PCIE_TX0_P")
					(number "V23")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PCIE_RX0_N")
					(number "Y22")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "PCIE_RX0_P")
					(number "Y23")
				)
			)
			(symbol "JHL6340SLLSQ_3_0"
				(text "SINK PORT 0"
					(at 26.67 -27.94 900)
				)
				(text "SINK PORT 1"
					(at 26.67 -80.01 900)
				)
				(text "SOURCE PORT 0"
					(at 30.48 -29.21 900)
				)
				(text "GPIO"
					(at 30.48 -60.96 900)
				)
				(text "POC_GPIO"
					(at 30.48 -90.17 900)
				)
			)
			(symbol "JHL6340SLLSQ_3_1"
				(pin bidirectional line
					(at 55.88 -71.12 180)
					(length 5.08)
					(name "GPIO_8")
					(number "AA1")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DPSNK0_HPD")
					(number "AA2")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "DPSNK0_ML0_P")
					(number "AB7")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "DPSNK0_ML1_P")
					(number "AB9")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "DPSNK0_ML2_P")
					(number "AB11")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "DPSNK0_ML3_P")
					(number "AB13")
				)
				(pin input line
					(at 0 -53.34 0)
					(length 5.08)
					(name "DPSNK1_ML0_P")
					(number "AB15")
				)
				(pin input line
					(at 0 -60.96 0)
					(length 5.08)
					(name "DPSNK1_ML1_P")
					(number "AB17")
				)
				(pin input line
					(at 0 -68.58 0)
					(length 5.08)
					(name "DPSNK1_ML2_P")
					(number "AB19")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 5.08)
					(name "DPSNK1_ML3_P")
					(number "AB21")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "DPSNK0_ML0_N")
					(number "AC7")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "DPSNK0_ML1_N")
					(number "AC9")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "DPSNK0_ML2_N")
					(number "AC11")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "DPSNK0_ML3_N")
					(number "AC13")
				)
				(pin input line
					(at 0 -55.88 0)
					(length 5.08)
					(name "DPSNK1_ML0_N")
					(number "AC15")
				)
				(pin input line
					(at 0 -63.5 0)
					(length 5.08)
					(name "DPSNK1_ML1_N")
					(number "AC17")
				)
				(pin input line
					(at 0 -71.12 0)
					(length 5.08)
					(name "DPSNK1_ML2_N")
					(number "AC19")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 5.08)
					(name "DPSNK1_ML3_N")
					(number "AC21")
				)
				(pin bidirectional line
					(at 55.88 -91.44 180)
					(length 5.08)
					(name "POC_GPIO_5")
					(number "D2")
				)
				(pin bidirectional line
					(at 55.88 -83.82 180)
					(length 5.08)
					(name "POC_GPIO_2")
					(number "D4")
				)
				(pin bidirectional line
					(at 55.88 -81.28 180)
					(length 5.08)
					(name "POC_GPIO_1")
					(number "E2")
				)
				(pin bidirectional line
					(at 55.88 -93.98 180)
					(length 5.08)
					(name "POC_GPIO_6")
					(number "F1")
				)
				(pin bidirectional line
					(at 55.88 -88.9 180)
					(length 5.08)
					(name "POC_GPIO_4")
					(number "F2")
				)
				(pin passive line
					(at 55.88 -38.1 180)
					(length 5.08)
					(name "DPSRC_HPD")
					(number "G1")
				)
				(pin bidirectional line
					(at 55.88 -86.36 180)
					(length 5.08)
					(name "POC_GPIO_3")
					(number "H4")
				)
				(pin output line
					(at 55.88 -25.4 180)
					(length 5.08)
					(name "DPSRC_ML3_N")
					(number "J1")
				)
				(pin output line
					(at 55.88 -22.86 180)
					(length 5.08)
					(name "DPSRC_ML3_P")
					(number "J2")
				)
				(pin bidirectional line
					(at 55.88 -78.74 180)
					(length 5.08)
					(name "POC_GPIO_0")
					(number "J4")
				)
				(pin output line
					(at 55.88 -17.78 180)
					(length 5.08)
					(name "DPSRC_ML2_N")
					(number "L1")
				)
				(pin output line
					(at 55.88 -15.24 180)
					(length 5.08)
					(name "DPSRC_ML2_P")
					(number "L2")
				)
				(pin output line
					(at 55.88 -10.16 180)
					(length 5.08)
					(name "DPSRC_ML1_N")
					(number "N1")
				)
				(pin output line
					(at 55.88 -7.62 180)
					(length 5.08)
					(name "DPSRC_ML1_P")
					(number "N2")
				)
				(pin passive line
					(at 0 -99.06 0)
					(length 5.08)
					(name "DPSNK1_DDC_DATA")
					(number "N4")
				)
				(pin passive line
					(at 55.88 -43.18 180)
					(length 5.08)
					(name "DPSRC_RBIAS")
					(number "N6")
				)
				(pin output line
					(at 55.88 -2.54 180)
					(length 5.08)
					(name "DPSRC_ML0_N")
					(number "R1")
				)
				(pin output line
					(at 55.88 0 180)
					(length 5.08)
					(name "DPSRC_ML0_P")
					(number "R2")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "DPSNK0_DDC_DATA")
					(number "R4")
				)
				(pin bidirectional line
					(at 55.88 -50.8 180)
					(length 5.08)
					(name "GPIO_0")
					(number "U1")
				)
				(pin bidirectional line
					(at 55.88 -53.34 180)
					(length 5.08)
					(name "GPIO_1")
					(number "U2")
				)
				(pin bidirectional line
					(at 55.88 -55.88 180)
					(length 5.08)
					(name "GPIO_2")
					(number "V1")
				)
				(pin bidirectional line
					(at 55.88 -58.42 180)
					(length 5.08)
					(name "GPIO_3")
					(number "V2")
				)
				(pin bidirectional line
					(at 55.88 -60.96 180)
					(length 5.08)
					(name "GPIO_4")
					(number "W1")
				)
				(pin bidirectional line
					(at 55.88 -63.5 180)
					(length 5.08)
					(name "GPIO_5")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "DPSNK0_AUX_N")
					(number "W11")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "DPSNK1_AUX_N")
					(number "W12")
				)
				(pin bidirectional line
					(at 55.88 -30.48 180)
					(length 5.08)
					(name "DPSRC_AUX_P")
					(number "W19")
				)
				(pin bidirectional line
					(at 55.88 -66.04 180)
					(length 5.08)
					(name "GPIO_6")
					(number "Y1")
				)
				(pin bidirectional line
					(at 55.88 -68.58 180)
					(length 5.08)
					(name "GPIO_7")
					(number "Y2")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "DPSNK0_DDC_CLK")
					(number "Y5")
				)
				(pin passive line
					(at 0 -91.44 0)
					(length 5.08)
					(name "DPSNK1_HPD")
					(number "Y6")
				)
				(pin passive line
					(at 0 -96.52 0)
					(length 5.08)
					(name "DPSNK1_DDC_CLK")
					(number "Y8")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "DPSNK0_AUXP")
					(number "Y11")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "DPSNK1_AUXP")
					(number "Y12")
				)
				(pin passive line
					(at 0 -104.14 0)
					(length 5.08)
					(name "DPSNK_RBIAS")
					(number "Y18")
				)
				(pin bidirectional line
					(at 55.88 -33.02 180)
					(length 5.08)
					(name "DPSRC_AUX_N")
					(number "Y19")
				)
			)
			(symbol "JHL6340SLLSQ_4_0"
				(text "MISCELLANEOUS"
					(at 20.32 -13.97 0)
				)
			)
			(symbol "JHL6340SLLSQ_4_1"
				(pin output line
					(at 55.88 -17.78 180)
					(length 5.08)
					(name "EE_DI")
					(number "AB3")
				)
				(pin output line
					(at 55.88 -25.4 180)
					(length 5.08)
					(name "EE_CLK")
					(number "AB4")
				)
				(pin input line
					(at 55.88 -2.54 180)
					(length 5.08)
					(name "TEST_PWR_GOOD")
					(number "AB5")
				)
				(pin output line
					(at 55.88 -22.86 180)
					(length 5.08)
					(name "EE_CS_N")
					(number "AC3")
				)
				(pin input line
					(at 55.88 -20.32 180)
					(length 5.08)
					(name "EE_D0")
					(number "AC4")
				)
				(pin input line
					(at 55.88 -10.16 180)
					(length 5.08)
					(name "XTAL_25_IN")
					(number "D22")
				)
				(pin input line
					(at 55.88 -12.7 180)
					(length 5.08)
					(name "XTAL_25_OUT")
					(number "D23")
				)
				(pin input line
					(at 55.88 0 180)
					(length 5.08)
					(name "TEST_EN")
					(number "E1")
				)
				(pin input line
					(at 55.88 -5.08 180)
					(length 5.08)
					(name "RESET_N")
					(number "F4")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "RBIAS")
					(number "H6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "RSENSE")
					(number "J6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 5.08)
					(name "TCK")
					(number "T4")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "TMS")
					(number "V4")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 5.08)
					(name "TDO")
					(number "W4")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "TDI")
					(number "Y4")
				)
			)
			(symbol "JHL6340SLLSQ_5_0"
				(text "TBT PORT A"
					(at 26.67 -31.75 900)
				)
				(text "TBT PORT B"
					(at 31.115 -31.75 900)
				)
			)
			(symbol "JHL6340SLLSQ_5_1"
				(pin input line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PA_LSRX")
					(number "A4")
				)
				(pin output line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PA_LSTX")
					(number "A5")
				)
				(pin input line
					(at 55.88 -10.16 180)
					(length 5.08)
					(name "PB_RX1_N")
					(number "A7")
				)
				(pin output line
					(at 55.88 -22.86 180)
					(length 5.08)
					(name "PB_TX1_P")
					(number "A9")
				)
				(pin output line
					(at 55.88 -15.24 180)
					(length 5.08)
					(name "PB_TX0_P")
					(number "A11")
				)
				(pin input line
					(at 55.88 0 180)
					(length 5.08)
					(name "PB_RX0_P")
					(number "A13")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PA_RX1_P")
					(number "A15")
				)
				(pin output line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PA_TX1_P")
					(number "A17")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PA_TX0_P")
					(number "A19")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PA_RX0_N")
					(number "A21")
				)
				(pin output line
					(at 55.88 -45.72 180)
					(length 5.08)
					(name "PB_LSTX")
					(number "B4")
				)
				(pin input line
					(at 55.88 -48.26 180)
					(length 5.08)
					(name "PB_LSRX")
					(number "B5")
				)
				(pin input line
					(at 55.88 -7.62 180)
					(length 5.08)
					(name "PB_RX1_P")
					(number "B7")
				)
				(pin output line
					(at 55.88 -25.4 180)
					(length 5.08)
					(name "PB_TX1_N")
					(number "B9")
				)
				(pin output line
					(at 55.88 -17.78 180)
					(length 5.08)
					(name "PB_TX0_N")
					(number "B11")
				)
				(pin input line
					(at 55.88 -2.54 180)
					(length 5.08)
					(name "PB_RX0_N")
					(number "B13")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PA_RX1_N")
					(number "B15")
				)
				(pin output line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PA_TX1_N")
					(number "B17")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PA_TX0_N")
					(number "B19")
				)
				(pin input line
					(at 0 0 0)
					(length 5.08)
					(name "PA_RX0_P")
					(number "B21")
				)
				(pin bidirectional line
					(at 55.88 -40.64 180)
					(length 5.08)
					(name "PB_USB2_D_N")
					(number "D19")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PA_USB2_D_N")
					(number "D20")
				)
				(pin bidirectional line
					(at 55.88 -38.1 180)
					(length 5.08)
					(name "PB_USB2_D_P")
					(number "E19")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PA_USB2_D_P")
					(number "E20")
				)
				(pin passive line
					(at 55.88 -55.88 180)
					(length 5.08)
					(name "PB_USB2_RBIAS")
					(number "F19")
				)
				(pin input line
					(at 55.88 -50.8 180)
					(length 5.08)
					(name "PB_DPSRC_HPD")
					(number "G2")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PA_USB2_RBIAS")
					(number "H19")
				)
				(pin input line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PA_DPSRC_HPD")
					(number "M4")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PA_DPSRC_AUX_N")
					(number "W15")
				)
				(pin bidirectional line
					(at 55.88 -33.02 180)
					(length 5.08)
					(name "PB_DPSRC_AUX_N")
					(number "W16")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PA_DPSRC_AUX_P")
					(number "Y15")
				)
				(pin bidirectional line
					(at 55.88 -30.48 180)
					(length 5.08)
					(name "PB_DPSRC_AUX_P")
					(number "Y16")
				)
			)
			(symbol "JHL6340SLLSQ_6_0"
				(text "DEBUG"
					(at 24.13 -15.24 0)
				)
			)
			(symbol "JHL6340SLLSQ_6_1"
				(pin passive line
					(at 55.88 -5.08 180)
					(length 5.08)
					(name "ATEST_P")
					(number "A23")
				)
				(pin passive line
					(at 55.88 -25.4 180)
					(length 5.08)
					(name "MONDC_DPSRC")
					(number "AB2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "THERMDA2")
					(number "AB23")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "TEST_EDM")
					(number "AC1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "THERMDA1")
					(number "AC23")
				)
				(pin passive line
					(at 55.88 -7.62 180)
					(length 5.08)
					(name "ATEST_N")
					(number "B23")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "MONDC_CIO_1")
					(number "C22")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "MONDC_CIO_0")
					(number "C23")
				)
				(pin passive line
					(at 55.88 0 180)
					(length 5.08)
					(name "MONDC_SVR")
					(number "D6")
				)
				(pin passive line
					(at 55.88 -12.7 180)
					(length 5.08)
					(name "USB2_ATEST")
					(number "E18")
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "FUSE_VQPS_64")
					(number "L15")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "FUSE_VQPS_128")
					(number "N15")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PCIE_ATEST")
					(number "V18")
				)
				(pin passive line
					(at 55.88 -17.78 180)
					(length 5.08)
					(name "MONDC_DPSNK_0")
					(number "W13")
				)
				(pin passive line
					(at 55.88 -20.32 180)
					(length 5.08)
					(name "MONDC_DPSNK_1")
					(number "W18")
				)
			)
			(embedded_fonts no)
		)
)
