(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "JHL8440"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 91.44 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "JHL8440"
				(at 91.44 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "JHL8440"
				(at 91.44 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.mouser.com/datasheet/2/612/thunderbolt_security_brief-1903286.pdf"
				(at 91.44 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Thunderbolt™ 3 Controller, I/O"
				(at 91.44 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Intel"
				(at 91.44 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "JHL8440"
				(at 91.44 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 91.44 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 91.44 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "JHL8440_1_1"
				(text "FLASH"
					(at 21.59 -6.35 900)
				)
				(text "JTAG"
					(at 21.59 -19.05 900)
				)
				(text "DEBUG"
					(at 21.59 -48.26 900)
				)
				(text "RBIAS\n"
					(at 21.59 -80.01 900)
				)
				(text "MISC &\nDEBUG"
					(at 31.75 -2.54 0)
				)
				(text "LC\nGPIO\n"
					(at 48.26 -13.97 0)
				)
				(text "POC\nGPIO"
					(at 48.26 -45.72 0)
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "P0_MONDC")
					(number "A5")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 5.08)
					(name "P1_MONDC")
					(number "A23")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "TEST_PWR_GOOD")
					(number "AA1")
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 5.08)
					(name "TEST_EDM")
					(number "AB1")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 5.08)
					(name "USB_MONDC")
					(number "AB23")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "P2_MONDC")
					(number "AC1")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "P3_MONDC")
					(number "AC23")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(name "USB2_ATEST")
					(number "B23")
				)
				(pin passive line
					(at 78.74 -81.28 180)
					(length 5.08)
					(name "XTAL_25_OUT")
					(number "C23")
				)
				(pin passive line
					(at 78.74 -78.74 180)
					(length 5.08)
					(name "XTAL_25_IN")
					(number "D23")
				)
				(pin passive line
					(at 78.74 -73.66 180)
					(length 5.08)
					(name "~{RESET}")
					(number "E5")
				)
				(pin passive line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PCIE_RBIAS")
					(number "E18")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "USB2_RBIAS")
					(number "F19")
				)
				(pin passive line
					(at 0 -66.04 0)
					(length 5.08)
					(name "ATEST_N")
					(number "H13")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "ATEST_P")
					(number "H15")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PCIE_ATEST")
					(number "H16")
				)
				(pin passive line
					(at 0 -81.28 0)
					(length 5.08)
					(name "RSENSE")
					(number "J1")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "RBIAS")
					(number "J2")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "MONDC_SVR")
					(number "J4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "EE_DO")
					(number "L1")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(name "~{EE_CS}")
					(number "L2")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "THERMDA")
					(number "L8")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "EE_CLK")
					(number "M1")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "EE_DI")
					(number "M2")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(name "FUSE_VQPS_64")
					(number "M5")
				)
				(pin passive line
					(at 78.74 -60.96 180)
					(length 5.08)
					(name "POC_GPIO_12")
					(number "M20")
					(alternate "HPD" passive line)
					(alternate "~{OVRCRNT}" passive line)
					(alternate "~{PC_I2C_INT}" passive line)
				)
				(pin passive line
					(at 78.74 -33.02 180)
					(length 5.08)
					(name "POC_GPIO_1")
					(number "M22")
					(alternate "I2C_SDA" passive line)
				)
				(pin passive line
					(at 78.74 -30.48 180)
					(length 5.08)
					(name "POC_GPIO_0")
					(number "M23")
					(alternate "I2C_SCL" passive line)
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "TCK")
					(number "N1")
				)
				(pin passive line
					(at 0 -12.7 0)
					(length 5.08)
					(name "TDI")
					(number "N2")
				)
				(pin passive line
					(at 78.74 -63.5 180)
					(length 5.08)
					(name "POC_GPIO_13")
					(number "N20")
					(alternate "USB2_MXCTL" passive line)
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(name "POC_GPIO_3")
					(number "N22")
					(alternate "FORCE_PWR" passive line)
				)
				(pin passive line
					(at 78.74 -35.56 180)
					(length 5.08)
					(name "POC_GPIO_2")
					(number "N23")
					(alternate "PA_VBUS_EN" passive line)
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(name "TDO")
					(number "P1")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "TMS")
					(number "P2")
				)
				(pin passive line
					(at 78.74 -43.18 180)
					(length 5.08)
					(name "POC_GPIO_5")
					(number "P22")
					(alternate "PM_S3_EN" passive line)
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(name "POC_GPIO_4")
					(number "P23")
					(alternate "~{PEWAKE}" passive line)
				)
				(pin passive line
					(at 78.74 0 180)
					(length 5.08)
					(name "GPIO_0")
					(number "R1")
					(alternate "PB_VBUS_EN" passive line)
				)
				(pin passive line
					(at 78.74 -2.54 180)
					(length 5.08)
					(name "GPIO_1")
					(number "R2")
					(alternate "PC_VBUS_EN" passive line)
				)
				(pin passive line
					(at 78.74 -66.04 180)
					(length 5.08)
					(name "POC_GPIO_14")
					(number "R20")
					(alternate "HPD" passive line)
					(alternate "~{OVRCRNT}" passive line)
					(alternate "~{PD_I2C_INT}" passive line)
				)
				(pin passive line
					(at 78.74 -48.26 180)
					(length 5.08)
					(name "POC_GPIO_7")
					(number "R22")
					(alternate "~{OVRCRNT}" passive line)
					(alternate "~{PB_I2C_INT}" passive line)
				)
				(pin passive line
					(at 78.74 -45.72 180)
					(length 5.08)
					(name "POC_GPIO_6")
					(number "R23")
					(alternate "~{PA_I2C_INT}" passive line)
				)
				(pin passive line
					(at 78.74 -5.08 180)
					(length 5.08)
					(name "GPIO_2")
					(number "T1")
					(alternate "PD_VBUS_EN" passive line)
				)
				(pin passive line
					(at 78.74 -7.62 180)
					(length 5.08)
					(name "GPIO_3")
					(number "T2")
					(alternate "TMU_CLKIN" passive line)
				)
				(pin passive line
					(at 78.74 -68.58 180)
					(length 5.08)
					(name "POC_GPIO_15")
					(number "T20")
				)
				(pin passive line
					(at 78.74 -53.34 180)
					(length 5.08)
					(name "POC_GPIO_9")
					(number "T22")
					(alternate "SMBUS_SDA" passive line)
				)
				(pin passive line
					(at 78.74 -50.8 180)
					(length 5.08)
					(name "POC_GPIO_8")
					(number "T23")
					(alternate "SMBUS_SCL" passive line)
				)
				(pin passive line
					(at 78.74 -10.16 180)
					(length 5.08)
					(name "GPIO_4")
					(number "U1")
					(alternate "PM_S0_EN" passive line)
				)
				(pin passive line
					(at 78.74 -12.7 180)
					(length 5.08)
					(name "GPIO_5")
					(number "U2")
					(alternate "~{PERST}" passive line)
				)
				(pin passive line
					(at 78.74 -58.42 180)
					(length 5.08)
					(name "POC_GPIO_11")
					(number "U22")
				)
				(pin passive line
					(at 78.74 -55.88 180)
					(length 5.08)
					(name "POC_GPIO_10")
					(number "U23")
					(alternate "~{PE_OVRCRNT}" passive line)
				)
				(pin passive line
					(at 78.74 -15.24 180)
					(length 5.08)
					(name "GPIO_6")
					(number "V1")
					(alternate "PE_VBUS_EN" passive line)
				)
				(pin passive line
					(at 78.74 -17.78 180)
					(length 5.08)
					(name "GPIO_7")
					(number "V2")
					(alternate "~{SMB_ALERT}" passive line)
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "TEST_EN")
					(number "V23")
				)
				(pin passive line
					(at 78.74 -20.32 180)
					(length 5.08)
					(name "GPIO_8")
					(number "W1")
					(alternate "TMU_CLKOUT" passive line)
				)
				(pin passive line
					(at 78.74 -22.86 180)
					(length 5.08)
					(name "GPIO_9")
					(number "W2")
				)
				(pin passive line
					(at 78.74 -25.4 180)
					(length 5.08)
					(name "GPIO_10")
					(number "Y1")
				)
			)
			(symbol "JHL8440_2_1"
				(text "Output\n3.3V"
					(at 21.59 -2.54 0)
				)
				(text "Input\n3.3V\n"
					(at 49.53 -2.54 0)
				)
				(text "iSVR\n0.9V\n"
					(at 49.53 -19.05 0)
				)
				(text "GND\n"
					(at 49.53 -38.1 0)
				)
				(pin power_in line
					(at 78.74 -22.86 180)
					(length 5.08)
					(name "SVR_VSS")
					(number "A1")
				)
				(pin passive line
					(at 78.74 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "SVR_VSS")
					(number "A2")
				)
				(pin power_in line
					(at 78.74 -12.7 180)
					(length 5.08)
					(name "VCC3P3_SVR")
					(number "A3")
				)
				(pin passive line
					(at 78.74 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3_SVR")
					(number "A4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A8")
				)
				(pin power_in line
					(at 78.74 -40.64 180)
					(length 5.08)
					(name "VSS_ANA")
					(number "A10")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A14")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "A22")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AA2")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AA22")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AA23")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB2")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB10")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB14")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AB22")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC2")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC10")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC14")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "AC22")
				)
				(pin passive line
					(at 78.74 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "SVR_VSS")
					(number "B1")
				)
				(pin passive line
					(at 78.74 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "SVR_VSS")
					(number "B2")
				)
				(pin passive line
					(at 78.74 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3_SVR")
					(number "B3")
				)
				(pin passive line
					(at 78.74 -12.7 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3_SVR")
					(number "B4")
				)
				(pin power_in line
					(at 78.74 -38.1 180)
					(length 5.08)
					(name "VSS")
					(number "B5")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B10")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B14")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "B22")
				)
				(pin passive line
					(at 78.74 -17.78 180)
					(length 5.08)
					(name "SVR_IND")
					(number "C1")
				)
				(pin passive line
					(at 78.74 -17.78 180)
					(length 5.08)
					(hide yes)
					(name "SVR_IND")
					(number "C2")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "C22")
				)
				(pin passive line
					(at 78.74 -17.78 180)
					(length 5.08)
					(hide yes)
					(name "SVR_IND")
					(number "D1")
				)
				(pin passive line
					(at 78.74 -17.78 180)
					(length 5.08)
					(hide yes)
					(name "SVR_IND")
					(number "D2")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D5")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D9")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D11")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D13")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D15")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D19")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "D22")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E1")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E2")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E4")
				)
				(pin power_in line
					(at 78.74 0 180)
					(length 5.08)
					(name "VCC3P3A")
					(number "E6")
				)
				(pin power_in line
					(at 78.74 -30.48 180)
					(length 5.08)
					(name "VCC0P9_SVR_BRD_SENSE")
					(number "E8")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P01_ANA")
					(number "E9")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 5.08)
					(name "VCC0P9_SVR_P01_ANA")
					(number "E11")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P01_ANA")
					(number "E12")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P01_ANA")
					(number "E13")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P01_ANA")
					(number "E15")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P01_ANA")
					(number "E16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E22")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "E23")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F5")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F9")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F11")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F13")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F15")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F16")
				)
				(pin power_in line
					(at 78.74 -2.54 180)
					(length 5.08)
					(name "VCC3P3")
					(number "F18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "F20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "G22")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "G23")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H1")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H2")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H5")
				)
				(pin power_in line
					(at 0 -40.64 0)
					(length 5.08)
					(name "VCC0P9_LVR_SENSE")
					(number "H6")
				)
				(pin power_in line
					(at 0 -38.1 0)
					(length 5.08)
					(name "VCC0P9_LVR")
					(number "H8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H9")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "H11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCC3P3_ANA")
					(number "H12")
				)
				(pin power_in line
					(at 78.74 -7.62 180)
					(length 5.08)
					(name "VCC3P3_ANA_USB2")
					(number "H18")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 5.08)
					(name "VCC0P9_ANA_PCIE_2")
					(number "H19")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 5.08)
					(name "VCC0P9_ANA_PCIE_1")
					(number "H20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J5")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J6")
				)
				(pin power_in line
					(at 0 -33.02 0)
					(length 5.08)
					(name "VCC0P9_LC")
					(number "J8")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "J9")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J11")
				)
				(pin power_in line
					(at 78.74 -27.94 180)
					(length 5.08)
					(name "VCC0P9_SVR")
					(number "J12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J13")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J15")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VCC3P3_ANA_PCIE")
					(number "J16")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_ANA_PCIE_2")
					(number "J18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J19")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J22")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "J23")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "K1")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "K2")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L5")
				)
				(pin passive line
					(at 78.74 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3")
					(number "L6")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "L9")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L11")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "L12")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L13")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "L15")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "L16")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "L18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L19")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L22")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "L23")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M4")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "M6")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M8")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "M9")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M11")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "M12")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M13")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "M15")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M16")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "M18")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "M19")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N4")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N5")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "N6")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N8")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "N9")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N11")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "N12")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N13")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "N15")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N16")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "N18")
				)
				(pin passive line
					(at 78.74 -2.54 180)
					(length 5.08)
					(hide yes)
					(name "VCC3P3")
					(number "N19")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R4")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R5")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "R6")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R8")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "R9")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R11")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "R12")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R13")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "R15")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R16")
				)
				(pin passive line
					(at 78.74 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR")
					(number "R18")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "R19")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCC3P3_LC")
					(number "T4")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T5")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T9")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T11")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCC3P3_ANA")
					(number "T13")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T15")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "T16")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 5.08)
					(name "VCC0P9_SVR_USB_ANA")
					(number "T18")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_USB_ANA")
					(number "T19")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V5")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V9")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V11")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V13")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V15")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V19")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V20")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "V22")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W5")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W6")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W8")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W9")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 5.08)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W11")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W12")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W13")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W15")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(hide yes)
					(name "VCC0P9_SVR_P23_ANA")
					(number "W16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W19")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "W20")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y2")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y4")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y5")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y6")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y8")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y9")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y11")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y12")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y13")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y15")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y16")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y18")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y19")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "VSS_ANA")
					(number "Y20")
				)
			)
			(symbol "JHL8440_3_1"
				(text "Port A\n- UFP"
					(at 21.59 -19.05 0)
				)
				(text "Port E\n"
					(at 21.59 -43.18 0)
				)
				(text "PCIe \nPort\n"
					(at 24.13 -78.74 0)
				)
				(text "Port B\n- UFP"
					(at 52.07 -19.05 0)
				)
				(text "Port C\n- UFP"
					(at 52.07 -55.88 0)
				)
				(text "Port D\n- UFP"
					(at 52.07 -93.98 0)
				)
				(pin passive line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PA_SSRXn2")
					(number "A7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PA_SSTXn2")
					(number "A9")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PA_SSTXp1")
					(number "A11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(name "PA_SSRXp1")
					(number "A13")
				)
				(pin passive line
					(at 78.74 -17.78 180)
					(length 5.08)
					(name "PB_SSRXn2")
					(number "A15")
				)
				(pin passive line
					(at 78.74 -25.4 180)
					(length 5.08)
					(name "PB_SSTXn2")
					(number "A17")
				)
				(pin passive line
					(at 78.74 -7.62 180)
					(length 5.08)
					(name "PB_SSTXp1")
					(number "A19")
				)
				(pin passive line
					(at 78.74 0 180)
					(length 5.08)
					(name "PB_SSRXp1")
					(number "A21")
				)
				(pin passive line
					(at 78.74 -40.64 180)
					(length 5.08)
					(name "PC_SSRXn1")
					(number "AB3")
				)
				(pin passive line
					(at 78.74 -48.26 180)
					(length 5.08)
					(name "PC_SSTXn1")
					(number "AB5")
				)
				(pin passive line
					(at 78.74 -60.96 180)
					(length 5.08)
					(name "PC_SSTXp2")
					(number "AB7")
				)
				(pin passive line
					(at 78.74 -53.34 180)
					(length 5.08)
					(name "PC_SSRXp2")
					(number "AB9")
				)
				(pin passive line
					(at 78.74 -78.74 180)
					(length 5.08)
					(name "PD_SSRXn1")
					(number "AB11")
				)
				(pin passive line
					(at 78.74 -86.36 180)
					(length 5.08)
					(name "PD_SSTXn1")
					(number "AB13")
				)
				(pin passive line
					(at 78.74 -99.06 180)
					(length 5.08)
					(name "PD_SSTXp2")
					(number "AB15")
				)
				(pin passive line
					(at 78.74 -91.44 180)
					(length 5.08)
					(name "PD_SSRXp2")
					(number "AB17")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 5.08)
					(name "U0_SSTXn1")
					(number "AB19")
				)
				(pin passive line
					(at 0 -40.64 0)
					(length 5.08)
					(name "U0_SSRXn1")
					(number "AB21")
				)
				(pin passive line
					(at 78.74 -38.1 180)
					(length 5.08)
					(name "PC_SSRXp1")
					(number "AC3")
				)
				(pin passive line
					(at 78.74 -45.72 180)
					(length 5.08)
					(name "PC_SSTXp1")
					(number "AC5")
				)
				(pin passive line
					(at 78.74 -63.5 180)
					(length 5.08)
					(name "PC_SSTXn2")
					(number "AC7")
				)
				(pin passive line
					(at 78.74 -55.88 180)
					(length 5.08)
					(name "PC_SSRXn2")
					(number "AC9")
				)
				(pin passive line
					(at 78.74 -76.2 180)
					(length 5.08)
					(name "PD_SSRXp1")
					(number "AC11")
				)
				(pin passive line
					(at 78.74 -83.82 180)
					(length 5.08)
					(name "PD_SSTXp1")
					(number "AC13")
				)
				(pin passive line
					(at 78.74 -101.6 180)
					(length 5.08)
					(name "PD_SSTXn2")
					(number "AC15")
				)
				(pin passive line
					(at 78.74 -93.98 180)
					(length 5.08)
					(name "PD_SSRXn2")
					(number "AC17")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 5.08)
					(name "U0_SSTXp1")
					(number "AC19")
				)
				(pin passive line
					(at 0 -38.1 0)
					(length 5.08)
					(name "U0_SSRXp1")
					(number "AC21")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PA_SSRXp2")
					(number "B7")
				)
				(pin passive line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PA_SSTXp2")
					(number "B9")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PA_SSTXn1")
					(number "B11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PA_SSRXn1")
					(number "B13")
				)
				(pin passive line
					(at 78.74 -15.24 180)
					(length 5.08)
					(name "PB_SSRXp2")
					(number "B15")
				)
				(pin passive line
					(at 78.74 -22.86 180)
					(length 5.08)
					(name "PB_SSTXp2")
					(number "B17")
				)
				(pin passive line
					(at 78.74 -10.16 180)
					(length 5.08)
					(name "PB_SSTXn1")
					(number "B19")
				)
				(pin passive line
					(at 78.74 -2.54 180)
					(length 5.08)
					(name "PB_SSRXn1")
					(number "B21")
				)
				(pin passive line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PA_USB2_D_N")
					(number "E19")
				)
				(pin passive line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PA_USB2_D_P")
					(number "E20")
				)
				(pin passive line
					(at 78.74 -30.48 180)
					(length 5.08)
					(name "PB_SBU1")
					(number "F1")
				)
				(pin passive line
					(at 78.74 -33.02 180)
					(length 5.08)
					(name "PB_SBU2")
					(number "F2")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PCIE_REFCLK_100_IN_P")
					(number "F22")
				)
				(pin passive line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PCIE_REFCLK_100_IN_N")
					(number "F23")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PA_SBU1")
					(number "G1")
				)
				(pin passive line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PA_SBU2")
					(number "G2")
				)
				(pin passive line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PCIE_RX0_N")
					(number "H22")
				)
				(pin passive line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PCIE_RX0_P")
					(number "H23")
				)
				(pin passive line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PCIE_TX0_N")
					(number "K22")
				)
				(pin passive line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PCIE_TX0_P")
					(number "K23")
				)
				(pin passive line
					(at 78.74 -68.58 180)
					(length 5.08)
					(name "PC_SBU1")
					(number "W22")
				)
				(pin passive line
					(at 78.74 -71.12 180)
					(length 5.08)
					(name "PC_SBU2")
					(number "W23")
				)
				(pin passive line
					(at 78.74 -106.68 180)
					(length 5.08)
					(name "PD_SBU1")
					(number "Y22")
				)
				(pin passive line
					(at 78.74 -109.22 180)
					(length 5.08)
					(name "PD_SBU2")
					(number "Y23")
				)
			)
			(embedded_fonts no)
		)
)
