(footprint "BGA-264-200_10x14.5mm_Layout12x22_P0.8x0.65mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "http://www.issi.com/WW/pdf/43-46LQ32256A-AL.pdf")
	(property "Reference" "REF**"
		(at -5.25 -7.75 0)
		(layer "F.SilkS")
	)
	(property "Value" "BGA-264-200_10x14.5mm_Layout12x22_P0.8x0.65mm"
		(at -5.5 9 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -5.5 10.25 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -5.5 11.5 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -5.5 12.75 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -4.396 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A2" smd circle
		(at -3.596 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A3" smd circle
		(at -2.795 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A4" smd circle
		(at -1.996 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A5" smd circle
		(at -1.196 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A8" smd circle
		(at 1.205 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A9" smd circle
		(at 2.004 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A10" smd circle
		(at 2.805 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A11" smd circle
		(at 3.604 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "A12" smd circle
		(at 4.405 -6.834)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA1" smd circle
		(at -4.396 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA2" smd circle
		(at -3.596 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA3" smd circle
		(at -2.795 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA4" smd circle
		(at -1.996 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA5" smd circle
		(at -1.196 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA8" smd circle
		(at 1.205 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA9" smd circle
		(at 2.004 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA10" smd circle
		(at 2.805 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA11" smd circle
		(at 3.604 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AA12" smd circle
		(at 4.405 6.166)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB1" smd circle
		(at -4.396 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB2" smd circle
		(at -3.596 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB3" smd circle
		(at -2.795 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB4" smd circle
		(at -1.996 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB5" smd circle
		(at -1.196 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB8" smd circle
		(at 1.205 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB9" smd circle
		(at 2.004 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB10" smd circle
		(at 2.805 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB11" smd circle
		(at 3.604 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "AB12" smd circle
		(at 4.405 6.817)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B1" smd circle
		(at -4.396 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B2" smd circle
		(at -3.596 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B3" smd circle
		(at -2.795 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B4" smd circle
		(at -1.996 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B5" smd circle
		(at -1.196 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B8" smd circle
		(at 1.205 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B9" smd circle
		(at 2.004 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B10" smd circle
		(at 2.805 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B11" smd circle
		(at 3.604 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "B12" smd circle
		(at 4.405 -6.183)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C1" smd circle
		(at -4.396 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C2" smd circle
		(at -3.596 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C3" smd circle
		(at -2.795 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C4" smd circle
		(at -1.996 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C5" smd circle
		(at -1.196 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C8" smd circle
		(at 1.205 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C9" smd circle
		(at 2.004 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C10" smd circle
		(at 2.805 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C11" smd circle
		(at 3.604 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "C12" smd circle
		(at 4.405 -5.534)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D1" smd circle
		(at -4.396 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D2" smd circle
		(at -3.596 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D3" smd circle
		(at -2.795 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D4" smd circle
		(at -1.996 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D5" smd circle
		(at -1.196 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D8" smd circle
		(at 1.205 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D9" smd circle
		(at 2.004 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D10" smd circle
		(at 2.805 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D11" smd circle
		(at 3.604 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "D12" smd circle
		(at 4.405 -4.883)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E1" smd circle
		(at -4.396 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E2" smd circle
		(at -3.596 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E3" smd circle
		(at -2.795 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E4" smd circle
		(at -1.996 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E5" smd circle
		(at -1.196 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E8" smd circle
		(at 1.205 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E9" smd circle
		(at 2.004 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E10" smd circle
		(at 2.805 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E11" smd circle
		(at 3.604 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "E12" smd circle
		(at 4.405 -4.233)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F1" smd circle
		(at -4.396 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F2" smd circle
		(at -3.596 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F3" smd circle
		(at -2.795 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F4" smd circle
		(at -1.996 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F5" smd circle
		(at -1.196 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F8" smd circle
		(at 1.205 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F9" smd circle
		(at 2.004 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F10" smd circle
		(at 2.805 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F11" smd circle
		(at 3.604 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "F12" smd circle
		(at 4.405 -3.584)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G1" smd circle
		(at -4.396 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G2" smd circle
		(at -3.596 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G3" smd circle
		(at -2.795 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G4" smd circle
		(at -1.996 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G5" smd circle
		(at -1.196 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G8" smd circle
		(at 1.205 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G9" smd circle
		(at 2.004 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G10" smd circle
		(at 2.805 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G11" smd circle
		(at 3.604 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "G12" smd circle
		(at 4.405 -2.934)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H1" smd circle
		(at -4.396 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H2" smd circle
		(at -3.596 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H3" smd circle
		(at -2.795 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H4" smd circle
		(at -1.996 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H5" smd circle
		(at -1.196 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H8" smd circle
		(at 1.205 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H9" smd circle
		(at 2.004 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H10" smd circle
		(at 2.805 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H11" smd circle
		(at 3.604 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "H12" smd circle
		(at 4.405 -2.283)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J1" smd circle
		(at -4.396 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J2" smd circle
		(at -3.596 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J3" smd circle
		(at -2.795 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J4" smd circle
		(at -1.996 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J5" smd circle
		(at -1.196 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J8" smd circle
		(at 1.205 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J9" smd circle
		(at 2.004 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J10" smd circle
		(at 2.805 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J11" smd circle
		(at 3.604 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "J12" smd circle
		(at 4.405 -1.633)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K1" smd circle
		(at -4.396 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K2" smd circle
		(at -3.596 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K3" smd circle
		(at -2.795 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K4" smd circle
		(at -1.996 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K5" smd circle
		(at -1.196 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K8" smd circle
		(at 1.205 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K9" smd circle
		(at 2.004 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K10" smd circle
		(at 2.805 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K11" smd circle
		(at 3.604 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "K12" smd circle
		(at 4.405 -0.983)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N1" smd circle
		(at -4.396 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N2" smd circle
		(at -3.596 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N3" smd circle
		(at -2.795 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N4" smd circle
		(at -1.996 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N5" smd circle
		(at -1.196 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N8" smd circle
		(at 1.205 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N9" smd circle
		(at 2.004 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N10" smd circle
		(at 2.805 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N11" smd circle
		(at 3.604 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "N12" smd circle
		(at 4.405 0.966)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P1" smd circle
		(at -4.396 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P2" smd circle
		(at -3.596 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P3" smd circle
		(at -2.795 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P4" smd circle
		(at -1.996 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P5" smd circle
		(at -1.196 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P8" smd circle
		(at 1.205 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P9" smd circle
		(at 2.004 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P10" smd circle
		(at 2.805 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P11" smd circle
		(at 3.604 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "P12" smd circle
		(at 4.405 1.616)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R1" smd circle
		(at -4.396 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R2" smd circle
		(at -3.596 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R3" smd circle
		(at -2.795 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R4" smd circle
		(at -1.996 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R5" smd circle
		(at -1.196 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R8" smd circle
		(at 1.205 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R9" smd circle
		(at 2.004 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R10" smd circle
		(at 2.805 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R11" smd circle
		(at 3.604 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "R12" smd circle
		(at 4.405 2.266)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T1" smd circle
		(at -4.396 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T2" smd circle
		(at -3.596 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T3" smd circle
		(at -2.795 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T4" smd circle
		(at -1.996 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T5" smd circle
		(at -1.196 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T8" smd circle
		(at 1.205 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T9" smd circle
		(at 2.004 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T10" smd circle
		(at 2.805 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T11" smd circle
		(at 3.604 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "T12" smd circle
		(at 4.405 2.917)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U1" smd circle
		(at -4.396 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U2" smd circle
		(at -3.596 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U3" smd circle
		(at -2.795 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U4" smd circle
		(at -1.996 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U5" smd circle
		(at -1.196 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U8" smd circle
		(at 1.205 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U9" smd circle
		(at 2.004 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U10" smd circle
		(at 2.805 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U11" smd circle
		(at 3.604 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "U12" smd circle
		(at 4.405 3.567)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V1" smd circle
		(at -4.396 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V2" smd circle
		(at -3.596 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V3" smd circle
		(at -2.795 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V4" smd circle
		(at -1.996 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V5" smd circle
		(at -1.196 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V8" smd circle
		(at 1.205 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V9" smd circle
		(at 2.004 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V10" smd circle
		(at 2.805 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V11" smd circle
		(at 3.604 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "V12" smd circle
		(at 4.405 4.217)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W1" smd circle
		(at -4.396 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W2" smd circle
		(at -3.596 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W3" smd circle
		(at -2.795 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W4" smd circle
		(at -1.996 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W5" smd circle
		(at -1.196 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W8" smd circle
		(at 1.205 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W9" smd circle
		(at 2.004 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W10" smd circle
		(at 2.805 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W11" smd circle
		(at 3.604 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "W12" smd circle
		(at 4.405 4.866)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y1" smd circle
		(at -4.396 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y2" smd circle
		(at -3.596 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y3" smd circle
		(at -2.795 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y4" smd circle
		(at -1.996 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y5" smd circle
		(at -1.196 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y8" smd circle
		(at 1.205 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y9" smd circle
		(at 2.004 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y10" smd circle
		(at 2.805 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y11" smd circle
		(at 3.604 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "Y12" smd circle
		(at 4.405 5.517)
		(size 0.27 0.27)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(embedded_fonts no)
	(model "antmicro_k4f6e3s4hm_mgcj.glb"
		(offset
			(xyz -5.14444 -6.78224 0.15)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
