(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "K4F6E3S4HM-MGCJ"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 48.26 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "K4F6E3S4HM-MGCJ"
				(at 48.26 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "K4F6E3S4HM-MGCJ"
				(at 48.26 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://semiconductor.samsung.com/dram/lpddr/lpddr4/k4f6e3s4hm-mgcj/"
				(at 48.26 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "LPDDR4 DRAM, 1GX32"
				(at 48.26 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "K4F6E3S4HM-MGCJ"
				(at 48.26 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Samsung Electronics"
				(at 48.26 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 48.26 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 48.26 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "IC, MEMORY, DDR"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "WFBGA200_10X14p5_DS_MRN WFBGA200_10X14p5_DS_MRN-M WFBGA200_10X14p5_DS_MRN-L"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "K4F6E3S4HM-MGCJ_1_1"
				(pin no_connect line
					(at 0 -58.42 0)
					(length 5.08)
					(name "DNU")
					(number "A1")
				)
				(pin no_connect line
					(at 0 -53.34 0)
					(length 5.08)
					(name "DNU")
					(number "A2")
				)
				(pin power_out line
					(at 0 -60.96 0)
					(length 5.08)
					(name "VSS")
					(number "A3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD2")
					(number "A4")
				)
				(pin unspecified line
					(at 34.29 -60.96 180)
					(length 5.08)
					(name "ZQ0")
					(number "A5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "A9")
				)
				(pin no_connect line
					(at 0 -55.88 0)
					(length 5.08)
					(name "DNU")
					(number "B1")
				)
				(pin bidirectional line
					(at 34.29 -10.16 180)
					(length 5.08)
					(name "DQ0_A")
					(number "B2")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDDQ")
					(number "B3")
				)
				(pin bidirectional line
					(at 34.29 -27.94 180)
					(length 5.08)
					(name "DQ7_A")
					(number "B4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "B5")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "B8")
				)
				(pin bidirectional line
					(at 34.29 -48.26 180)
					(length 5.08)
					(name "DQ15_A")
					(number "B9")
				)
				(pin bidirectional line
					(at 34.29 -30.48 180)
					(length 5.08)
					(name "DQ8_A")
					(number "B11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C1")
				)
				(pin bidirectional line
					(at 34.29 -12.7 180)
					(length 5.08)
					(name "DQ1_A")
					(number "C2")
				)
				(pin bidirectional line
					(at 34.29 -50.8 180)
					(length 5.08)
					(name "DMI0_A")
					(number "C3")
				)
				(pin bidirectional line
					(at 34.29 -25.4 180)
					(length 5.08)
					(name "DQ6_A")
					(number "C4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C8")
				)
				(pin bidirectional line
					(at 34.29 -45.72 180)
					(length 5.08)
					(name "DQ14_A")
					(number "C9")
				)
				(pin bidirectional line
					(at 34.29 -53.34 180)
					(length 5.08)
					(name "DMI1_A")
					(number "C10")
				)
				(pin bidirectional line
					(at 34.29 -33.02 180)
					(length 5.08)
					(name "DQ9_A")
					(number "C11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "D1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D2")
				)
				(pin bidirectional line
					(at 34.29 -2.54 180)
					(length 5.08)
					(name "DQS0_t_A")
					(number "D3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "D5")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "D8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D9")
				)
				(pin bidirectional line
					(at 34.29 -7.62 180)
					(length 5.08)
					(name "DQS1_t_A")
					(number "D10")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E1")
				)
				(pin bidirectional line
					(at 34.29 -15.24 180)
					(length 5.08)
					(name "DQ2_A")
					(number "E2")
				)
				(pin bidirectional line
					(at 34.29 0 180)
					(length 5.08)
					(name "DQS0_c_A")
					(number "E3")
				)
				(pin bidirectional line
					(at 34.29 -22.86 180)
					(length 5.08)
					(name "DQ5_A")
					(number "E4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E8")
				)
				(pin bidirectional line
					(at 34.29 -43.18 180)
					(length 5.08)
					(name "DQ13_A")
					(number "E9")
				)
				(pin bidirectional line
					(at 34.29 -5.08 180)
					(length 5.08)
					(name "DQS1_c_A")
					(number "E10")
				)
				(pin bidirectional line
					(at 34.29 -35.56 180)
					(length 5.08)
					(name "DQ10_A")
					(number "E11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDD1")
					(number "F1")
				)
				(pin bidirectional line
					(at 34.29 -17.78 180)
					(length 5.08)
					(name "DQ3_A")
					(number "F2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F3")
				)
				(pin bidirectional line
					(at 34.29 -20.32 180)
					(length 5.08)
					(name "DQ4_A")
					(number "F4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "F5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "F8")
				)
				(pin bidirectional line
					(at 34.29 -40.64 180)
					(length 5.08)
					(name "DQ12_A")
					(number "F9")
				)
				(pin bidirectional line
					(at 34.29 -38.1 180)
					(length 5.08)
					(name "DQ11_A")
					(number "F11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G1")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "ODT_CA_A")
					(number "G2")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "G4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "G9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "H1")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "CA0_A")
					(number "H2")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H3")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "CS0_A")
					(number "H4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "H5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "H8")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "CA2_A")
					(number "H9")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "CA3_A")
					(number "H10")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "CA4_A")
					(number "H11")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J1")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "CA1_A")
					(number "J2")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J3")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "CKE0_A")
					(number "J4")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "J5")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "CK_t_A")
					(number "J8")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "CK_c_A")
					(number "J9")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "CA5_A")
					(number "J11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "K1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "K3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K4")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K5")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "K8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K9")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "N1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N2")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "N3")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N4")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N5")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "N8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N9")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P3")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "P5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "R1")
				)
				(pin no_connect line
					(at 5.08 -40.64 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "R3")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "R5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "R8")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T1")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "T4")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T5")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "T9")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 5.08)
					(name "RESET_n")
					(number "T11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "U1")
				)
			)
			(symbol "K4F6E3S4HM-MGCJ_2_1"
				(pin no_connect line
					(at 29.21 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "A8")
				)
				(pin power_out line
					(at 0 -58.42 0)
					(length 5.08)
					(name "VSS")
					(number "A10")
				)
				(pin no_connect line
					(at 0 -40.64 0)
					(length 5.08)
					(name "DNU")
					(number "A11")
				)
				(pin no_connect line
					(at 0 -50.8 0)
					(length 5.08)
					(name "DNU")
					(number "A12")
				)
				(pin no_connect line
					(at 0 -48.26 0)
					(length 5.08)
					(name "DNU")
					(number "AA1")
				)
				(pin bidirectional line
					(at 34.29 -10.16 180)
					(length 5.08)
					(name "DQ0_B")
					(number "AA2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "AA3")
				)
				(pin bidirectional line
					(at 34.29 -27.94 180)
					(length 5.08)
					(name "DQ7_B")
					(number "AA4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "AA5")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "AA8")
				)
				(pin bidirectional line
					(at 34.29 -48.26 180)
					(length 5.08)
					(name "DQ15_B")
					(number "AA9")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VDDQ")
					(number "AA10")
				)
				(pin bidirectional line
					(at 34.29 -30.48 180)
					(length 5.08)
					(name "DQ8_B")
					(number "AA11")
				)
				(pin no_connect line
					(at 0 -45.72 0)
					(length 5.08)
					(name "DNU")
					(number "AA12")
				)
				(pin no_connect line
					(at 0 -43.18 0)
					(length 5.08)
					(name "DNU")
					(number "AB1")
				)
				(pin no_connect line
					(at 0 -53.34 0)
					(length 5.08)
					(name "DNU")
					(number "AB2")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB3")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VDD2")
					(number "AB4")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB5")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB8")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "AB9")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "AB10")
				)
				(pin no_connect line
					(at 0 -38.1 0)
					(length 5.08)
					(name "DNU")
					(number "AB11")
				)
				(pin no_connect line
					(at 0 -35.56 0)
					(length 5.08)
					(name "DNU")
					(number "AB12")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "B10")
				)
				(pin no_connect line
					(at 0 -55.88 0)
					(length 5.08)
					(name "DNU")
					(number "B12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "C12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "D11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "D12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "E12")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "F10")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VDD1")
					(number "F12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G10")
				)
				(pin no_connect line
					(at 29.21 -58.42 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G11")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "G12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "H12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J10")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "J12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "K10")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "K11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "K12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "N10")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "N11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "N12")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 5.08)
					(name "CA1_B")
					(number "P2")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 5.08)
					(name "CKE0_B")
					(number "P4")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 5.08)
					(name "CK_t_B")
					(number "P8")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 5.08)
					(name "CK_c_B")
					(number "P9")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P10")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 5.08)
					(name "CA5_B")
					(number "P11")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "P12")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 5.08)
					(name "CA0_B")
					(number "R2")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 5.08)
					(name "CS0_B")
					(number "R4")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 5.08)
					(name "CA2_B")
					(number "R9")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 5.08)
					(name "CA3_B")
					(number "R10")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 5.08)
					(name "CA4_B")
					(number "R11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "R12")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 5.08)
					(name "ODT_CA_B")
					(number "T2")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T10")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "T12")
				)
				(pin bidirectional line
					(at 34.29 -17.78 180)
					(length 5.08)
					(name "DQ3_B")
					(number "U2")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "U3")
				)
				(pin bidirectional line
					(at 34.29 -20.32 180)
					(length 5.08)
					(name "DQ4_B")
					(number "U4")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "U5")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VDD2")
					(number "U8")
				)
				(pin bidirectional line
					(at 34.29 -40.64 180)
					(length 5.08)
					(name "DQ12_B")
					(number "U9")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "U10")
				)
				(pin bidirectional line
					(at 34.29 -38.1 180)
					(length 5.08)
					(name "DQ11_B")
					(number "U11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VDD1")
					(number "U12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V1")
				)
				(pin bidirectional line
					(at 34.29 -15.24 180)
					(length 5.08)
					(name "DQ2_B")
					(number "V2")
				)
				(pin bidirectional line
					(at 34.29 0 180)
					(length 5.08)
					(name "DQS0_c_B")
					(number "V3")
				)
				(pin bidirectional line
					(at 34.29 -22.86 180)
					(length 5.08)
					(name "DQ5_B")
					(number "V4")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V5")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V8")
				)
				(pin bidirectional line
					(at 34.29 -43.18 180)
					(length 5.08)
					(name "DQ13_B")
					(number "V9")
				)
				(pin bidirectional line
					(at 34.29 -5.08 180)
					(length 5.08)
					(name "DQS1_c_B")
					(number "V10")
				)
				(pin bidirectional line
					(at 34.29 -35.56 180)
					(length 5.08)
					(name "DQ10_B")
					(number "V11")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "V12")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "W1")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W2")
				)
				(pin bidirectional line
					(at 34.29 -2.54 180)
					(length 5.08)
					(name "DQS0_t_B")
					(number "W3")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W4")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "W5")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "W8")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W9")
				)
				(pin bidirectional line
					(at 34.29 -7.62 180)
					(length 5.08)
					(name "DQS1_t_B")
					(number "W10")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "W11")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VDDQ")
					(number "W12")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y1")
				)
				(pin bidirectional line
					(at 34.29 -12.7 180)
					(length 5.08)
					(name "DQ1_B")
					(number "Y2")
				)
				(pin bidirectional line
					(at 34.29 -50.8 180)
					(length 5.08)
					(name "DMI0_B")
					(number "Y3")
				)
				(pin bidirectional line
					(at 34.29 -25.4 180)
					(length 5.08)
					(name "DQ6_B")
					(number "Y4")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y5")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y8")
				)
				(pin bidirectional line
					(at 34.29 -45.72 180)
					(length 5.08)
					(name "DQ14_B")
					(number "Y9")
				)
				(pin bidirectional line
					(at 34.29 -53.34 180)
					(length 5.08)
					(name "DMI1_B")
					(number "Y10")
				)
				(pin bidirectional line
					(at 34.29 -33.02 180)
					(length 5.08)
					(name "DQ9_B")
					(number "Y11")
				)
				(pin passive line
					(at 0 -58.42 0)
					(length 5.08)
					(hide yes)
					(name "VSS")
					(number "Y12")
				)
			)
			(embedded_fonts no)
		)
)
