(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "KSZ8851SNLI-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "KSZ8851SNLI-TR"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "KSZ8851SNLI-TR"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en581700"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ethernet Controller, MAC & PHY Ethernet Controller, IEEE 802.3, IEEE 802.3u, 3.1 V, 3.5 V, QFN"
				(at 50.8 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KSZ8851SNLI-TR"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, ETHERNET, PHY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "KSZ8851SNLI-TR_1_1"
				(pin output line
					(at 25.4 -15.24 180)
					(length 2.54)
					(name "LED0")
					(number "1")
				)
				(pin output line
					(at 25.4 -45.72 180)
					(length 2.54)
					(name "PME")
					(number "2")
				)
				(pin output line
					(at 25.4 -48.26 180)
					(length 2.54)
					(name "INTRN")
					(number "3")
				)
				(pin power_in line
					(at 0 -43.18 0)
					(length 2.54)
					(name "DGND")
					(number "4")
				)
				(pin power_out line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VDD_CO1.8")
					(number "5")
				)
				(pin passive line
					(at 25.4 -22.86 180)
					(length 2.54)
					(name "EDD_IO")
					(number "6")
				)
				(pin passive line
					(at 25.4 -25.4 180)
					(length 2.54)
					(name "EESK")
					(number "7")
				)
				(pin power_in line
					(at 0 -45.72 0)
					(length 2.54)
					(name "AGND")
					(number "8")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD_A1.8")
					(number "9")
				)
				(pin passive line
					(at 25.4 -27.94 180)
					(length 2.54)
					(name "EECS")
					(number "10")
				)
				(pin passive line
					(at 25.4 -7.62 180)
					(length 2.54)
					(name "RXP")
					(number "11")
				)
				(pin passive line
					(at 25.4 -10.16 180)
					(length 2.54)
					(name "RXM")
					(number "12")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "13")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 2.54)
					(name "TXP")
					(number "14")
				)
				(pin passive line
					(at 25.4 -2.54 180)
					(length 2.54)
					(name "TXM")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDD_A3.3")
					(number "16")
				)
				(pin passive line
					(at 0 -35.56 0)
					(length 2.54)
					(name "ISET")
					(number "17")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(hide yes)
					(name "AGND")
					(number "18")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RSTN")
					(number "19")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 2.54)
					(name "X1")
					(number "20")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 2.54)
					(name "X2")
					(number "21")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "DGND")
					(number "22")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 2.54)
					(name "VDD_D1.8")
					(number "23")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "DGND")
					(number "24")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 2.54)
					(name "VDD_IO")
					(number "25")
				)
				(pin passive line
					(at 25.4 -40.64 180)
					(length 2.54)
					(name "CSN")
					(number "26")
				)
				(pin passive line
					(at 25.4 -35.56 180)
					(length 2.54)
					(name "SO")
					(number "27")
				)
				(pin passive line
					(at 25.4 -38.1 180)
					(length 2.54)
					(name "SCLK")
					(number "28")
				)
				(pin passive line
					(at 0 -43.18 0)
					(length 2.54)
					(hide yes)
					(name "DGND")
					(number "29")
				)
				(pin passive line
					(at 0 -15.24 0)
					(length 2.54)
					(hide yes)
					(name "VDD_IO")
					(number "30")
				)
				(pin passive line
					(at 25.4 -33.02 180)
					(length 2.54)
					(name "SI")
					(number "31")
				)
				(pin output line
					(at 25.4 -17.78 180)
					(length 2.54)
					(name "LED1")
					(number "32")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "EPAD")
					(number "33")
				)
			)
			(embedded_fonts no)
		)
)
