(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "KSZ9031RNXCA"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 76.2 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "KSZ9031RNXCA"
				(at 76.2 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "KSZ9031RNXCA"
				(at 76.2 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002117F.pdf"
				(at 76.2 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ethernet Controller, 1000 Mbps, IEEE 802.3, 1.14 V, 3.465 V, QFN, 48 Pins"
				(at 76.2 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 76.2 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KSZ9031RNXCA"
				(at 76.2 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 76.2 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 76.2 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, ETHERNET, PHY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "KSZ9031RNXCA_1_1"
				(text "10/100/1000"
					(at 21.59 -1.27 0)
				)
				(text "Ethernet PHY"
					(at 21.59 -3.81 0)
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 2.54)
					(name "AVDDH")
					(number "1")
				)
				(pin bidirectional line
					(at 44.45 -13.97 180)
					(length 2.54)
					(name "TXRXP_A")
					(number "2")
				)
				(pin bidirectional line
					(at 44.45 -16.51 180)
					(length 2.54)
					(name "TXRXM_A")
					(number "3")
				)
				(pin power_in line
					(at 44.45 -3.81 180)
					(length 2.54)
					(name "AVDDL")
					(number "4")
				)
				(pin bidirectional line
					(at 44.45 -20.32 180)
					(length 2.54)
					(name "TXRXP_B")
					(number "5")
				)
				(pin bidirectional line
					(at 44.45 -22.86 180)
					(length 2.54)
					(name "TXRXM_B")
					(number "6")
				)
				(pin bidirectional line
					(at 44.45 -26.67 180)
					(length 2.54)
					(name "TXRXP_C")
					(number "7")
				)
				(pin bidirectional line
					(at 44.45 -29.21 180)
					(length 2.54)
					(name "TXRXM_C")
					(number "8")
				)
				(pin passive line
					(at 44.45 -3.81 180)
					(length 2.54)
					(hide yes)
					(name "AVDDL")
					(number "9")
				)
				(pin bidirectional line
					(at 44.45 -33.02 180)
					(length 2.54)
					(name "TXRXP_D")
					(number "10")
				)
				(pin bidirectional line
					(at 44.45 -35.56 180)
					(length 2.54)
					(name "TXRXM_D")
					(number "11")
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 2.54)
					(hide yes)
					(name "AVDDH")
					(number "12")
				)
				(pin no_connect line
					(at 41.91 -53.34 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "13")
				)
				(pin power_in line
					(at 44.45 0 180)
					(length 2.54)
					(name "DVDDL")
					(number "14")
				)
				(pin bidirectional line
					(at 44.45 -44.45 180)
					(length 2.54)
					(name "LED2/PHYAD1")
					(number "15")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "DVDDH")
					(number "16")
				)
				(pin bidirectional line
					(at 44.45 -41.91 180)
					(length 2.54)
					(name "LED1/PHYAD0/PME_N1")
					(number "17")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "DVDDL")
					(number "18")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "TXD0")
					(number "19")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TXD1")
					(number "20")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "TXD2")
					(number "21")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TXD3")
					(number "22")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "DVDDL")
					(number "23")
				)
				(pin input clock
					(at 0 -33.02 0)
					(length 2.54)
					(name "GTX_CLK")
					(number "24")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "TX_EN")
					(number "25")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "DVDDL")
					(number "26")
				)
				(pin input line
					(at 0 -46.99 0)
					(length 2.54)
					(name "RXD3/MODE3")
					(number "27")
				)
				(pin input line
					(at 0 -44.45 0)
					(length 2.54)
					(name "RXD2/MODE2")
					(number "28")
				)
				(pin power_in line
					(at 44.45 -59.69 180)
					(length 2.54)
					(name "VSS")
					(number "29")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "DVDDL")
					(number "30")
				)
				(pin input line
					(at 0 -41.91 0)
					(length 2.54)
					(name "RXD1/MODE1")
					(number "31")
				)
				(pin input line
					(at 0 -39.37 0)
					(length 2.54)
					(name "RXD0/MODE0")
					(number "32")
				)
				(pin input line
					(at 0 -36.83 0)
					(length 2.54)
					(name "RX_DV/CLK125_EN")
					(number "33")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "DVDDH")
					(number "34")
				)
				(pin input clock
					(at 0 -49.53 0)
					(length 2.54)
					(name "RX_CLK/PHYAD2")
					(number "35")
				)
				(pin input line
					(at 0 -13.97 0)
					(length 2.54)
					(name "MDC")
					(number "36")
				)
				(pin input line
					(at 0 -16.51 0)
					(length 2.54)
					(name "MDIO")
					(number "37")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "~{INT/PME}")
					(number "38")
				)
				(pin passive line
					(at 44.45 0 180)
					(length 2.54)
					(hide yes)
					(name "DVDDL")
					(number "39")
				)
				(pin passive line
					(at 0 0 0)
					(length 2.54)
					(hide yes)
					(name "DVDDH")
					(number "40")
				)
				(pin input clock
					(at 0 -53.34 0)
					(length 2.54)
					(name "CLK125_NDO/LED_MODE")
					(number "41")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{RESET}")
					(number "42")
				)
				(pin input line
					(at 44.45 -8.89 180)
					(length 2.54)
					(name "LDO_O")
					(number "43")
				)
				(pin power_in line
					(at 44.45 -6.35 180)
					(length 2.54)
					(name "AVDDL_PLL")
					(number "44")
				)
				(pin input line
					(at 0 -59.69 0)
					(length 2.54)
					(name "XO")
					(number "45")
				)
				(pin input line
					(at 0 -57.15 0)
					(length 2.54)
					(name "XI")
					(number "46")
				)
				(pin no_connect line
					(at 41.91 -52.07 180)
					(length 2.54)
					(hide yes)
					(name "NC")
					(number "47")
				)
				(pin output line
					(at 44.45 -49.53 180)
					(length 2.54)
					(name "ISET")
					(number "48")
				)
				(pin power_in line
					(at 44.45 -57.15 180)
					(length 2.54)
					(name "PAD_GND")
					(number "49")
				)
			)
			(embedded_fonts no)
		)
)
