(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "KTM4GH1AHI01"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 46.99 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "KTM4GH1AHI01"
				(at 46.99 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "KTM4GH1AHI01"
				(at 46.99 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://smartsemi.com/wp-content/uploads/2024/11/SMARTsemi_DS708_KTMxGH1AHI01_rev0.6.pdf"
				(at 46.99 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "eMMC EMMC 5.1 FLASH, 4 GB, x 1 / x 4 / x 8, 95/155/170 MB/s, 9.5/9.5/10 MB/s, 153-FBGA, 1.8V / 3.3V, -40C to +85C (industrial)"
				(at 46.99 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KTM4GH1AHI01"
				(at 46.99 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "SMARTsemi"
				(at 46.99 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 46.99 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 46.99 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "MEMORY, BGA, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "KTM4GH1AHI01_1_1"
				(pin free line
					(at 8.89 2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A1")
				)
				(pin free line
					(at 8.89 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A2")
				)
				(pin bidirectional line
					(at 24.13 0 180)
					(length 3.81)
					(name "DAT0")
					(number "A3")
				)
				(pin bidirectional line
					(at 24.13 -2.54 180)
					(length 3.81)
					(name "DAT1")
					(number "A4")
				)
				(pin bidirectional line
					(at 24.13 -5.08 180)
					(length 3.81)
					(name "DAT2")
					(number "A5")
				)
				(pin power_in line
					(at 0 -25.4 0)
					(length 3.81)
					(name "VSS")
					(number "A6")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "A7")
				)
				(pin free line
					(at 8.89 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A8")
				)
				(pin free line
					(at 8.89 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A9")
				)
				(pin free line
					(at 8.89 1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A10")
				)
				(pin free line
					(at 8.89 0 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A11")
				)
				(pin free line
					(at 8.89 -1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A12")
				)
				(pin free line
					(at 8.89 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A13")
				)
				(pin free line
					(at 8.89 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "A14")
				)
				(pin free line
					(at 6.35 2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B1")
				)
				(pin bidirectional line
					(at 24.13 -7.62 180)
					(length 3.81)
					(name "DAT3")
					(number "B2")
				)
				(pin bidirectional line
					(at 24.13 -10.16 180)
					(length 3.81)
					(name "DAT4")
					(number "B3")
				)
				(pin bidirectional line
					(at 24.13 -12.7 180)
					(length 3.81)
					(name "DAT5")
					(number "B4")
				)
				(pin bidirectional line
					(at 24.13 -15.24 180)
					(length 3.81)
					(name "DAT6")
					(number "B5")
				)
				(pin bidirectional line
					(at 24.13 -17.78 180)
					(length 3.81)
					(name "DAT7")
					(number "B6")
				)
				(pin free line
					(at 6.35 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B7")
				)
				(pin free line
					(at 6.35 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B8")
				)
				(pin free line
					(at 6.35 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B9")
				)
				(pin free line
					(at 6.35 1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B10")
				)
				(pin free line
					(at 6.35 0 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B11")
				)
				(pin free line
					(at 6.35 -1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B12")
				)
				(pin free line
					(at 6.35 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B13")
				)
				(pin free line
					(at 6.35 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "B14")
				)
				(pin free line
					(at 6.35 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C1")
				)
				(pin power_out line
					(at 0 -5.08 0)
					(length 3.81)
					(name "VDDI")
					(number "C2")
				)
				(pin free line
					(at 6.35 -16.51 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C3")
				)
				(pin power_in line
					(at 0 -27.94 0)
					(length 3.81)
					(name "VSSQ")
					(number "C4")
				)
				(pin free line
					(at 6.35 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C5")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 3.81)
					(name "VCCQ")
					(number "C6")
				)
				(pin free line
					(at 6.35 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C7")
				)
				(pin free line
					(at 6.35 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C8")
				)
				(pin free line
					(at 6.35 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C9")
				)
				(pin free line
					(at 6.35 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C10")
				)
				(pin free line
					(at 6.35 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C11")
				)
				(pin free line
					(at 6.35 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C12")
				)
				(pin free line
					(at 6.35 -13.97 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C13")
				)
				(pin free line
					(at 6.35 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "C14")
				)
				(pin free line
					(at 6.35 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D1")
				)
				(pin free line
					(at 6.35 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D2")
				)
				(pin free line
					(at 11.43 2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D3")
				)
				(pin free line
					(at 11.43 1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D4")
				)
				(pin free line
					(at 6.35 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D12")
				)
				(pin free line
					(at 6.35 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D13")
				)
				(pin free line
					(at 6.35 -26.67 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D14")
				)
				(pin free line
					(at 11.43 0 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E1")
				)
				(pin free line
					(at 11.43 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E2")
				)
				(pin free line
					(at 11.43 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E3")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "E5")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCC")
					(number "E6")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "E7")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "E8")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "E9")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "E10")
				)
				(pin free line
					(at 11.43 -1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E12")
				)
				(pin free line
					(at 11.43 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E13")
				)
				(pin free line
					(at 11.43 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "E14")
				)
				(pin free line
					(at 11.43 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F1")
				)
				(pin free line
					(at 8.89 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F2")
				)
				(pin free line
					(at 8.89 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F3")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "F5")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "F10")
				)
				(pin free line
					(at 11.43 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F12")
				)
				(pin free line
					(at 8.89 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F13")
				)
				(pin free line
					(at 11.43 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "F14")
				)
				(pin free line
					(at 8.89 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G1")
				)
				(pin free line
					(at 8.89 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G2")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "G3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G5")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "G10")
				)
				(pin free line
					(at 8.89 -13.97 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G12")
				)
				(pin free line
					(at 8.89 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G13")
				)
				(pin free line
					(at 8.89 -16.51 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "G14")
				)
				(pin free line
					(at 8.89 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H1")
				)
				(pin free line
					(at 8.89 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H2")
				)
				(pin free line
					(at 8.89 -26.67 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H3")
				)
				(pin output line
					(at 24.13 -27.94 180)
					(length 3.81)
					(name "DS")
					(number "H5")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H10")
				)
				(pin free line
					(at 8.89 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H12")
				)
				(pin free line
					(at 8.89 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H13")
				)
				(pin free line
					(at 8.89 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "H14")
				)
				(pin free line
					(at 8.89 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J1")
				)
				(pin free line
					(at 13.97 0 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J2")
				)
				(pin free line
					(at 13.97 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J3")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J5")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "J10")
				)
				(pin free line
					(at 8.89 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J12")
				)
				(pin free line
					(at 13.97 2.54 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J13")
				)
				(pin free line
					(at 13.97 1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "J14")
				)
				(pin free line
					(at 13.97 -1.27 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K1")
				)
				(pin free line
					(at 13.97 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K2")
				)
				(pin free line
					(at 13.97 -8.89 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K3")
				)
				(pin input line
					(at 24.13 -25.4 180)
					(length 3.81)
					(name "~{RST}")
					(number "K5")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "K6")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "K7")
				)
				(pin passive line
					(at 0 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "K9")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "K10")
				)
				(pin free line
					(at 13.97 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K12")
				)
				(pin free line
					(at 13.97 -5.08 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K13")
				)
				(pin free line
					(at 13.97 -6.35 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "K14")
				)
				(pin free line
					(at 13.97 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L1")
				)
				(pin free line
					(at 13.97 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L2")
				)
				(pin free line
					(at 13.97 -16.51 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L3")
				)
				(pin free line
					(at 13.97 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L12")
				)
				(pin free line
					(at 13.97 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L13")
				)
				(pin free line
					(at 13.97 -13.97 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "L14")
				)
				(pin free line
					(at 13.97 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M1")
				)
				(pin free line
					(at 13.97 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M2")
				)
				(pin free line
					(at 13.97 -26.67 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "M4")
				)
				(pin bidirectional line
					(at 24.13 -20.32 180)
					(length 3.81)
					(name "CMD")
					(number "M5")
				)
				(pin input clock
					(at 24.13 -22.86 180)
					(length 3.81)
					(name "CLK")
					(number "M6")
				)
				(pin free line
					(at 13.97 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M7")
				)
				(pin free line
					(at 13.97 -29.21 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M8")
				)
				(pin free line
					(at 11.43 -11.43 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M9")
				)
				(pin free line
					(at 13.97 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M10")
				)
				(pin free line
					(at 13.97 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M11")
				)
				(pin free line
					(at 13.97 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M12")
				)
				(pin free line
					(at 13.97 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M13")
				)
				(pin free line
					(at 13.97 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "M14")
				)
				(pin free line
					(at 11.43 -12.7 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N1")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "N2")
				)
				(pin free line
					(at 11.43 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N3")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "N4")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "N5")
				)
				(pin free line
					(at 11.43 -21.59 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N6")
				)
				(pin free line
					(at 11.43 -22.86 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N7")
				)
				(pin free line
					(at 11.43 -24.13 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N8")
				)
				(pin free line
					(at 11.43 -25.4 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N9")
				)
				(pin free line
					(at 11.43 -13.97 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N10")
				)
				(pin free line
					(at 11.43 -15.24 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N11")
				)
				(pin free line
					(at 11.43 -16.51 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N12")
				)
				(pin free line
					(at 11.43 -17.78 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N13")
				)
				(pin free line
					(at 11.43 -19.05 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "N14")
				)
				(pin free line
					(at 11.43 -26.67 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P1")
				)
				(pin free line
					(at 6.35 -29.21 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "P3")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "P4")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(hide yes)
					(name "VCCQ")
					(number "P5")
				)
				(pin passive line
					(at 0 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "VSSQ")
					(number "P6")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "P7")
				)
				(pin free line
					(at 13.97 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P8")
				)
				(pin free line
					(at 8.89 -29.21 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P9")
				)
				(pin no_connect line
					(at 3.81 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "RFU")
					(number "P10")
				)
				(pin free line
					(at 11.43 -27.94 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P11")
				)
				(pin free line
					(at 11.43 -29.21 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P12")
				)
				(pin free line
					(at 11.43 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P13")
				)
				(pin free line
					(at 6.35 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "P14")
				)
			)
			(embedded_fonts no)
		)
)
