(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "KTM5000B0T"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 76.2 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "KTM5000B0T"
				(at 76.2 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "KTM5000B0T"
				(at 76.2 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/936/KTM50x0_04b_Datasheet_Brief-3105379.pdf"
				(at 76.2 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Display Interface IC DisplayPort 1.4 MST Hub"
				(at 76.2 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Kinetic Technologies"
				(at 76.2 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "KTM5000B0T"
				(at 76.2 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 76.2 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 76.2 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "BGA, DISPLAYPORT, HDMI, SPLITTER, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "KTM5000B0T_1_1"
				(pin output line
					(at 0 0 0)
					(length 3.81)
					(name "HPD_OUT_GPIO2")
					(number "A1")
				)
				(pin input line
					(at 43.18 -40.64 180)
					(length 3.81)
					(name "SSRX2_P_RX3_N")
					(number "A3")
				)
				(pin bidirectional line
					(at 43.18 -33.02 180)
					(length 3.81)
					(name "SSTX2_P_RX2_N")
					(number "A5")
				)
				(pin bidirectional line
					(at 43.18 -22.86 180)
					(length 3.81)
					(name "SSTX1_P_RX1_P")
					(number "A10")
				)
				(pin input line
					(at 43.18 -15.24 180)
					(length 3.81)
					(name "SSRX1_P_RX0_P")
					(number "A12")
				)
				(pin input line
					(at 43.18 -7.62 180)
					(length 3.81)
					(name "TX0_SSRX_P")
					(number "A14")
				)
				(pin output line
					(at 43.18 0 180)
					(length 3.81)
					(name "TX0_SSTX_P")
					(number "A16")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "I2CM_SCL_PCONF1")
					(number "B1")
				)
				(pin input line
					(at 43.18 -38.1 180)
					(length 3.81)
					(name "SSRX2_N_RX3_P")
					(number "B3")
				)
				(pin bidirectional line
					(at 43.18 -30.48 180)
					(length 3.81)
					(name "SSTX2_N_RX2_P")
					(number "B5")
				)
				(pin bidirectional line
					(at 43.18 -25.4 180)
					(length 3.81)
					(name "SSTX1_N_RX1_N")
					(number "B10")
				)
				(pin input line
					(at 43.18 -17.78 180)
					(length 3.81)
					(name "SSRX1_N_RX0_N")
					(number "B12")
				)
				(pin input line
					(at 43.18 -10.16 180)
					(length 3.81)
					(name "TX0_SSRX_N")
					(number "B14")
				)
				(pin output line
					(at 43.18 -2.54 180)
					(length 3.81)
					(name "TX0_SSTX_N")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "~{ALERTN_PPOL}")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "I2CM_SDA_PCONF0")
					(number "D1")
				)
				(pin bidirectional line
					(at 43.18 -48.26 180)
					(length 3.81)
					(name "RX_AUX_N_SBU1")
					(number "D3")
				)
				(pin bidirectional line
					(at 43.18 -45.72 180)
					(length 3.81)
					(name "RX_AUX_P_SBU2")
					(number "D4")
				)
			)
			(symbol "KTM5000B0T_2_1"
				(pin input line
					(at 0 -40.64 0)
					(length 3.81)
					(name "RX_REXT")
					(number "A7")
				)
				(pin bidirectional line
					(at 38.1 -33.02 180)
					(length 3.81)
					(name "SPI_DO")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "GPIO0_I2C_SDA")
					(number "E2")
				)
				(pin bidirectional line
					(at 38.1 -35.56 180)
					(length 3.81)
					(name "SPI_CLK")
					(number "E16")
				)
				(pin bidirectional line
					(at 38.1 -25.4 180)
					(length 3.81)
					(name "SPI_HOLD")
					(number "E17")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "GPIO1_I2C_SCL")
					(number "F2")
				)
				(pin output line
					(at 38.1 -27.94 180)
					(length 3.81)
					(name "SPI_CSN")
					(number "F16")
				)
				(pin bidirectional line
					(at 38.1 -30.48 180)
					(length 3.81)
					(name "SPI_DI")
					(number "F17")
				)
				(pin bidirectional line
					(at 38.1 -22.86 180)
					(length 3.81)
					(name "SPI_WPN")
					(number "G16")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "URX_GPIO8")
					(number "G17")
				)
				(pin output line
					(at 0 -17.78 0)
					(length 3.81)
					(name "UTX_GPIO9")
					(number "H16")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "DBUG0_GPIO6")
					(number "J16")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "I2S_WCK_GPIO14")
					(number "K16")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "DBUG1_GPIO7")
					(number "K17")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "I2S_D0_GPIO16")
					(number "L16")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "I2S_FCK_GPIO15")
					(number "L17")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "I2S_D2_GPIO18")
					(number "M15")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "I2S_D3_GPIO19")
					(number "M16")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "I2S_D1_GPIO17")
					(number "M17")
				)
			)
			(symbol "KTM5000B0T_3_1"
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "TX1_CONFIG1_GPIO11")
					(number "D16")
				)
				(pin bidirectional line
					(at 40.64 -7.62 180)
					(length 3.81)
					(name "TX1_DDC_SDA")
					(number "H1")
				)
				(pin output line
					(at 40.64 -10.16 180)
					(length 3.81)
					(name "TX1_DDC_SCL")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "TX1_CEC_GPIO10")
					(number "K1")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 3.81)
					(name "TX1_HPD_IN")
					(number "K2")
				)
				(pin output line
					(at 40.64 5.08 180)
					(length 3.81)
					(name "TX1_L3_HDMICLK_N")
					(number "N1")
				)
				(pin output line
					(at 40.64 7.62 180)
					(length 3.81)
					(name "TX1_L3_HDMICLK_P")
					(number "P1")
				)
				(pin bidirectional line
					(at 40.64 -2.54 180)
					(length 3.81)
					(name "TX1_AUX_N")
					(number "P3")
				)
				(pin output line
					(at 40.64 12.7 180)
					(length 3.81)
					(name "TX1_L2_HDMICH0_N")
					(number "R1")
				)
				(pin bidirectional line
					(at 40.64 0 180)
					(length 3.81)
					(name "TX1_AUX_P")
					(number "R3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "TX1_CM")
					(number "R5")
				)
				(pin output line
					(at 40.64 15.24 180)
					(length 3.81)
					(name "TX1_L2_HDMICH0_P")
					(number "T1")
				)
				(pin output line
					(at 40.64 20.32 180)
					(length 3.81)
					(name "TX1_L1_HDMICH1_N")
					(number "U1")
				)
				(pin output line
					(at 40.64 22.86 180)
					(length 3.81)
					(name "TX1_L1_HDMICH1_P")
					(number "U2")
				)
				(pin output line
					(at 40.64 27.94 180)
					(length 3.81)
					(name "TX1_L0_HDMICH2_N")
					(number "U3")
				)
				(pin output line
					(at 40.64 30.48 180)
					(length 3.81)
					(name "TX1_L0_HDMICH2_P")
					(number "U4")
				)
			)
			(symbol "KTM5000B0T_4_1"
				(pin output line
					(at 40.64 -10.16 180)
					(length 3.81)
					(name "TX2_DDC_SCL")
					(number "G1")
				)
				(pin bidirectional line
					(at 40.64 -7.62 180)
					(length 3.81)
					(name "TX2_DDC_SDA")
					(number "H2")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "TX2_CONFIG1_GPIO12")
					(number "H17")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 3.81)
					(name "TX2_HPD_IN")
					(number "J2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "TX2_CEC_GPIO37")
					(number "L2")
				)
				(pin bidirectional line
					(at 40.64 -2.54 180)
					(length 3.81)
					(name "TX2_AUX_N")
					(number "M3")
				)
				(pin bidirectional line
					(at 40.64 0 180)
					(length 3.81)
					(name "TX2_AUX_P")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "TX2_CM")
					(number "R8")
				)
				(pin output line
					(at 40.64 5.08 180)
					(length 3.81)
					(name "TX2_L3_HDMICLK_N")
					(number "T6")
				)
				(pin output line
					(at 40.64 30.48 180)
					(length 3.81)
					(name "TX2_L0_HDMICH2_P")
					(number "T11")
				)
				(pin output line
					(at 40.64 7.62 180)
					(length 3.81)
					(name "TX2_L3_HDMICLK_P")
					(number "U6")
				)
				(pin output line
					(at 40.64 12.7 180)
					(length 3.81)
					(name "TX2_L2_HDMICH0_N")
					(number "U7")
				)
				(pin output line
					(at 40.64 15.24 180)
					(length 3.81)
					(name "TX2_L2_HDMICH0_P")
					(number "U8")
				)
				(pin output line
					(at 40.64 20.32 180)
					(length 3.81)
					(name "TX2_L1_HDMICH1_N")
					(number "U9")
				)
				(pin output line
					(at 40.64 22.86 180)
					(length 3.81)
					(name "TX2_L1_HDMICH1_P")
					(number "U10")
				)
				(pin output line
					(at 40.64 27.94 180)
					(length 3.81)
					(name "TX2_L0_HDMICH2_N")
					(number "U11")
				)
			)
			(symbol "KTM5000B0T_5_1"
				(pin output line
					(at 40.64 -10.16 180)
					(length 3.81)
					(name "TX3_DDC_SCL")
					(number "E1")
				)
				(pin input line
					(at 40.64 -15.24 180)
					(length 3.81)
					(name "TX3_HPD_IN")
					(number "F1")
				)
				(pin bidirectional line
					(at 40.64 -7.62 180)
					(length 3.81)
					(name "TX3_DDC_SDA")
					(number "G2")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "TX3_CONFIG1_GPIO13")
					(number "J17")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "TX3_CEC_GPIO36")
					(number "L1")
				)
				(pin bidirectional line
					(at 40.64 -2.54 180)
					(length 3.81)
					(name "TX3_AUX_N")
					(number "P15")
				)
				(pin output line
					(at 40.64 30.48 180)
					(length 3.81)
					(name "TX3_L0_HDMICH2_P")
					(number "P17")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "TX3_CM")
					(number "R12")
				)
				(pin bidirectional line
					(at 40.64 0 180)
					(length 3.81)
					(name "TX3_AUX_P")
					(number "R15")
				)
				(pin output line
					(at 40.64 27.94 180)
					(length 3.81)
					(name "TX3_L0_HDMICH2_N")
					(number "R17")
				)
				(pin output line
					(at 40.64 22.86 180)
					(length 3.81)
					(name "TX3_L1_HDMICH1_P")
					(number "T17")
				)
				(pin output line
					(at 40.64 5.08 180)
					(length 3.81)
					(name "TX3_L3_HDMICLK_N")
					(number "U13")
				)
				(pin output line
					(at 40.64 7.62 180)
					(length 3.81)
					(name "TX3_L3_HDMICLK_P")
					(number "U14")
				)
				(pin output line
					(at 40.64 12.7 180)
					(length 3.81)
					(name "TX3_L2_HDMICH0_N")
					(number "U15")
				)
				(pin output line
					(at 40.64 15.24 180)
					(length 3.81)
					(name "TX3_L2_HDMICH0_P")
					(number "U16")
				)
				(pin output line
					(at 40.64 20.32 180)
					(length 3.81)
					(name "TX3_L1_HDMICH1_N")
					(number "U17")
				)
			)
			(symbol "KTM5000B0T_6_1"
				(pin output line
					(at 34.29 0 180)
					(length 3.81)
					(name "REFCLK_OUT")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "~{EXT_RESETN}")
					(number "B7")
				)
				(pin bidirectional line
					(at 34.29 -5.08 180)
					(length 3.81)
					(name "XTAL_IN")
					(number "C7")
				)
				(pin bidirectional line
					(at 34.29 -10.16 180)
					(length 3.81)
					(name "XTAL_OUT")
					(number "C8")
				)
			)
			(symbol "KTM5000B0T_7_1"
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A9")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 3.81)
					(name "GND")
					(number "A11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "A17")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "B17")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C3")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C9")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "AVDD18_UFP")
					(number "C10")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_UFP")
					(number "C11")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_UFP")
					(number "C12")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_UFP")
					(number "C13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C16")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C17")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D2")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D5")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D6")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D7")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D8")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D9")
				)
				(pin power_in line
					(at 33.02 0 180)
					(length 3.81)
					(name "AVDDP9_UFP")
					(number "D10")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D11")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D12")
				)
				(pin passive line
					(at 33.02 0 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_UFP")
					(number "D13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "D14")
				)
				(pin no_connect line
					(at 29.21 -26.67 180)
					(length 3.81)
					(hide yes)
					(name "NC")
					(number "D15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E3")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "E4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E13")
				)
				(pin power_in line
					(at 33.02 -20.32 180)
					(length 3.81)
					(name "DVDDP9")
					(number "E14")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "DVDD18")
					(number "E15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F3")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "F4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "F13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "F14")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "DVDD18")
					(number "F15")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "DVDD18")
					(number "G3")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "G4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "TEST")
					(number "G15")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "DVDD18")
					(number "H3")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "H4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "H13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "H14")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "DVDD18")
					(number "H15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J3")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "J4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "J13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "J14")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "DVDD18")
					(number "J15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "K4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "K13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "K14")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "DVDD18")
					(number "K15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L3")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "L4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "L13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "L14")
				)
				(pin passive line
					(at 0 -20.32 0)
					(length 3.81)
					(hide yes)
					(name "DVDD18")
					(number "L15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M1")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M2")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "M4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "M13")
				)
				(pin passive line
					(at 33.02 -20.32 180)
					(length 3.81)
					(hide yes)
					(name "DVDDP9")
					(number "M14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N6")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N11")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N16")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "N17")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P2")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P4")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P5")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P6")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P7")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P8")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P9")
				)
				(pin power_in line
					(at 33.02 -10.16 180)
					(length 3.81)
					(name "AVDDP9_TX")
					(number "P10")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P11")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P12")
				)
				(pin passive line
					(at 33.02 -10.16 180)
					(length 3.81)
					(hide yes)
					(name "AVDDP9_TX")
					(number "P13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "P16")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "R2")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_TX")
					(number "R4")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_TX")
					(number "R6")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_TX")
					(number "R7")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_TX")
					(number "R9")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "AVDD18_TX")
					(number "R10")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_TX")
					(number "R11")
				)
				(pin passive line
					(at 0 -10.16 0)
					(length 3.81)
					(hide yes)
					(name "AVDD18_TX")
					(number "R13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "R14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "R16")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T2")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T3")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T4")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T7")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T8")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T9")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T10")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T12")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T13")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T14")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T15")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "T16")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "U5")
				)
				(pin passive line
					(at 0 -30.48 0)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "U12")
				)
			)
			(embedded_fonts no)
		)
)
