(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LAN8720A-CP-TR-ABC"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 53.34 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LAN8720A-CP-TR-ABC"
				(at 53.34 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LAN8720A-CP-TR-ABC"
				(at 53.34 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/8720a.pdf"
				(at 53.34 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ethernet Controller, 100 Mbps, IEEE 802.3, IEEE 802.3u, 3 V, 3.6 V, SQFN, 24 Pins"
				(at 53.34 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LAN8720A-CP-TR-ABC"
				(at 53.34 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 53.34 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 53.34 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 53.34 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, TRANSCEIVER, IC, ETHERNET, PHY, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LAN8720A-CP-TR-ABC_1_1"
				(text "RMII"
					(at 14.605 -12.7 0)
				)
				(pin power_in line
					(at 38.1 -2.54 180)
					(length 2.54)
					(name "VDD2A")
					(number "1")
				)
				(pin bidirectional line
					(at 38.1 -40.64 180)
					(length 2.54)
					(name "LED2/NINTSEL")
					(number "2")
				)
				(pin bidirectional line
					(at 38.1 -38.1 180)
					(length 2.54)
					(name "LED1/REGOFF")
					(number "3")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "XTAL2")
					(number "4")
				)
				(pin passive line
					(at 0 -45.72 0)
					(length 2.54)
					(name "XTAL1/CLKIN")
					(number "5")
				)
				(pin power_in line
					(at 38.1 -5.08 180)
					(length 2.54)
					(name "VDDCR")
					(number "6")
				)
				(pin output line
					(at 0 -35.56 0)
					(length 2.54)
					(name "RXD1/MODE1")
					(number "7")
				)
				(pin output line
					(at 0 -33.02 0)
					(length 2.54)
					(name "RXD0/MODE0")
					(number "8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "VDDIO")
					(number "9")
				)
				(pin output line
					(at 0 -38.1 0)
					(length 2.54)
					(name "RXER/PHYAD0")
					(number "10")
				)
				(pin output line
					(at 0 -30.48 0)
					(length 2.54)
					(name "CRS_DV/MODE2")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "MDIO")
					(number "12")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 2.54)
					(name "MDC")
					(number "13")
				)
				(pin output line
					(at 0 -7.62 0)
					(length 2.54)
					(name "~{INT}/REFCLKO")
					(number "14")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 2.54)
					(name "~{RST}")
					(number "15")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 2.54)
					(name "TXEN")
					(number "16")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "TXD0")
					(number "17")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "TXD1")
					(number "18")
				)
				(pin power_in line
					(at 38.1 0 180)
					(length 2.54)
					(name "VDD1A")
					(number "19")
				)
				(pin output line
					(at 38.1 -25.4 180)
					(length 2.54)
					(name "TXN")
					(number "20")
				)
				(pin output line
					(at 38.1 -22.86 180)
					(length 2.54)
					(name "TXP")
					(number "21")
				)
				(pin output line
					(at 38.1 -30.48 180)
					(length 2.54)
					(name "RXN")
					(number "22")
				)
				(pin output line
					(at 38.1 -27.94 180)
					(length 2.54)
					(name "RXP")
					(number "23")
				)
				(pin input line
					(at 38.1 -45.72 180)
					(length 2.54)
					(name "RBIAS")
					(number "24")
				)
				(pin power_in line
					(at 38.1 -48.26 180)
					(length 2.54)
					(name "VSS")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
