(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LAN8742A-CZ-TR"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LAN8742A-CZ-TR"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LAN8742A-CZ-TR"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/DS_LAN8742_00001989A.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "Ethernet ICs Small Footprint RMII 10/100 Ethernet Transceiver"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Manufacturer" "Microchip Technology"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LAN8742A-CZ-TR"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "T_storage" "[-55,150]"
				(at 55.88 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "T_abient" "[0,70]"
				(at 55.88 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC, PHY, ETHERNET, TRANSCEIVER, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LAN8742A-CZ-TR_1_1"
				(pin power_in line
					(at 40.64 -5.08 180)
					(length 2.54)
					(name "VDD2A")
					(number "1")
				)
				(pin output line
					(at 40.64 -43.18 180)
					(length 2.54)
					(name "LED2")
					(number "2")
					(alternate "~{INTSEL}" input line)
					(alternate "~{INT}" output line)
					(alternate "~{PME}" output line)
				)
				(pin output line
					(at 40.64 -40.64 180)
					(length 2.54)
					(name "LED1")
					(number "3")
					(alternate "REGOFF" input line)
					(alternate "~{INT}" output line)
					(alternate "~{PME}" output line)
				)
				(pin passive line
					(at 0 -50.8 0)
					(length 2.54)
					(name "XTAL2")
					(number "4")
				)
				(pin passive line
					(at 0 -48.26 0)
					(length 2.54)
					(name "XTAL1")
					(number "5")
					(alternate "CLKIN" input clock)
				)
				(pin passive line
					(at 40.64 -7.62 180)
					(length 2.54)
					(name "VDDCR")
					(number "6")
				)
				(pin output line
					(at 0 -20.32 0)
					(length 2.54)
					(name "RXD1")
					(number "7")
					(alternate "MODE1" input line)
				)
				(pin output line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RXD0")
					(number "8")
					(alternate "MODE0" input line)
				)
				(pin power_in line
					(at 40.64 0 180)
					(length 2.54)
					(name "VDDIO")
					(number "9")
				)
				(pin output line
					(at 0 -27.94 0)
					(length 2.54)
					(name "RXER")
					(number "10")
					(alternate "PHYAD0" input line)
				)
				(pin output line
					(at 0 -25.4 0)
					(length 2.54)
					(name "CRS_DV")
					(number "11")
					(alternate "MODE2" input line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 2.54)
					(name "MDIO")
					(number "12")
				)
				(pin input clock
					(at 0 0 0)
					(length 2.54)
					(name "MDC")
					(number "13")
				)
				(pin output line
					(at 0 -43.18 0)
					(length 2.54)
					(name "~{INT}")
					(number "14")
					(alternate "REFCLKO" output clock)
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{RST}")
					(number "15")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 2.54)
					(name "TXEN")
					(number "16")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 2.54)
					(name "TXD0")
					(number "17")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 2.54)
					(name "TXD1")
					(number "18")
				)
				(pin power_in line
					(at 40.64 -2.54 180)
					(length 2.54)
					(name "VDD1A")
					(number "19")
				)
				(pin bidirectional line
					(at 40.64 -27.94 180)
					(length 2.54)
					(name "TXN")
					(number "20")
				)
				(pin bidirectional line
					(at 40.64 -25.4 180)
					(length 2.54)
					(name "TXP")
					(number "21")
				)
				(pin bidirectional line
					(at 40.64 -35.56 180)
					(length 2.54)
					(name "RXN")
					(number "22")
				)
				(pin bidirectional line
					(at 40.64 -33.02 180)
					(length 2.54)
					(name "RXP")
					(number "23")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "RBIAS")
					(number "24")
				)
				(pin power_in line
					(at 40.64 -50.8 180)
					(length 2.54)
					(name "VSS")
					(number "25")
				)
			)
			(embedded_fonts no)
		)
)
