(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LCMXO3D-9400HC-5BG400C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 55.88 -2.54 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LCMXO3D-9400HC-5BG400C"
				(at 55.88 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LCMXO3D-9400HC-5BG400C"
				(at 55.88 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/6971/CertusPro-NX%20Family%20Datasheet.pdf"
				(at 55.88 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FPGA - Field Programmable Gate Array Lattice MachXO3D ; 9400LUTs 2.5V/3.3V"
				(at 55.88 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LCMXO3D-9400HC-5BG400C"
				(at 55.88 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lattice Semiconductor"
				(at 55.88 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 55.88 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 55.88 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "FPGA, IC, SMT, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LCMXO3D-9400HC-5BG400C_1_1"
				(pin bidirectional line
					(at 0 -6.35 0)
					(length 7.62)
					(name "PT9B")
					(number "A1")
				)
				(pin bidirectional line
					(at 0 -16.51 0)
					(length 7.62)
					(name "PT10B")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -26.67 0)
					(length 7.62)
					(name "PT11B")
					(number "A3")
				)
				(pin bidirectional line
					(at 0 -36.83 0)
					(length 7.62)
					(name "PT12B")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -46.99 0)
					(length 7.62)
					(name "PT14B")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -57.15 0)
					(length 7.62)
					(name "PT15B")
					(number "A6")
				)
				(pin bidirectional line
					(at 0 -67.31 0)
					(length 7.62)
					(name "PT20B")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -77.47 0)
					(length 7.62)
					(name "PT21B")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -87.63 0)
					(length 7.62)
					(name "PT22B")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -97.79 0)
					(length 7.62)
					(name "PT23B")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -107.95 0)
					(length 7.62)
					(name "PT24B")
					(number "A11")
				)
				(pin bidirectional line
					(at 41.91 -3.81 180)
					(length 7.62)
					(name "PT27A")
					(number "A12")
				)
				(pin bidirectional line
					(at 41.91 -13.97 180)
					(length 7.62)
					(name "PT28A")
					(number "A13")
				)
				(pin bidirectional line
					(at 41.91 -24.13 180)
					(length 7.62)
					(name "PT29A")
					(number "A14")
				)
				(pin bidirectional line
					(at 41.91 -34.29 180)
					(length 7.62)
					(name "PT31A")
					(number "A15")
				)
				(pin bidirectional line
					(at 41.91 -44.45 180)
					(length 7.62)
					(name "PT38A")
					(number "A16")
				)
				(pin bidirectional line
					(at 41.91 -54.61 180)
					(length 7.62)
					(name "PT39A")
					(number "A17")
				)
				(pin bidirectional line
					(at 41.91 -74.93 180)
					(length 7.62)
					(name "PT42A")
					(number "A18")
				)
				(pin bidirectional line
					(at 41.91 -102.87 180)
					(length 7.62)
					(name "PT44D")
					(number "A19")
				)
				(pin bidirectional line
					(at 41.91 -97.79 180)
					(length 7.62)
					(name "PT44B")
					(number "A20")
				)
				(pin bidirectional line
					(at 0 -3.81 0)
					(length 7.62)
					(name "PT9A")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -13.97 0)
					(length 7.62)
					(name "PT10A")
					(number "B2")
				)
				(pin bidirectional line
					(at 0 -24.13 0)
					(length 7.62)
					(name "PT11A")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -34.29 0)
					(length 7.62)
					(name "PT12A")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -44.45 0)
					(length 7.62)
					(name "PT14A")
					(number "B5")
				)
				(pin bidirectional line
					(at 0 -54.61 0)
					(length 7.62)
					(name "PT15A")
					(number "B6")
				)
				(pin bidirectional line
					(at 0 -64.77 0)
					(length 7.62)
					(name "PT20A")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -74.93 0)
					(length 7.62)
					(name "PT21A")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -85.09 0)
					(length 7.62)
					(name "PT22A")
					(number "B9")
				)
				(pin bidirectional line
					(at 0 -95.25 0)
					(length 7.62)
					(name "PT23A")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -105.41 0)
					(length 7.62)
					(name "PT24A")
					(number "B11")
				)
				(pin bidirectional line
					(at 41.91 -6.35 180)
					(length 7.62)
					(name "PT27B")
					(number "B12")
				)
				(pin bidirectional line
					(at 41.91 -16.51 180)
					(length 7.62)
					(name "PT28B")
					(number "B13")
				)
				(pin bidirectional line
					(at 41.91 -26.67 180)
					(length 7.62)
					(name "PT29B")
					(number "B14")
				)
				(pin bidirectional line
					(at 41.91 -36.83 180)
					(length 7.62)
					(name "PT31B")
					(number "B15")
				)
				(pin bidirectional line
					(at 41.91 -46.99 180)
					(length 7.62)
					(name "PT38B")
					(number "B16")
				)
				(pin bidirectional line
					(at 41.91 -57.15 180)
					(length 7.62)
					(name "PT39B")
					(number "B17")
				)
				(pin bidirectional line
					(at 41.91 -77.47 180)
					(length 7.62)
					(name "PT42B")
					(number "B18")
				)
				(pin bidirectional line
					(at 41.91 -95.25 180)
					(length 7.62)
					(name "PT44A")
					(number "B19")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "C5")
				)
				(pin bidirectional line
					(at 0 -39.37 0)
					(length 7.62)
					(name "PT12C")
					(number "C6")
				)
				(pin bidirectional line
					(at 0 -62.23 0)
					(length 7.62)
					(name "PT15D")
					(number "C7")
				)
				(pin bidirectional line
					(at 0 -82.55 0)
					(length 7.62)
					(name "PT21D")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -90.17 0)
					(length 7.62)
					(name "PT22C")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -113.03 0)
					(length 7.62)
					(name "PT24D")
					(number "C10")
				)
				(pin bidirectional line
					(at 41.91 -8.89 180)
					(length 7.62)
					(name "PT27C")
					(number "C11")
				)
				(pin bidirectional line
					(at 41.91 -31.75 180)
					(length 7.62)
					(name "PT30B")
					(number "C12")
				)
				(pin bidirectional line
					(at 41.91 -39.37 180)
					(length 7.62)
					(name "PT31C")
					(number "C13")
				)
				(pin bidirectional line
					(at 41.91 -59.69 180)
					(length 7.62)
					(name "PT39C")
					(number "C14")
				)
				(pin bidirectional line
					(at 41.91 -64.77 180)
					(length 7.62)
					(name "PT41A")
					(number "C15")
				)
				(pin bidirectional line
					(at 41.91 -67.31 180)
					(length 7.62)
					(name "PT41B")
					(number "C16")
				)
				(pin bidirectional line
					(at 41.91 -100.33 180)
					(length 7.62)
					(name "PT44C")
					(number "C17")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "D3")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -21.59 0)
					(length 7.62)
					(name "PT10D")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -29.21 0)
					(length 7.62)
					(name "PT11C")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -41.91 0)
					(length 7.62)
					(name "PT12D")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -80.01 0)
					(length 7.62)
					(name "PT21C")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 -92.71 0)
					(length 7.62)
					(name "PT22D")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -110.49 0)
					(length 7.62)
					(name "PT24C")
					(number "D10")
				)
				(pin bidirectional line
					(at 41.91 -11.43 180)
					(length 7.62)
					(name "PT27D")
					(number "D11")
				)
				(pin bidirectional line
					(at 41.91 -29.21 180)
					(length 7.62)
					(name "PT30A")
					(number "D12")
				)
				(pin bidirectional line
					(at 41.91 -41.91 180)
					(length 7.62)
					(name "PT31D")
					(number "D13")
				)
				(pin bidirectional line
					(at 41.91 -62.23 180)
					(length 7.62)
					(name "PT39D")
					(number "D14")
				)
				(pin bidirectional line
					(at 41.91 -82.55 180)
					(length 7.62)
					(name "PT42D")
					(number "D15")
				)
				(pin bidirectional line
					(at 41.91 -87.63 180)
					(length 7.62)
					(name "PT43B")
					(number "D16")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin bidirectional line
					(at 0 -19.05 0)
					(length 7.62)
					(name "PT10C")
					(number "E6")
				)
				(pin bidirectional line
					(at 0 -31.75 0)
					(length 7.62)
					(name "PT11D")
					(number "E7")
				)
				(pin bidirectional line
					(at 0 -59.69 0)
					(length 7.62)
					(name "PT15C")
					(number "E8")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E9")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E10")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E11")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E12")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E13")
				)
				(pin bidirectional line
					(at 41.91 -80.01 180)
					(length 7.62)
					(name "PT42C")
					(number "E14")
				)
				(pin bidirectional line
					(at 41.91 -85.09 180)
					(length 7.62)
					(name "PT43A")
					(number "E15")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E16")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "E18")
				)
				(pin bidirectional line
					(at 0 -11.43 0)
					(length 7.62)
					(name "PT9D")
					(number "F7")
				)
				(pin bidirectional line
					(at 0 -52.07 0)
					(length 7.62)
					(name "PT14D")
					(number "F8")
				)
				(pin bidirectional line
					(at 0 -72.39 0)
					(length 7.62)
					(name "PT20D")
					(number "F9")
				)
				(pin bidirectional line
					(at 0 -102.87 0)
					(length 7.62)
					(name "PT23D")
					(number "F10")
				)
				(pin bidirectional line
					(at 41.91 -21.59 180)
					(length 7.62)
					(name "PT28D")
					(number "F11")
				)
				(pin bidirectional line
					(at 41.91 -52.07 180)
					(length 7.62)
					(name "PT38D")
					(number "F12")
				)
				(pin bidirectional line
					(at 41.91 -72.39 180)
					(length 7.62)
					(name "PT41D")
					(number "F13")
				)
				(pin bidirectional line
					(at 41.91 -92.71 180)
					(length 7.62)
					(name "PT43D")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -8.89 0)
					(length 7.62)
					(name "PT9C")
					(number "G7")
				)
				(pin bidirectional line
					(at 0 -49.53 0)
					(length 7.62)
					(name "PT14C")
					(number "G8")
				)
				(pin bidirectional line
					(at 0 -69.85 0)
					(length 7.62)
					(name "PT20C")
					(number "G9")
				)
				(pin bidirectional line
					(at 0 -100.33 0)
					(length 7.62)
					(name "PT23C")
					(number "G10")
				)
				(pin bidirectional line
					(at 41.91 -19.05 180)
					(length 7.62)
					(name "PT28C")
					(number "G11")
				)
				(pin bidirectional line
					(at 41.91 -49.53 180)
					(length 7.62)
					(name "PT38C")
					(number "G12")
				)
				(pin bidirectional line
					(at 41.91 -69.85 180)
					(length 7.62)
					(name "PT41C")
					(number "G13")
				)
				(pin bidirectional line
					(at 41.91 -90.17 180)
					(length 7.62)
					(name "PT43C")
					(number "G14")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "G18")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "H5")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO0")
					(number "H8")
				)
				(pin power_in line
					(at 41.91 0 180)
					(length 7.62)
					(name "VCCIO0")
					(number "H9")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO0")
					(number "H10")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO0")
					(number "H11")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "H12")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "H13")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "J9")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "J10")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "J11")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO0")
					(number "J12")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "K3")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "K10")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "K12")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "L8")
				)
				(pin power_in line
					(at 0 0 0)
					(length 7.62)
					(name "VCC")
					(number "L9")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "L10")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "L12")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "L18")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "M10")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "M11")
				)
				(pin passive line
					(at 0 0 0)
					(length 7.62)
					(hide yes)
					(name "VCC")
					(number "M12")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "N7")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "R18")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "T15")
				)
				(pin power_in line
					(at 41.91 -113.03 180)
					(length 7.62)
					(name "GND")
					(number "U3")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "U7")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "U8")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "U13")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "U16")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "V7")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 41.91 -113.03 180)
					(length 7.62)
					(hide yes)
					(name "GND")
					(number "V18")
				)
			)
			(symbol "LCMXO3D-9400HC-5BG400C_2_1"
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 7.62)
					(name "PR4A")
					(number "B20")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 7.62)
					(name "PR2B")
					(number "C18")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 7.62)
					(name "PR3A")
					(number "C19")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 7.62)
					(name "PR4B")
					(number "C20")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 7.62)
					(name "PR2A")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 7.62)
					(name "PR3D")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 7.62)
					(name "PR5A")
					(number "D19")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 7.62)
					(name "PR5C")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 7.62)
					(name "PR3B")
					(number "E17")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 7.62)
					(name "PR5D")
					(number "E19")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 7.62)
					(name "PR6D")
					(number "E20")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 7.62)
					(name "PR2C")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 7.62)
					(name "PR3C")
					(number "F16")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 7.62)
					(name "PR5B")
					(number "F17")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 7.62)
					(name "PR6B")
					(number "F18")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 7.62)
					(name "PR7A")
					(number "F19")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 7.62)
					(name "PR7B")
					(number "F20")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 7.62)
					(name "PR2D")
					(number "G15")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 7.62)
					(name "PR6A")
					(number "G16")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 7.62)
					(name "PR6C")
					(number "G17")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 7.62)
					(name "PR11A")
					(number "G19")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 7.62)
					(name "PR11D")
					(number "G20")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 7.62)
					(name "PR4C")
					(number "H14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 7.62)
					(name "PR4D")
					(number "H15")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 7.62)
					(name "PR11C")
					(number "H16")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 7.62)
					(name "PR11B")
					(number "H17")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 7.62)
					(name "PR12A")
					(number "H18")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 7.62)
					(name "PR12B")
					(number "H19")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 7.62)
					(name "PR12D")
					(number "H20")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO1")
					(number "J13")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 7.62)
					(name "PR10C")
					(number "J14")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 7.62)
					(name "PR10D")
					(number "J15")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 7.62)
					(name "PR14B")
					(number "J16")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 7.62)
					(name "PR12C")
					(number "J17")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 7.62)
					(name "PR14A")
					(number "J18")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 7.62)
					(name "PR16A")
					(number "J19")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 7.62)
					(name "PR16B")
					(number "J20")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO1")
					(number "K13")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 7.62)
					(name "PR14C")
					(number "K14")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 7.62)
					(name "PR14D")
					(number "K15")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 7.62)
					(name "PR17C")
					(number "K16")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 7.62)
					(name "PR16C")
					(number "K17")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 7.62)
					(name "PR16D")
					(number "K18")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 7.62)
					(name "PR17A")
					(number "K19")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 7.62)
					(name "PR17B")
					(number "K20")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO1")
					(number "L13")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 7.62)
					(name "PR18C")
					(number "L14")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 7.62)
					(name "PR18D")
					(number "L15")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 7.62)
					(name "PR19C")
					(number "L16")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 7.62)
					(name "PR17D")
					(number "L17")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 7.62)
					(name "PR18A")
					(number "L19")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 7.62)
					(name "PR18B")
					(number "L20")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO1")
					(number "M13")
				)
				(pin bidirectional line
					(at 41.91 -58.42 180)
					(length 7.62)
					(name "PR24D")
					(number "M14")
				)
				(pin bidirectional line
					(at 41.91 -55.88 180)
					(length 7.62)
					(name "PR24C")
					(number "M15")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 7.62)
					(name "PR20C")
					(number "M16")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 7.62)
					(name "PR20A")
					(number "M17")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 7.62)
					(name "PR19D")
					(number "M18")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 7.62)
					(name "PR19B")
					(number "M19")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 7.62)
					(name "PR19A")
					(number "M20")
				)
				(pin power_in line
					(at 41.91 0 180)
					(length 7.62)
					(name "VCCIO1")
					(number "N13")
				)
				(pin bidirectional line
					(at 41.91 -88.9 180)
					(length 7.62)
					(name "PR28D")
					(number "N14")
				)
				(pin bidirectional line
					(at 41.91 -86.36 180)
					(length 7.62)
					(name "PR28C")
					(number "N15")
				)
				(pin bidirectional line
					(at 41.91 -60.96 180)
					(length 7.62)
					(name "PR25A")
					(number "N16")
				)
				(pin bidirectional line
					(at 41.91 -43.18 180)
					(length 7.62)
					(name "PR21B")
					(number "N17")
				)
				(pin bidirectional line
					(at 41.91 -40.64 180)
					(length 7.62)
					(name "PR21A")
					(number "N18")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 7.62)
					(name "PR20D")
					(number "N19")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 7.62)
					(name "PR20B")
					(number "N20")
				)
				(pin bidirectional line
					(at 41.91 -96.52 180)
					(length 7.62)
					(name "PR29C")
					(number "P15")
				)
				(pin bidirectional line
					(at 41.91 -83.82 180)
					(length 7.62)
					(name "PR28B")
					(number "P16")
				)
				(pin bidirectional line
					(at 41.91 -73.66 180)
					(length 7.62)
					(name "PR26B")
					(number "P17")
				)
				(pin bidirectional line
					(at 41.91 -50.8 180)
					(length 7.62)
					(name "PR24A")
					(number "P18")
				)
				(pin bidirectional line
					(at 41.91 -48.26 180)
					(length 7.62)
					(name "PR21D")
					(number "P19")
				)
				(pin bidirectional line
					(at 41.91 -45.72 180)
					(length 7.62)
					(name "PR21C")
					(number "P20")
				)
				(pin bidirectional line
					(at 41.91 -99.06 180)
					(length 7.62)
					(name "PR29D")
					(number "R16")
				)
				(pin bidirectional line
					(at 41.91 -91.44 180)
					(length 7.62)
					(name "PR29A")
					(number "R17")
				)
				(pin bidirectional line
					(at 41.91 -63.5 180)
					(length 7.62)
					(name "PR25B")
					(number "R19")
				)
				(pin bidirectional line
					(at 41.91 -53.34 180)
					(length 7.62)
					(name "PR24B")
					(number "R20")
				)
				(pin bidirectional line
					(at 41.91 -104.14 180)
					(length 7.62)
					(name "PR30B")
					(number "T17")
				)
				(pin bidirectional line
					(at 41.91 -76.2 180)
					(length 7.62)
					(name "PR27C")
					(number "T18")
				)
				(pin bidirectional line
					(at 41.91 -68.58 180)
					(length 7.62)
					(name "PR25D")
					(number "T19")
				)
				(pin bidirectional line
					(at 41.91 -66.04 180)
					(length 7.62)
					(name "PR25C")
					(number "T20")
				)
				(pin bidirectional line
					(at 41.91 -106.68 180)
					(length 7.62)
					(name "PR30C")
					(number "U17")
				)
				(pin bidirectional line
					(at 41.91 -93.98 180)
					(length 7.62)
					(name "PR29B")
					(number "U18")
				)
				(pin bidirectional line
					(at 41.91 -78.74 180)
					(length 7.62)
					(name "PR27D")
					(number "U19")
				)
				(pin bidirectional line
					(at 41.91 -71.12 180)
					(length 7.62)
					(name "PR26A")
					(number "U20")
				)
				(pin bidirectional line
					(at 41.91 -109.22 180)
					(length 7.62)
					(name "PR30D")
					(number "V17")
				)
				(pin bidirectional line
					(at 41.91 -101.6 180)
					(length 7.62)
					(name "PR30A")
					(number "V19")
				)
				(pin bidirectional line
					(at 41.91 -81.28 180)
					(length 7.62)
					(name "PR28A")
					(number "V20")
				)
			)
			(symbol "LCMXO3D-9400HC-5BG400C_3_1"
				(pin power_in line
					(at 41.91 0 180)
					(length 7.62)
					(name "VCCIO2")
					(number "N8")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO2")
					(number "N9")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO2")
					(number "N10")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO2")
					(number "N11")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO2")
					(number "N12")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 7.62)
					(name "PB7C")
					(number "P7")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 7.62)
					(name "PB10C")
					(number "P8")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 7.62)
					(name "PB16C")
					(number "P9")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 7.62)
					(name "PB22C")
					(number "P10")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 7.62)
					(name "PB29C")
					(number "P11")
				)
				(pin bidirectional line
					(at 41.91 -45.72 180)
					(length 7.62)
					(name "PB33C")
					(number "P12")
				)
				(pin bidirectional line
					(at 41.91 -66.04 180)
					(length 7.62)
					(name "PB38C")
					(number "P13")
				)
				(pin bidirectional line
					(at 41.91 -96.52 180)
					(length 7.62)
					(name "PB44C")
					(number "P14")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 7.62)
					(name "PB5C")
					(number "R6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 7.62)
					(name "PB7D")
					(number "R7")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 7.62)
					(name "PB10D")
					(number "R8")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 7.62)
					(name "PB16D")
					(number "R9")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 7.62)
					(name "PB22D")
					(number "R10")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 7.62)
					(name "PB29D")
					(number "R11")
				)
				(pin bidirectional line
					(at 41.91 -48.26 180)
					(length 7.62)
					(name "PB33D")
					(number "R12")
				)
				(pin bidirectional line
					(at 41.91 -68.58 180)
					(length 7.62)
					(name "PB38D")
					(number "R13")
				)
				(pin bidirectional line
					(at 41.91 -99.06 180)
					(length 7.62)
					(name "PB44D")
					(number "R14")
				)
				(pin bidirectional line
					(at 41.91 -109.22 180)
					(length 7.62)
					(name "PB46D")
					(number "R15")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 7.62)
					(name "PB5D")
					(number "T6")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 7.62)
					(name "PB13C")
					(number "T7")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 7.62)
					(name "PB13D")
					(number "T8")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 7.62)
					(name "PB19B")
					(number "T9")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 7.62)
					(name "PB27D")
					(number "T10")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 7.62)
					(name "PB32D")
					(number "T11")
				)
				(pin bidirectional line
					(at 41.91 -55.88 180)
					(length 7.62)
					(name "PB35C")
					(number "T12")
				)
				(pin bidirectional line
					(at 41.91 -58.42 180)
					(length 7.62)
					(name "PB35D")
					(number "T13")
				)
				(pin bidirectional line
					(at 41.91 -86.36 180)
					(length 7.62)
					(name "PB43C")
					(number "T14")
				)
				(pin bidirectional line
					(at 41.91 -106.68 180)
					(length 7.62)
					(name "PB46C")
					(number "T16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 7.62)
					(name "PB8D")
					(number "U6")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 7.62)
					(name "PB18D")
					(number "U9")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 7.62)
					(name "PB24C")
					(number "U10")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 7.62)
					(name "PB27C")
					(number "U11")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 7.62)
					(name "PB32C")
					(number "U12")
				)
				(pin bidirectional line
					(at 41.91 -73.66 180)
					(length 7.62)
					(name "PB41B")
					(number "U14")
				)
				(pin bidirectional line
					(at 41.91 -88.9 180)
					(length 7.62)
					(name "PB43D")
					(number "U15")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 7.62)
					(name "PB8C")
					(number "V6")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 7.62)
					(name "PB18C")
					(number "V8")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 7.62)
					(name "PB19A")
					(number "V9")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 7.62)
					(name "PB24D")
					(number "V10")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 7.62)
					(name "PB30C")
					(number "V12")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 7.62)
					(name "PB30D")
					(number "V13")
				)
				(pin bidirectional line
					(at 41.91 -71.12 180)
					(length 7.62)
					(name "PB41A")
					(number "V14")
				)
				(pin bidirectional line
					(at 41.91 -76.2 180)
					(length 7.62)
					(name "PB41C")
					(number "V15")
				)
				(pin bidirectional line
					(at 41.91 -78.74 180)
					(length 7.62)
					(name "PB41D")
					(number "V16")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 7.62)
					(name "PB5A")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 7.62)
					(name "PB7A")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 7.62)
					(name "PB8A")
					(number "W3")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 7.62)
					(name "PB10A")
					(number "W4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 7.62)
					(name "PB13A")
					(number "W5")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 7.62)
					(name "PB16A")
					(number "W6")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 7.62)
					(name "PB18A")
					(number "W7")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 7.62)
					(name "PB21A")
					(number "W8")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 7.62)
					(name "PB22A")
					(number "W9")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 7.62)
					(name "PB24B")
					(number "W10")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 7.62)
					(name "PB27B")
					(number "W11")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 7.62)
					(name "PB29B")
					(number "W12")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 7.62)
					(name "PB30B")
					(number "W13")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 7.62)
					(name "PB32B")
					(number "W14")
				)
				(pin bidirectional line
					(at 41.91 -43.18 180)
					(length 7.62)
					(name "PB33B")
					(number "W15")
				)
				(pin bidirectional line
					(at 41.91 -53.34 180)
					(length 7.62)
					(name "PB35B")
					(number "W16")
				)
				(pin bidirectional line
					(at 41.91 -63.5 180)
					(length 7.62)
					(name "PB38B")
					(number "W17")
				)
				(pin bidirectional line
					(at 41.91 -83.82 180)
					(length 7.62)
					(name "PB43B")
					(number "W18")
				)
				(pin bidirectional line
					(at 41.91 -93.98 180)
					(length 7.62)
					(name "PB44B")
					(number "W19")
				)
				(pin bidirectional line
					(at 41.91 -104.14 180)
					(length 7.62)
					(name "PB46B")
					(number "W20")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 7.62)
					(name "PB5B")
					(number "Y1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 7.62)
					(name "PB7B")
					(number "Y2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 7.62)
					(name "PB8B")
					(number "Y3")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 7.62)
					(name "PB10B")
					(number "Y4")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 7.62)
					(name "PB13B")
					(number "Y5")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 7.62)
					(name "PB16B")
					(number "Y6")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 7.62)
					(name "PB18B")
					(number "Y7")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 7.62)
					(name "PB21B")
					(number "Y8")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 7.62)
					(name "PB22B")
					(number "Y9")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 7.62)
					(name "PB24A")
					(number "Y10")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 7.62)
					(name "PB27A")
					(number "Y11")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 7.62)
					(name "PB29A")
					(number "Y12")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 7.62)
					(name "PB30A")
					(number "Y13")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 7.62)
					(name "PB32A")
					(number "Y14")
				)
				(pin bidirectional line
					(at 41.91 -40.64 180)
					(length 7.62)
					(name "PB33A")
					(number "Y15")
				)
				(pin bidirectional line
					(at 41.91 -50.8 180)
					(length 7.62)
					(name "PB35A")
					(number "Y16")
				)
				(pin bidirectional line
					(at 41.91 -60.96 180)
					(length 7.62)
					(name "PB38A")
					(number "Y17")
				)
				(pin bidirectional line
					(at 41.91 -81.28 180)
					(length 7.62)
					(name "PB43A")
					(number "Y18")
				)
				(pin bidirectional line
					(at 41.91 -91.44 180)
					(length 7.62)
					(name "PB44A")
					(number "Y19")
				)
				(pin bidirectional line
					(at 41.91 -101.6 180)
					(length 7.62)
					(name "PB46A")
					(number "Y20")
				)
			)
			(symbol "LCMXO3D-9400HC-5BG400C_4_1"
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 7.62)
					(name "PL20C")
					(number "M6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 7.62)
					(name "PL20D")
					(number "M7")
				)
				(pin power_in line
					(at 41.91 0 180)
					(length 7.62)
					(name "VCCIO3")
					(number "M8")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO3")
					(number "M9")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 7.62)
					(name "PL20A")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 7.62)
					(name "PL20B")
					(number "N4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 7.62)
					(name "PL26C")
					(number "N5")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 7.62)
					(name "PL26D")
					(number "N6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 7.62)
					(name "PL25A")
					(number "P3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 7.62)
					(name "PL25B")
					(number "P4")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 7.62)
					(name "PL29C")
					(number "P5")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 7.62)
					(name "PL29D")
					(number "P6")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 7.62)
					(name "PL21C")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 7.62)
					(name "PL21D")
					(number "R2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 7.62)
					(name "PL27C")
					(number "R3")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 7.62)
					(name "PL27D")
					(number "R4")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 7.62)
					(name "PL30B")
					(number "R5")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 7.62)
					(name "PL26A")
					(number "T1")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 7.62)
					(name "PL26B")
					(number "T2")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 7.62)
					(name "PL28A")
					(number "T3")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 7.62)
					(name "PL28B")
					(number "T4")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 7.62)
					(name "PL30A")
					(number "T5")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 7.62)
					(name "PL27A")
					(number "U1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 7.62)
					(name "PL27B")
					(number "U2")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 7.62)
					(name "PL30C")
					(number "U4")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 7.62)
					(name "PL30D")
					(number "U5")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 7.62)
					(name "PL28C")
					(number "V1")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 7.62)
					(name "PL28D")
					(number "V2")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 7.62)
					(name "PL29A")
					(number "V3")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 7.62)
					(name "PL29B")
					(number "V4")
				)
			)
			(symbol "LCMXO3D-9400HC-5BG400C_5_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 7.62)
					(name "PL14B")
					(number "K1")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 7.62)
					(name "PL14D")
					(number "K7")
				)
				(pin power_in line
					(at 41.91 0 180)
					(length 7.62)
					(name "VCCIO4")
					(number "K8")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO4")
					(number "K9")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 7.62)
					(name "PL16A")
					(number "L1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 7.62)
					(name "PL16B")
					(number "L2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 7.62)
					(name "PL16C")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 7.62)
					(name "PL16D")
					(number "L4")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 7.62)
					(name "PL18A")
					(number "L5")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 7.62)
					(name "PL18C")
					(number "L6")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 7.62)
					(name "PL18D")
					(number "L7")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 7.62)
					(name "PL17A")
					(number "M1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 7.62)
					(name "PL17B")
					(number "M2")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 7.62)
					(name "PL17C")
					(number "M3")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 7.62)
					(name "PL17D")
					(number "M4")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 7.62)
					(name "PL18B")
					(number "M5")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 7.62)
					(name "PL19A")
					(number "N1")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 7.62)
					(name "PL19B")
					(number "N2")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 7.62)
					(name "PL19C")
					(number "P1")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 7.62)
					(name "PL19D")
					(number "P2")
				)
			)
			(symbol "LCMXO3D-9400HC-5BG400C_6_1"
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 7.62)
					(name "PL3B")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 7.62)
					(name "PL3A")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 7.62)
					(name "PL2B")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 7.62)
					(name "PL2A")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 7.62)
					(name "PL4B")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 7.62)
					(name "PL4A")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 7.62)
					(name "PL7B")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 7.62)
					(name "PL7A")
					(number "E2")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 7.62)
					(name "PL3D")
					(number "E3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 7.62)
					(name "PL3C")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 7.62)
					(name "PL7D")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 7.62)
					(name "PL7C")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 7.62)
					(name "PL6B")
					(number "F3")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 7.62)
					(name "PL6A")
					(number "F4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 7.62)
					(name "PL4C")
					(number "F5")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 7.62)
					(name "PL2C")
					(number "F6")
				)
				(pin bidirectional line
					(at 41.91 -17.78 180)
					(length 7.62)
					(name "PL11B")
					(number "G1")
				)
				(pin bidirectional line
					(at 41.91 -15.24 180)
					(length 7.62)
					(name "PL11A")
					(number "G2")
				)
				(pin bidirectional line
					(at 41.91 -7.62 180)
					(length 7.62)
					(name "PL10B")
					(number "G3")
				)
				(pin bidirectional line
					(at 41.91 -5.08 180)
					(length 7.62)
					(name "PL10A")
					(number "G4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 7.62)
					(name "PL4D")
					(number "G5")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 7.62)
					(name "PL2D")
					(number "G6")
				)
				(pin bidirectional line
					(at 41.91 -27.94 180)
					(length 7.62)
					(name "PL12B")
					(number "H1")
				)
				(pin bidirectional line
					(at 41.91 -25.4 180)
					(length 7.62)
					(name "PL12A")
					(number "H2")
				)
				(pin bidirectional line
					(at 41.91 -10.16 180)
					(length 7.62)
					(name "PL10C")
					(number "H3")
				)
				(pin bidirectional line
					(at 41.91 -12.7 180)
					(length 7.62)
					(name "PL10D")
					(number "H4")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 7.62)
					(name "PL5C")
					(number "H6")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 7.62)
					(name "PL5D")
					(number "H7")
				)
				(pin bidirectional line
					(at 41.91 -38.1 180)
					(length 7.62)
					(name "PL13B")
					(number "J1")
				)
				(pin bidirectional line
					(at 41.91 -35.56 180)
					(length 7.62)
					(name "PL13A")
					(number "J2")
				)
				(pin bidirectional line
					(at 41.91 -33.02 180)
					(length 7.62)
					(name "PL12D")
					(number "J3")
				)
				(pin bidirectional line
					(at 41.91 -30.48 180)
					(length 7.62)
					(name "PL12C")
					(number "J4")
				)
				(pin bidirectional line
					(at 41.91 -22.86 180)
					(length 7.62)
					(name "PL11D")
					(number "J5")
				)
				(pin bidirectional line
					(at 41.91 -20.32 180)
					(length 7.62)
					(name "PL11C")
					(number "J6")
				)
				(pin power_in line
					(at 41.91 0 180)
					(length 7.62)
					(name "VCCIO5")
					(number "J7")
				)
				(pin passive line
					(at 41.91 0 180)
					(length 7.62)
					(hide yes)
					(name "VCCIO5")
					(number "J8")
				)
				(pin bidirectional line
					(at 41.91 -45.72 180)
					(length 7.62)
					(name "PL14A")
					(number "K2")
				)
				(pin bidirectional line
					(at 41.91 -43.18 180)
					(length 7.62)
					(name "PL13D")
					(number "K4")
				)
				(pin bidirectional line
					(at 41.91 -40.64 180)
					(length 7.62)
					(name "PL13C")
					(number "K5")
				)
				(pin bidirectional line
					(at 41.91 -48.26 180)
					(length 7.62)
					(name "PL14C")
					(number "K6")
				)
			)
			(embedded_fonts no)
		)
)
