(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "GNSS_LEA-M8T"
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 50.8 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "GNSS_LEA-M8T"
				(at 50.8 -15.24 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "GNSS_LEA-M8T"
				(at 50.8 -17.78 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://eu.mouser.com/datasheet/2/1025/NEO_LEA_M8T_FW3_DataSheet_UBX_15025193-3180171.pdf"
				(at 50.8 -20.32 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "RF receiver"
				(at 50.8 -27.94 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LEA-M8T-0"
				(at 50.8 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "u-blox"
				(at 50.8 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 50.8 -22.86 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 50.8 -25.4 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_fp_filters" "ublox*LEA*"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "GNSS_LEA-M8T_1_1"
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 2.54)
					(name "SDA/~{SPI_CS}")
					(number "1")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 2.54)
					(name "SCL/SPI_CLK")
					(number "2")
				)
				(pin output line
					(at 0 -15.24 0)
					(length 2.54)
					(name "TXD/SPI_MISO")
					(number "3")
				)
				(pin input line
					(at 0 -17.78 0)
					(length 2.54)
					(name "RXD/SPI_MOSI")
					(number "4")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 2.54)
					(name "D_SEL")
					(number "5")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 2.54)
					(name "VCC")
					(number "6")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "7")
				)
				(pin power_out line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "VCC_OUT")
					(number "8")
				)
				(pin no_connect line
					(at 25.4 -11.43 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "9")
				)
				(pin input line
					(at 0 -33.02 0)
					(length 2.54)
					(name "~{RESET}")
					(number "10")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 2.54)
					(name "V_BCKP")
					(number "11")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 2.54)
					(name "TP2/~{SAFEBOOT}")
					(number "12")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 2.54)
					(name "GND")
					(number "13")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "14")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "15")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 2.54)
					(name "RF_IN")
					(number "16")
				)
				(pin passive line
					(at 27.94 -38.1 180)
					(length 2.54)
					(hide yes)
					(name "GND")
					(number "17")
				)
				(pin power_out line
					(at 27.94 0 180)
					(length 2.54)
					(name "VCC_RF")
					(number "18")
				)
				(pin power_in line
					(at 0 0 0)
					(length 2.54)
					(name "V_ANT")
					(number "19")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 2.54)
					(name "EXTINT1")
					(number "20")
				)
				(pin no_connect line
					(at 25.4 -12.7 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "21")
				)
				(pin no_connect line
					(at 25.4 -8.89 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "22")
				)
				(pin no_connect line
					(at 25.4 -10.16 180)
					(length 2.54)
					(hide yes)
					(name "RESERVED")
					(number "23")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 2.54)
					(name "VDD_USB")
					(number "24")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 2.54)
					(name "USB_DM")
					(number "25")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 2.54)
					(name "USB_DP")
					(number "26")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 2.54)
					(name "EXTINT0")
					(number "27")
				)
				(pin output line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "TIMEPULSE")
					(number "28")
				)
			)
			(embedded_fonts no)
		)
)
