(footprint "FCCSP-256_14x14mm_Layout16x16_P0.8mm"
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(layer "F.Cu")
	(descr "Flip-Chip Chip-Scale Package, Low Profile")
	(property "Reference" "REF**"
		(at -7.49 -7.62 0)
		(layer "F.SilkS")
	)
	(property "Value" "FCCSP-256_14x14mm_Layout16x16_P0.8mm"
		(at -8 8.55 0)
		(layer "F.Fab")
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(stackup
		(layer "F.Cu")
		(layer "B.Cu")
		(layer "User.1")
		(layer "User.2")
		(layer "User.3")
		(layer "User.4")
		(layer "User.5")
		(layer "User.6")
		(layer "User.7")
		(layer "User.8")
		(layer "User.9")
	)
	(duplicate_pad_numbers_are_jumpers no)
	(fp_text user "${REFERENCE}"
		(at -8 10.55 0)
		(layer "F.Fab")
	)
	(fp_text user "Author: Antmicro"
		(at -8 11.749 0)
		(layer "F.Fab")
	)
	(fp_text user "License: Apache-2.0"
		(at -8 12.95 0)
		(layer "F.Fab")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "A1" smd circle
		(at -6 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A2" smd circle
		(at -5.2 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A3" smd circle
		(at -4.4 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A4" smd circle
		(at -3.6 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A5" smd circle
		(at -2.8 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A6" smd circle
		(at -2 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A7" smd circle
		(at -1.2 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A8" smd circle
		(at -0.4 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A9" smd circle
		(at 0.4 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A10" smd circle
		(at 1.2 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A11" smd circle
		(at 2 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A12" smd circle
		(at 2.8 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A13" smd circle
		(at 3.6 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A14" smd circle
		(at 4.4 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A15" smd circle
		(at 5.2 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "A16" smd circle
		(at 6 -6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B1" smd circle
		(at -6 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B2" smd circle
		(at -5.2 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B3" smd circle
		(at -4.4 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B4" smd circle
		(at -3.6 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B5" smd circle
		(at -2.8 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B6" smd circle
		(at -2 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B7" smd circle
		(at -1.2 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B8" smd circle
		(at -0.4 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B9" smd circle
		(at 0.4 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B10" smd circle
		(at 1.2 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B11" smd circle
		(at 2 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B12" smd circle
		(at 2.8 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B13" smd circle
		(at 3.6 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B14" smd circle
		(at 4.4 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B15" smd circle
		(at 5.2 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "B16" smd circle
		(at 6 -5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C1" smd circle
		(at -6 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C2" smd circle
		(at -5.2 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C3" smd circle
		(at -4.4 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C4" smd circle
		(at -3.6 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C5" smd circle
		(at -2.8 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C6" smd circle
		(at -2 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C7" smd circle
		(at -1.2 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C8" smd circle
		(at -0.4 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C9" smd circle
		(at 0.4 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C10" smd circle
		(at 1.2 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C11" smd circle
		(at 2 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C12" smd circle
		(at 2.8 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C13" smd circle
		(at 3.6 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C14" smd circle
		(at 4.4 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C15" smd circle
		(at 5.2 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "C16" smd circle
		(at 6 -4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D1" smd circle
		(at -6 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D2" smd circle
		(at -5.2 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D3" smd circle
		(at -4.4 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D4" smd circle
		(at -3.6 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D5" smd circle
		(at -2.8 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D6" smd circle
		(at -2 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D7" smd circle
		(at -1.2 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D8" smd circle
		(at -0.4 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D9" smd circle
		(at 0.4 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D10" smd circle
		(at 1.2 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D11" smd circle
		(at 2 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D12" smd circle
		(at 2.8 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D13" smd circle
		(at 3.6 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D14" smd circle
		(at 4.4 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D15" smd circle
		(at 5.2 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "D16" smd circle
		(at 6 -3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E1" smd circle
		(at -6 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E2" smd circle
		(at -5.2 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E3" smd circle
		(at -4.4 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E4" smd circle
		(at -3.6 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E5" smd circle
		(at -2.8 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E6" smd circle
		(at -2 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E7" smd circle
		(at -1.2 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E8" smd circle
		(at -0.4 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E9" smd circle
		(at 0.4 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E10" smd circle
		(at 1.2 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E11" smd circle
		(at 2 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E12" smd circle
		(at 2.8 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E13" smd circle
		(at 3.6 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E14" smd circle
		(at 4.4 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E15" smd circle
		(at 5.2 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "E16" smd circle
		(at 6 -2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F1" smd circle
		(at -6 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F2" smd circle
		(at -5.2 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F3" smd circle
		(at -4.4 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F4" smd circle
		(at -3.6 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F5" smd circle
		(at -2.8 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F6" smd circle
		(at -2 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F7" smd circle
		(at -1.2 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F8" smd circle
		(at -0.4 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F9" smd circle
		(at 0.4 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F10" smd circle
		(at 1.2 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F11" smd circle
		(at 2 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F12" smd circle
		(at 2.8 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F13" smd circle
		(at 3.6 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F14" smd circle
		(at 4.4 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F15" smd circle
		(at 5.2 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "F16" smd circle
		(at 6 -2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G1" smd circle
		(at -6 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G2" smd circle
		(at -5.2 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G3" smd circle
		(at -4.4 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G4" smd circle
		(at -3.6 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G5" smd circle
		(at -2.8 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G6" smd circle
		(at -2 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G7" smd circle
		(at -1.2 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G8" smd circle
		(at -0.4 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G9" smd circle
		(at 0.4 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G10" smd circle
		(at 1.2 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G11" smd circle
		(at 2 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G12" smd circle
		(at 2.8 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G13" smd circle
		(at 3.6 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G14" smd circle
		(at 4.4 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G15" smd circle
		(at 5.2 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "G16" smd circle
		(at 6 -1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H1" smd circle
		(at -6 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H2" smd circle
		(at -5.2 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H3" smd circle
		(at -4.4 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H4" smd circle
		(at -3.6 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H5" smd circle
		(at -2.8 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H6" smd circle
		(at -2 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H7" smd circle
		(at -1.2 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H8" smd circle
		(at -0.4 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H9" smd circle
		(at 0.4 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H10" smd circle
		(at 1.2 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H11" smd circle
		(at 2 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H12" smd circle
		(at 2.8 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H13" smd circle
		(at 3.6 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H14" smd circle
		(at 4.4 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H15" smd circle
		(at 5.2 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "H16" smd circle
		(at 6 -0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J1" smd circle
		(at -6 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J2" smd circle
		(at -5.2 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J3" smd circle
		(at -4.4 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J4" smd circle
		(at -3.6 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J5" smd circle
		(at -2.8 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J6" smd circle
		(at -2 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J7" smd circle
		(at -1.2 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J8" smd circle
		(at -0.4 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J9" smd circle
		(at 0.4 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J10" smd circle
		(at 1.2 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J11" smd circle
		(at 2 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J12" smd circle
		(at 2.8 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J13" smd circle
		(at 3.6 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J14" smd circle
		(at 4.4 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J15" smd circle
		(at 5.2 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "J16" smd circle
		(at 6 0.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K1" smd circle
		(at -6 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K2" smd circle
		(at -5.2 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K3" smd circle
		(at -4.4 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K4" smd circle
		(at -3.6 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K5" smd circle
		(at -2.8 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K6" smd circle
		(at -2 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K7" smd circle
		(at -1.2 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K8" smd circle
		(at -0.4 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K9" smd circle
		(at 0.4 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K10" smd circle
		(at 1.2 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K11" smd circle
		(at 2 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K12" smd circle
		(at 2.8 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K13" smd circle
		(at 3.6 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K14" smd circle
		(at 4.4 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K15" smd circle
		(at 5.2 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "K16" smd circle
		(at 6 1.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L1" smd circle
		(at -6 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L2" smd circle
		(at -5.2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L3" smd circle
		(at -4.4 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L4" smd circle
		(at -3.6 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L5" smd circle
		(at -2.8 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L6" smd circle
		(at -2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L7" smd circle
		(at -1.2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L8" smd circle
		(at -0.4 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L9" smd circle
		(at 0.4 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L10" smd circle
		(at 1.2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L11" smd circle
		(at 2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L12" smd circle
		(at 2.8 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L13" smd circle
		(at 3.6 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L14" smd circle
		(at 4.4 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L15" smd circle
		(at 5.2 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "L16" smd circle
		(at 6 2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M1" smd circle
		(at -6 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M2" smd circle
		(at -5.2 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M3" smd circle
		(at -4.4 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M4" smd circle
		(at -3.6 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M5" smd circle
		(at -2.8 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M6" smd circle
		(at -2 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M7" smd circle
		(at -1.2 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M8" smd circle
		(at -0.4 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M9" smd circle
		(at 0.4 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M10" smd circle
		(at 1.2 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M11" smd circle
		(at 2 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M12" smd circle
		(at 2.8 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M13" smd circle
		(at 3.6 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M14" smd circle
		(at 4.4 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M15" smd circle
		(at 5.2 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "M16" smd circle
		(at 6 2.8)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N1" smd circle
		(at -6 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N2" smd circle
		(at -5.2 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N3" smd circle
		(at -4.4 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N4" smd circle
		(at -3.6 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N5" smd circle
		(at -2.8 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N6" smd circle
		(at -2 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N7" smd circle
		(at -1.2 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N8" smd circle
		(at -0.4 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N9" smd circle
		(at 0.4 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N10" smd circle
		(at 1.2 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N11" smd circle
		(at 2 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N12" smd circle
		(at 2.8 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N13" smd circle
		(at 3.6 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N14" smd circle
		(at 4.4 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N15" smd circle
		(at 5.2 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "N16" smd circle
		(at 6 3.6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P1" smd circle
		(at -6 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P2" smd circle
		(at -5.2 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P3" smd circle
		(at -4.4 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P4" smd circle
		(at -3.6 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P5" smd circle
		(at -2.8 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P6" smd circle
		(at -2 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P7" smd circle
		(at -1.2 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P8" smd circle
		(at -0.4 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P9" smd circle
		(at 0.4 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P10" smd circle
		(at 1.2 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P11" smd circle
		(at 2 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P12" smd circle
		(at 2.8 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P13" smd circle
		(at 3.6 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P14" smd circle
		(at 4.4 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P15" smd circle
		(at 5.2 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "P16" smd circle
		(at 6 4.4)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R1" smd circle
		(at -6 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R2" smd circle
		(at -5.2 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R3" smd circle
		(at -4.4 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R4" smd circle
		(at -3.6 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R5" smd circle
		(at -2.8 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R6" smd circle
		(at -2 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R7" smd circle
		(at -1.2 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R8" smd circle
		(at -0.4 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R9" smd circle
		(at 0.4 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R10" smd circle
		(at 1.2 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R11" smd circle
		(at 2 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R12" smd circle
		(at 2.8 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R13" smd circle
		(at 3.6 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R14" smd circle
		(at 4.4 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R15" smd circle
		(at 5.2 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "R16" smd circle
		(at 6 5.2)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T1" smd circle
		(at -6 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T2" smd circle
		(at -5.2 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T3" smd circle
		(at -4.4 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T4" smd circle
		(at -3.6 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T5" smd circle
		(at -2.8 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T6" smd circle
		(at -2 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T7" smd circle
		(at -1.2 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T8" smd circle
		(at -0.4 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T9" smd circle
		(at 0.4 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T10" smd circle
		(at 1.2 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T11" smd circle
		(at 2 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T12" smd circle
		(at 2.8 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T13" smd circle
		(at 3.6 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T14" smd circle
		(at 4.4 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T15" smd circle
		(at 5.2 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(pad "T16" smd circle
		(at 6 6)
		(size 0.35 0.35)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(solder_mask_margin 0.025)
	)
	(embedded_fonts no)
	(model "antmicro_lfcpnx_100_8cbg256c.glb"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
