(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "ECP5_LFE5UM5G-85"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 77.47 -3.81 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "ECP5_LFE5UM5G-85"
				(at 77.47 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "ECP5_LFE5UM5G-85"
				(at 77.47 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.latticesemi.com/-/media/LatticeSemi/Documents/DataSheets/ECP5/FPGA-DS-02012-2-2-ECP5-ECP5G-Family-Data-Sheet.ashx?document_id=50461"
				(at 77.47 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "ECP5-5G Field Programmable Gate Array"
				(at 77.47 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LFE5UM5G-85F-8BG756C"
				(at 77.47 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lattice Semiconductor"
				(at 77.47 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 77.47 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 77.47 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "SMT, FPGA, IC"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "ECP5_LFE5UM5G-85_1_1"
				(pin power_in line
					(at 38.1 -40.64 180)
					(length 5.08)
					(name "GND")
					(number "AA11")
				)
				(pin power_in line
					(at 0 0 0)
					(length 5.08)
					(name "VCC")
					(number "AA12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "AA21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AA22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB11")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AB22")
				)
				(pin no_connect line
					(at 33.02 -21.59 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC4")
				)
				(pin power_in line
					(at 0 -8.89 0)
					(length 5.08)
					(name "VCCAUX")
					(number "AC11")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC12")
				)
				(pin power_in line
					(at 38.1 -2.54 180)
					(length 5.08)
					(name "VCCHTX0_D0CH0")
					(number "AC13")
				)
				(pin power_in line
					(at 38.1 -7.62 180)
					(length 5.08)
					(name "VCCHRX0_D0CH0")
					(number "AC14")
				)
				(pin power_in line
					(at 38.1 -17.78 180)
					(length 5.08)
					(name "VCCHRX1_D0CH1")
					(number "AC15")
				)
				(pin power_in line
					(at 38.1 -12.7 180)
					(length 5.08)
					(name "VCCHTX1_D0CH1")
					(number "AC16")
				)
				(pin power_in line
					(at 38.1 0 180)
					(length 5.08)
					(name "VCCHTX0_D1CH0")
					(number "AC17")
				)
				(pin power_in line
					(at 38.1 -5.08 180)
					(length 5.08)
					(name "VCCHRX0_D1CH0")
					(number "AC18")
				)
				(pin power_in line
					(at 38.1 -15.24 180)
					(length 5.08)
					(name "VCCHRX1_D1CH1")
					(number "AC19")
				)
				(pin power_in line
					(at 38.1 -10.16 180)
					(length 5.08)
					(name "VCCHTX1_D1CH1")
					(number "AC20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AC21")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "AC22")
				)
				(pin no_connect line
					(at 33.02 -20.32 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AC29")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD28")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AD31")
				)
				(pin no_connect line
					(at 33.02 -24.13 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AE7")
				)
				(pin no_connect line
					(at 33.02 -22.86 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AE26")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF11")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF20")
				)
				(pin power_in line
					(at 0 -5.08 0)
					(length 5.08)
					(name "VCCA1")
					(number "AF22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AF23")
				)
				(pin no_connect line
					(at 33.02 -25.4 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AG2")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCA0")
					(number "AG9")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG11")
				)
				(pin power_in line
					(at 0 -2.54 0)
					(length 5.08)
					(name "VCCA0")
					(number "AG12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AG19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG20")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AG22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AG23")
				)
				(pin no_connect line
					(at 33.02 -26.67 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AG24")
				)
				(pin no_connect line
					(at 33.02 -27.94 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "AG31")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH7")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCA0")
					(number "AH9")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCA0")
					(number "AH12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AH19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH20")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AH22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH23")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH24")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH25")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH26")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH29")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AH31")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ7")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ8")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCA0")
					(number "AJ9")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCA0")
					(number "AJ10")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ11")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCA0")
					(number "AJ12")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 5.08)
					(hide yes)
					(name "VCCA0")
					(number "AJ13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ14")
				)
				(pin power_in line
					(at 0 -11.43 0)
					(length 5.08)
					(name "VCCAUXA0")
					(number "AJ15")
				)
				(pin passive line
					(at 0 -11.43 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUXA0")
					(number "AJ16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ17")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AJ18")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AJ19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ20")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AJ21")
				)
				(pin passive line
					(at 0 -5.08 0)
					(length 5.08)
					(hide yes)
					(name "VCCA1")
					(number "AJ22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ23")
				)
				(pin power_in line
					(at 0 -13.97 0)
					(length 5.08)
					(name "VCCAUXA1")
					(number "AJ24")
				)
				(pin passive line
					(at 0 -13.97 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUXA1")
					(number "AJ25")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AJ26")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK7")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK8")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK11")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK14")
				)
				(pin no_connect line
					(at 5.08 -34.29 0)
					(length 5.08)
					(hide yes)
					(name "RESERVED")
					(number "AK15")
				)
				(pin no_connect line
					(at 5.08 -35.56 0)
					(length 5.08)
					(hide yes)
					(name "RESERVED")
					(number "AK16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK23")
				)
				(pin no_connect line
					(at 5.08 -36.83 0)
					(length 5.08)
					(hide yes)
					(name "RESERVED")
					(number "AK24")
				)
				(pin no_connect line
					(at 5.08 -38.1 0)
					(length 5.08)
					(hide yes)
					(name "RESERVED")
					(number "AK25")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AK26")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL7")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL8")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL9")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL11")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL23")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL24")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL26")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL29")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AL31")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM7")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "AM26")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B9")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B24")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B28")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "B31")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin no_connect line
					(at 33.02 -30.48 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E7")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E9")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E24")
				)
				(pin no_connect line
					(at 33.02 -29.21 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "E26")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E28")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "E31")
				)
				(pin no_connect line
					(at 5.08 -31.75 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G9")
				)
				(pin no_connect line
					(at 33.02 -31.75 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G10")
				)
				(pin no_connect line
					(at 33.02 -33.02 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G11")
				)
				(pin no_connect line
					(at 33.02 -34.29 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G14")
				)
				(pin no_connect line
					(at 5.08 -21.59 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G15")
				)
				(pin no_connect line
					(at 5.08 -22.86 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G16")
				)
				(pin no_connect line
					(at 5.08 -24.13 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G17")
				)
				(pin no_connect line
					(at 5.08 -25.4 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G18")
				)
				(pin no_connect line
					(at 5.08 -26.67 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G19")
				)
				(pin no_connect line
					(at 5.08 -27.94 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G22")
				)
				(pin no_connect line
					(at 5.08 -29.21 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G23")
				)
				(pin no_connect line
					(at 5.08 -30.48 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "G24")
				)
				(pin no_connect line
					(at 5.08 -17.78 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H4")
				)
				(pin no_connect line
					(at 5.08 -16.51 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "H29")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J28")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "J31")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K10")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K11")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "K13")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "K20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "K23")
				)
				(pin no_connect line
					(at 5.08 -20.32 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L10")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L11")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L20")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "L23")
				)
				(pin no_connect line
					(at 5.08 -19.05 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "L28")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M12")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M13")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M14")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M15")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M16")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M17")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M18")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M19")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "M21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "M22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N5")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "N10")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "N12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "N21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N22")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "N23")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N28")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "N31")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "P12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "P21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "P22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R2")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "R12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "R21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R28")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "R31")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "T12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "T21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "T22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "U12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "U21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "U22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V2")
				)
				(pin no_connect line
					(at 33.02 -35.56 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V3")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V5")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "V12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "V21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V22")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V28")
				)
				(pin no_connect line
					(at 33.02 -36.83 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "V30")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "V31")
				)
				(pin no_connect line
					(at 5.08 -33.02 0)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W6")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "W12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "W21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "W22")
				)
				(pin no_connect line
					(at 33.02 -38.1 180)
					(length 5.08)
					(hide yes)
					(name "NC")
					(number "W27")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y2")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "Y10")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y11")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "Y12")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y13")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y14")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y15")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y16")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y17")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y18")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y19")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y20")
				)
				(pin passive line
					(at 0 0 0)
					(length 5.08)
					(hide yes)
					(name "VCC")
					(number "Y21")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y22")
				)
				(pin passive line
					(at 0 -8.89 0)
					(length 5.08)
					(hide yes)
					(name "VCCAUX")
					(number "Y23")
				)
				(pin passive line
					(at 38.1 -40.64 180)
					(length 5.08)
					(hide yes)
					(name "GND")
					(number "Y31")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_2_1"
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "PT6A")
					(number "A2")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "PT6B")
					(number "A3")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "PT9A")
					(number "A4")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "PT9B")
					(number "A5")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PT13B")
					(number "A7")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PT20B")
					(number "A8")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PT24B")
					(number "A9")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PT31B")
					(number "A10")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PT38B")
					(number "A11")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PT42B")
					(number "A13")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PT49B")
					(number "A14")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PT54B")
					(number "A15")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PT60B")
					(number "A16")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PT63A")
					(number "A17")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "PT4A")
					(number "B3")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "PT4B")
					(number "B4")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PT13A")
					(number "B7")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PT20A")
					(number "B8")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PT31A")
					(number "B10")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PT38A")
					(number "B11")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PT49A")
					(number "B14")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PT60A")
					(number "B16")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PT63B")
					(number "B17")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "PT11B")
					(number "C7")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PT18B")
					(number "C8")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PT24A")
					(number "C9")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PT29B")
					(number "C10")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PT36B")
					(number "C11")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PT42A")
					(number "C13")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PT47B")
					(number "C14")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PT54A")
					(number "C15")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PT58B")
					(number "C16")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PT65A")
					(number "C17")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "PT11A")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PT18A")
					(number "D8")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PT22B")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PT29A")
					(number "D10")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PT36A")
					(number "D11")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PT40B")
					(number "D13")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PT47A")
					(number "D14")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PT51B")
					(number "D15")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PT58A")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PT65B")
					(number "D17")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PT15B")
					(number "E8")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PT27B")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PT33B")
					(number "E11")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PT45B")
					(number "E14")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PT56B")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PT15A")
					(number "F8")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PT22A")
					(number "F9")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PT27A")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PT33A")
					(number "F11")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PT40A")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PT45A")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PT51A")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PT56A")
					(number "F16")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 5.08)
					(name "VCCIO0")
					(number "K12")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO0")
					(number "K14")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO0")
					(number "K15")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO0")
					(number "K16")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_3_1"
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PT71A")
					(number "A18")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PT76A")
					(number "A19")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PT83A")
					(number "A20")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PT87A")
					(number "A22")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PT94A")
					(number "A23")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PT101A")
					(number "A24")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PT105A")
					(number "A25")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PT112A")
					(number "A26")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PT116A")
					(number "A28")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PT116B")
					(number "A29")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PT119A")
					(number "A30")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PT119B")
					(number "A31")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PT76B")
					(number "B19")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PT87B")
					(number "B22")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PT94B")
					(number "B23")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PT105B")
					(number "B25")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PT112B")
					(number "B26")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PT121A")
					(number "B29")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PT121B")
					(number "B30")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PT71B")
					(number "C18")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PT78A")
					(number "C19")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PT83B")
					(number "C20")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PT89A")
					(number "C22")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PT96A")
					(number "C23")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PT101B")
					(number "C24")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PT107A")
					(number "C25")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PT114A")
					(number "C26")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PT74A")
					(number "D18")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PT78B")
					(number "D19")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PT85A")
					(number "D20")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PT89B")
					(number "D22")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PT96B")
					(number "D23")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PT103A")
					(number "D24")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PT107B")
					(number "D25")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PT114B")
					(number "D26")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PT69A")
					(number "E17")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PT80A")
					(number "E19")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PT92A")
					(number "E22")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PT98A")
					(number "E23")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PT110A")
					(number "E25")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PT69B")
					(number "F17")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PT74B")
					(number "F18")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PT80B")
					(number "F19")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PT85B")
					(number "F20")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PT92B")
					(number "F22")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PT98B")
					(number "F23")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PT103B")
					(number "F24")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PT110B")
					(number "F25")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 5.08)
					(name "VCCIO1")
					(number "K17")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO1")
					(number "K18")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO1")
					(number "K19")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO1")
					(number "K21")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_4_1"
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PR17A")
					(number "B32")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PR11A")
					(number "C28")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PR11C")
					(number "C29")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PR11D")
					(number "C30")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PR17B")
					(number "C31")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PR20C")
					(number "C32")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PR11B")
					(number "D28")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PR14A")
					(number "D29")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PR17C")
					(number "D30")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PR17D")
					(number "D31")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PR20D")
					(number "D32")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PR14B")
					(number "E29")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PR20B")
					(number "E30")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PR23B")
					(number "E32")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PR14D")
					(number "F28")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PR14C")
					(number "F29")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PR20A")
					(number "F30")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PR23A")
					(number "F31")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PR23C")
					(number "F32")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PR35A")
					(number "H27")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PR35B")
					(number "H28")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PR26B")
					(number "H30")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PR26A")
					(number "H31")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PR23D")
					(number "H32")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PR35C")
					(number "J26")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PR35D")
					(number "J27")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PR32C")
					(number "J29")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PR26C")
					(number "J30")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PR29B")
					(number "J32")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PR38B")
					(number "K26")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PR38A")
					(number "K27")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PR38C")
					(number "K28")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PR32D")
					(number "K29")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PR26D")
					(number "K30")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PR29A")
					(number "K31")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PR29C")
					(number "K32")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PR41C")
					(number "L26")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PR41D")
					(number "L27")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PR38D")
					(number "L29")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PR32B")
					(number "L30")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PR32A")
					(number "L31")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PR29D")
					(number "L32")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 5.08)
					(name "VCCIO2")
					(number "M23")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PR44B")
					(number "N26")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PR44A")
					(number "N27")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PR41B")
					(number "N29")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PR41A")
					(number "N30")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO2")
					(number "P23")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PR44D")
					(number "P26")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PR44C")
					(number "P27")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO2")
					(number "R23")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO2")
					(number "T23")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_5_1"
				(pin power_in line
					(at 27.94 0 180)
					(length 5.08)
					(name "VCCIO3")
					(number "AA23")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PR74C")
					(number "AB26")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PR77B")
					(number "AB27")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PR77A")
					(number "AB28")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PR83B")
					(number "AB29")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PR83A")
					(number "AB30")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PR89B")
					(number "AB31")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PR92A")
					(number "AB32")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PR77C")
					(number "AC26")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PR74D")
					(number "AC27")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PR83C")
					(number "AC28")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PR89A")
					(number "AC30")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PR89C")
					(number "AC31")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PR92B")
					(number "AC32")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PR77D")
					(number "AD26")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PR80A")
					(number "AD27")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PR83D")
					(number "AD29")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PR86C")
					(number "AD30")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PR92C")
					(number "AD32")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PR80B")
					(number "AE27")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PR80C")
					(number "AE28")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PR80D")
					(number "AE29")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PR86D")
					(number "AE30")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PR89D")
					(number "AE31")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PR92D")
					(number "AE32")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PR62A")
					(number "N32")
				)
				(pin bidirectional line
					(at 0 -160.02 0)
					(length 5.08)
					(name "PR47A")
					(number "P28")
				)
				(pin bidirectional line
					(at 0 -154.94 0)
					(length 5.08)
					(name "PR47B")
					(number "P29")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PR59B")
					(number "P30")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PR59A")
					(number "P31")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PR62B")
					(number "P32")
				)
				(pin bidirectional line
					(at 0 -157.48 0)
					(length 5.08)
					(name "PR47C")
					(number "R26")
				)
				(pin bidirectional line
					(at 0 -149.86 0)
					(length 5.08)
					(name "PR50A")
					(number "R27")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "PR53A")
					(number "R29")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PR59C")
					(number "R30")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PR65A")
					(number "R32")
				)
				(pin bidirectional line
					(at 0 -152.4 0)
					(length 5.08)
					(name "PR47D")
					(number "T26")
				)
				(pin bidirectional line
					(at 0 -144.78 0)
					(length 5.08)
					(name "PR50B")
					(number "T27")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "PR53B")
					(number "T28")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "PR53C")
					(number "T29")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PR59D")
					(number "T30")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PR65B")
					(number "T31")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PR68A")
					(number "T32")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO3")
					(number "U23")
				)
				(pin bidirectional line
					(at 0 -142.24 0)
					(length 5.08)
					(name "PR50D")
					(number "U26")
				)
				(pin bidirectional line
					(at 0 -147.32 0)
					(length 5.08)
					(name "PR50C")
					(number "U27")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "PR53D")
					(number "U28")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "PR56A")
					(number "U29")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PR62D")
					(number "U30")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PR62C")
					(number "U31")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PR68B")
					(number "U32")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO3")
					(number "V23")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "PR56D")
					(number "V26")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "PR56C")
					(number "V27")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "PR56B")
					(number "V29")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PR68C")
					(number "V32")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO3")
					(number "W23")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PR71D")
					(number "W28")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PR74B")
					(number "W29")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PR65C")
					(number "W30")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PR86A")
					(number "W31")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PR68D")
					(number "W32")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PR71A")
					(number "Y26")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PR71B")
					(number "Y27")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PR71C")
					(number "Y28")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PR74A")
					(number "Y29")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PR65D")
					(number "Y30")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PR86B")
					(number "Y32")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_6_1"
				(pin power_in line
					(at 27.94 0 180)
					(length 5.08)
					(name "VCCIO4")
					(number "AB23")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO4")
					(number "AC23")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PB110A")
					(number "AG28")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PB110B")
					(number "AG29")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PB114B")
					(number "AG30")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PB119B")
					(number "AG32")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PB112B")
					(number "AH28")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PB114A")
					(number "AH30")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PB119A")
					(number "AH32")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PB112A")
					(number "AJ28")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PB121A")
					(number "AJ29")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PB121B")
					(number "AJ30")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PB105B")
					(number "AJ31")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PB101B")
					(number "AJ32")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PB98B")
					(number "AK28")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PB116A")
					(number "AK29")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PB116B")
					(number "AK30")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PB105A")
					(number "AK31")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PB101A")
					(number "AK32")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PB98A")
					(number "AL28")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PB103B")
					(number "AL30")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PB107B")
					(number "AL32")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PB96A")
					(number "AM28")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PB96B")
					(number "AM29")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PB103A")
					(number "AM30")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PB107A")
					(number "AM31")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_7_1"
				(pin power_in line
					(at 27.94 0 180)
					(length 5.08)
					(name "VCCIO6")
					(number "AA10")
				)
				(pin bidirectional line
					(at 0 -152.4 0)
					(length 5.08)
					(name "PL92A")
					(number "AB1")
				)
				(pin bidirectional line
					(at 0 -147.32 0)
					(length 5.08)
					(name "PL89B")
					(number "AB2")
				)
				(pin bidirectional line
					(at 0 -121.92 0)
					(length 5.08)
					(name "PL83A")
					(number "AB3")
				)
				(pin bidirectional line
					(at 0 -127 0)
					(length 5.08)
					(name "PL83B")
					(number "AB4")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PL77A")
					(number "AB5")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PL77B")
					(number "AB6")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PL74C")
					(number "AB7")
				)
				(pin bidirectional line
					(at 0 -154.94 0)
					(length 5.08)
					(name "PL92B")
					(number "AC1")
				)
				(pin bidirectional line
					(at 0 -144.78 0)
					(length 5.08)
					(name "PL89C")
					(number "AC2")
				)
				(pin bidirectional line
					(at 0 -142.24 0)
					(length 5.08)
					(name "PL89A")
					(number "AC3")
				)
				(pin bidirectional line
					(at 0 -124.46 0)
					(length 5.08)
					(name "PL83C")
					(number "AC5")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PL74D")
					(number "AC6")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PL77C")
					(number "AC7")
				)
				(pin bidirectional line
					(at 0 -157.48 0)
					(length 5.08)
					(name "PL92C")
					(number "AD1")
				)
				(pin bidirectional line
					(at 0 -134.62 0)
					(length 5.08)
					(name "PL86C")
					(number "AD3")
				)
				(pin bidirectional line
					(at 0 -129.54 0)
					(length 5.08)
					(name "PL83D")
					(number "AD4")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PL80A")
					(number "AD6")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PL77D")
					(number "AD7")
				)
				(pin bidirectional line
					(at 0 -160.02 0)
					(length 5.08)
					(name "PL92D")
					(number "AE1")
				)
				(pin bidirectional line
					(at 0 -149.86 0)
					(length 5.08)
					(name "PL89D")
					(number "AE2")
				)
				(pin bidirectional line
					(at 0 -139.7 0)
					(length 5.08)
					(name "PL86D")
					(number "AE3")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PL80D")
					(number "AE4")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PL80C")
					(number "AE5")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PL80B")
					(number "AE6")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PL62A")
					(number "N1")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PL62B")
					(number "P1")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PL59A")
					(number "P2")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PL59B")
					(number "P3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PL47B")
					(number "P4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PL47A")
					(number "P5")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PL65A")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PL59C")
					(number "R3")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PL53A")
					(number "R4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PL50A")
					(number "R6")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PL47C")
					(number "R7")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PL68A")
					(number "T1")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PL65B")
					(number "T2")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PL59D")
					(number "T3")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PL53C")
					(number "T4")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PL53B")
					(number "T5")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PL50B")
					(number "T6")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PL47D")
					(number "T7")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PL68B")
					(number "U1")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PL62C")
					(number "U2")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PL62D")
					(number "U3")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PL56A")
					(number "U4")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PL53D")
					(number "U5")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PL50C")
					(number "U6")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PL50D")
					(number "U7")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO6")
					(number "U10")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PL68C")
					(number "V1")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PL56B")
					(number "V4")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PL56C")
					(number "V6")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PL56D")
					(number "V7")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO6")
					(number "V10")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PL68D")
					(number "W1")
				)
				(pin bidirectional line
					(at 0 -132.08 0)
					(length 5.08)
					(name "PL86A")
					(number "W2")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PL65C")
					(number "W3")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PL74B")
					(number "W4")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PL71D")
					(number "W5")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO6")
					(number "W10")
				)
				(pin bidirectional line
					(at 0 -137.16 0)
					(length 5.08)
					(name "PL86B")
					(number "Y1")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PL65D")
					(number "Y3")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PL74A")
					(number "Y4")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PL71C")
					(number "Y5")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PL71B")
					(number "Y6")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PL71A")
					(number "Y7")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_8_1"
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PL17A")
					(number "B1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "PL20C")
					(number "C1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PL17B")
					(number "C2")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PL11D")
					(number "C3")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PL11C")
					(number "C4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PL11A")
					(number "C5")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PL20D")
					(number "D1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PL17D")
					(number "D2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PL17C")
					(number "D3")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PL14A")
					(number "D4")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PL11B")
					(number "D5")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "PL23B")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "PL20B")
					(number "E3")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PL14B")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "PL23C")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "PL23A")
					(number "F2")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PL20A")
					(number "F3")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PL14C")
					(number "F4")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PL14D")
					(number "F5")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "PL23D")
					(number "H1")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 5.08)
					(name "PL26A")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 5.08)
					(name "PL26B")
					(number "H3")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 5.08)
					(name "PL35B")
					(number "H5")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 5.08)
					(name "PL35A")
					(number "H6")
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 5.08)
					(name "PL29B")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 5.08)
					(name "PL26C")
					(number "J3")
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 5.08)
					(name "PL32C")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 5.08)
					(name "PL35D")
					(number "J6")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 5.08)
					(name "PL35C")
					(number "J7")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 5.08)
					(name "PL29C")
					(number "K1")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 5.08)
					(name "PL29A")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 5.08)
					(name "PL26D")
					(number "K3")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 5.08)
					(name "PL32D")
					(number "K4")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 5.08)
					(name "PL38C")
					(number "K5")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 5.08)
					(name "PL38A")
					(number "K6")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 5.08)
					(name "PL38B")
					(number "K7")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 5.08)
					(name "PL29D")
					(number "L1")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 5.08)
					(name "PL32A")
					(number "L2")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 5.08)
					(name "PL32B")
					(number "L3")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 5.08)
					(name "PL38D")
					(number "L4")
				)
				(pin bidirectional line
					(at 0 -109.22 0)
					(length 5.08)
					(name "PL41D")
					(number "L6")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 5.08)
					(name "PL41C")
					(number "L7")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 5.08)
					(name "VCCIO7")
					(number "M10")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 5.08)
					(name "PL41A")
					(number "N3")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 5.08)
					(name "PL41B")
					(number "N4")
				)
				(pin bidirectional line
					(at 0 -111.76 0)
					(length 5.08)
					(name "PL44A")
					(number "N6")
				)
				(pin bidirectional line
					(at 0 -116.84 0)
					(length 5.08)
					(name "PL44B")
					(number "N7")
				)
				(pin bidirectional line
					(at 0 -114.3 0)
					(length 5.08)
					(name "PL44C")
					(number "P6")
				)
				(pin bidirectional line
					(at 0 -119.38 0)
					(length 5.08)
					(name "PL44D")
					(number "P7")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO7")
					(number "P10")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO7")
					(number "R10")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO7")
					(number "T10")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_9_1"
				(pin power_in line
					(at 25.4 0 180)
					(length 5.08)
					(name "VCCIO8")
					(number "AB10")
				)
				(pin passive line
					(at 25.4 0 180)
					(length 5.08)
					(hide yes)
					(name "VCCIO8")
					(number "AC10")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "PB4A")
					(number "AG1")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "PB13A")
					(number "AG3")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 5.08)
					(name "INITN")
					(number "AG4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "PB4B")
					(number "AH1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 5.08)
					(name "PB13B")
					(number "AH3")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 5.08)
					(name "PROGRAMN")
					(number "AH4")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "PB6A")
					(number "AJ1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "PB11A")
					(number "AJ2")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "PB15A")
					(number "AJ3")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 5.08)
					(name "DONE")
					(number "AJ4")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "PB6B")
					(number "AK1")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "PB11B")
					(number "AK2")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 5.08)
					(name "PB15B")
					(number "AK3")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 5.08)
					(name "CFG_2")
					(number "AK4")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "PB9A")
					(number "AL1")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 5.08)
					(name "PB18A")
					(number "AL3")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 5.08)
					(name "CFG_1")
					(number "AL4")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "PB9B")
					(number "AM2")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 5.08)
					(name "CCLK")
					(number "AM3")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 5.08)
					(name "CFG_0")
					(number "AM4")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_10_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "TDO")
					(number "AG5")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "TDI")
					(number "AJ5")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "TCK")
					(number "AK5")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "TMS")
					(number "AM5")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_11_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "HDTXP0_D0CH0")
					(number "AK9")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "HDTXN0_D0CH0")
					(number "AK10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "HDTXP0_D0CH1")
					(number "AK12")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "HDTXN0_D0CH1")
					(number "AK13")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "HDRXP0_D0CH0")
					(number "AM8")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "HDRXN0_D0CH0")
					(number "AM9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "HDRXP0_D0CH1")
					(number "AM11")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "HDRXN0_D0CH1")
					(number "AM12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "REFCLKP_D0")
					(number "AM14")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "REFCLKN_D0")
					(number "AM15")
				)
			)
			(symbol "ECP5_LFE5UM5G-85_12_1"
				(pin bidirectional line
					(at 0 0 0)
					(length 5.08)
					(name "HDTXP0_D1CH0")
					(number "AK18")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 5.08)
					(name "HDTXN0_D1CH0")
					(number "AK19")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 5.08)
					(name "HDTXP0_D1CH1")
					(number "AK21")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 5.08)
					(name "HDTXN0_D1CH1")
					(number "AK22")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 5.08)
					(name "HDRXP0_D1CH0")
					(number "AM17")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 5.08)
					(name "HDRXN0_D1CH0")
					(number "AM18")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 5.08)
					(name "HDRXP0_D1CH1")
					(number "AM20")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 5.08)
					(name "HDRXN0_D1CH1")
					(number "AM21")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 5.08)
					(name "REFCLKP_D1")
					(number "AM23")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 5.08)
					(name "REFCLKN_D1")
					(number "AM24")
				)
			)
			(embedded_fonts no)
		)
)
