(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "LFMXO5-55TD-8BBG256C"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 19.812 10.16 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "LFMXO5-55TD-8BBG256C"
				(at 19.812 5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "LFMXO5-55TD-8BBG256C"
				(at 19.812 2.54 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/6971/CertusPro-NX%20Family%20Datasheet.pdf"
				(at 19.812 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FPGA Lattice CertusPro -NX General Purpose Low-Power FPGA on Nexus platform (28nm FD-SOI)"
				(at 19.812 -12.7 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LFMXO5-55TD-8BBG256C"
				(at 19.812 7.62 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lattice Semiconductor"
				(at 19.812 -5.08 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 19.812 -7.62 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 19.812 -10.16 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_locked" ""
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "ki_keywords" "FPGA, IC, SMT"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "LFMXO5-55TD-8BBG256C_1_1")
			(symbol "LFMXO5-55TD-8BBG256C_2_1"
				(text "BANK 1"
					(at 10.16 1.524 0)
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "JTAG_EN")
					(number "D6")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PR13A")
					(number "E2")
					(alternate "PMU_EXT_CLK" input line)
					(alternate "SCLK" input line)
					(alternate "TCK" input line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PR11A")
					(number "E3")
					(alternate "S4_IN" input line)
					(alternate "SD3" input line)
					(alternate "SDA" bidirectional line)
					(alternate "USER_SDA" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PR10A")
					(number "E4")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PR3B")
					(number "E6")
					(alternate "S8_IN" input line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PR13B")
					(number "F2")
					(alternate "PMU_WAKEUPN" input line)
					(alternate "S4_OUT" output line)
					(alternate "SD11" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PR11B")
					(number "F3")
					(alternate "S3_IN" input line)
					(alternate "SCL" bidirectional line)
					(alternate "SD2" bidirectional line)
					(alternate "USER_SCL" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PR10B")
					(number "F4")
					(alternate "S3_OUT" output line)
					(alternate "SD1" bidirectional line)
					(alternate "SSO" output line)
					(alternate "TDO" output line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PR8B")
					(number "F5")
					(alternate "S5_OUT" output line)
					(alternate "SD0" bidirectional line)
					(alternate "SSI" input line)
					(alternate "TDI" input line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PR8A")
					(number "F6")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PR6A")
					(number "F7")
					(alternate "URC_GPLL0T_MFGOUT1" output line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PR4B")
					(number "F9")
					(alternate "SD10" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PR4A")
					(number "F10")
					(alternate "S8_OUT" output line)
					(alternate "URC_GPLL0_IN" input line)
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 3.81)
					(name "VCCIO1")
					(number "G1")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PR31A")
					(number "G2")
					(alternate "PCLKT1_0" input line)
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PR17B")
					(number "G3")
					(alternate "SD13" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PR17A")
					(number "G4")
					(alternate "SD12" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PR15B")
					(number "G5")
					(alternate "SD8" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PR15A")
					(number "G6")
					(alternate "SD9" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PR6B")
					(number "G7")
					(alternate "S5_IN" input line)
					(alternate "SCSN" input line)
					(alternate "TMS" input line)
					(alternate "URC_GPLL0T_MFGOUT2" output line)
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PR31B")
					(number "H1")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PR29B")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PR29A")
					(number "H3")
					(alternate "PCLKT1_1" input line)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PR28B")
					(number "H4")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PR28A")
					(number "H5")
					(alternate "PCLKT1_2" input line)
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PR19B")
					(number "H6")
					(alternate "SD15" bidirectional line)
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PR19A")
					(number "H7")
					(alternate "SD14" bidirectional line)
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_3_1"
				(text "BANK 2"
					(at 10.16 1.524 0)
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 3.81)
					(name "VCCIO2")
					(number "J1")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PR46B")
					(number "J2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PR46A")
					(number "J3")
					(alternate "PCLKT2_2" input line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PR44B")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PR44A")
					(number "J5")
					(alternate "PCLKT2_1" input line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PR42B")
					(number "J6")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PR42A")
					(number "J7")
					(alternate "PCLKT2_0" input line)
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_4_1"
				(text "BANK 3"
					(at 10.16 1.524 0)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PB154B")
					(number "L2")
					(alternate "ADC_CN15" input line)
					(alternate "LRC_GPLL0T_MFGOUT2" output line)
					(alternate "PCLKC3_3" input line)
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PB154A")
					(number "L3")
					(alternate "ADC_CP15" input line)
					(alternate "LRC_GPLL0T_MFGOUT1" output line)
					(alternate "PCLKT3_3" input line)
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PB152A")
					(number "L4")
					(alternate "ADC_CP12" input line)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PB156B")
					(number "M1")
					(alternate "ATB_SENSE" input line)
					(alternate "LRC_GPLL0C_IN" input line)
					(alternate "VREF3_2" input line)
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PB156A")
					(number "M2")
					(alternate "ATB_FORCE" output line)
					(alternate "LRC_GPLL0T_IN" input line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PB146A")
					(number "M3")
					(alternate "ADC_CP14" input line)
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PB152B")
					(number "M4")
					(alternate "ADC_CN12" input line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PB116A")
					(number "M5")
					(alternate "ADC_CP8" input line)
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PB150B")
					(number "N1")
					(alternate "ADC_CN11" input line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PB148A")
					(number "N2")
					(alternate "COMP3IP" input line)
					(alternate "PCLKT3_2" input line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PB146B")
					(number "N3")
					(alternate "ADC_CN14" input line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PB116B")
					(number "N4")
					(alternate "ADC_CN8" input line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PB112A")
					(number "N5")
					(alternate "ADC_CP4" input line)
					(alternate "PCLKT3_0" input line)
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PB150A")
					(number "P1")
					(alternate "ADC_CP11" input line)
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PB148B")
					(number "P2")
					(alternate "COMP3IN" input line)
					(alternate "PCLKC3_2" input line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PB118A")
					(number "P3")
					(alternate "COMP2IP" input line)
					(alternate "PCLKT3_1" input line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PB118B")
					(number "P4")
					(alternate "COMP2IN" input line)
					(alternate "PCLKC3_1" input line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PB112B")
					(number "P5")
					(alternate "ADC_CN4" input line)
					(alternate "PCLKC3_0" input line)
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 3.81)
					(name "VCCIO3")
					(number "R1")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PB120A")
					(number "R2")
					(alternate "ADC_CP13" input line)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PB120B")
					(number "R3")
					(alternate "ADC_CN13" input line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PB110B")
					(number "R4")
					(alternate "ADC_CN10" input line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PB110A")
					(number "R5")
					(alternate "ADC_CP10" input line)
					(alternate "VREF3_1" input line)
				)
				(pin passive line
					(at 27.94 0 180)
					(length 3.81)
					(hide yes)
					(name "VCCIO3")
					(number "T2")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PB114A")
					(number "T3")
					(alternate "COMP1IP" input line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PB114B")
					(number "T4")
					(alternate "COMP1IP" input line)
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_5_1"
				(text "BANK 4"
					(at 10.16 1.524 0)
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PB60B")
					(number "K9")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PB50A")
					(number "K10")
					(alternate "VREF4_1" input line)
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PB98A")
					(number "L7")
					(alternate "ADC_CP5" input line)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PB60A")
					(number "L9")
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PB50B")
					(number "L10")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PB104A")
					(number "M6")
					(alternate "ADC_CP9" input line)
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PB98B")
					(number "M7")
					(alternate "ADC_CN5" input line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PB58B")
					(number "M9")
					(alternate "PCLKC4_1" input line)
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PB104B")
					(number "N6")
					(alternate "ADC_CN9" input line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PB58A")
					(number "N9")
					(alternate "PCLKT4_1" input line)
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PB106A")
					(number "P6")
					(alternate "PCLKT4_3" input line)
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PB100A")
					(number "P8")
					(alternate "ADC_CP7" input line)
					(alternate "PCLKT4_2" input line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PB56B")
					(number "P9")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PB52A")
					(number "P10")
					(alternate "PCLKT4_0" input line)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PB106B")
					(number "R6")
					(alternate "PCLKC4_3" input line)
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 3.81)
					(name "VCCIO4")
					(number "R7")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PB100B")
					(number "R8")
					(alternate "ADC_CN7" input line)
					(alternate "PCLKC4_2" input line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PB56A")
					(number "R9")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PB52B")
					(number "R10")
					(alternate "PCLKC4_0" input line)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PB108B")
					(number "T5")
					(alternate "VREF4_2" input line)
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PB108A")
					(number "T6")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PB102B")
					(number "T7")
					(alternate "ADC_CN6" input line)
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PB102A")
					(number "T8")
					(alternate "ADC_CP6" input line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PB54B")
					(number "T9")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PB54A")
					(number "T10")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 3.81)
					(hide yes)
					(name "VCCIO4")
					(number "T11")
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_6_1"
				(text "BANK 5"
					(at 10.16 1.524 0)
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PB12A")
					(number "K11")
					(alternate "CDR1_TESTP" input line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PB4B")
					(number "K12")
					(alternate "ADC_CN1" input line)
					(alternate "CDR_RXN1" input line)
					(alternate "COMP2N" input line)
					(alternate "LLC_GPLL0T_MFGOUT2" output line)
					(alternate "PCLKC5_0" input line)
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PB8A")
					(number "K13")
					(alternate "ADC_CP3" input line)
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PB10B")
					(number "K14")
					(alternate "ADC_CN2" input line)
					(alternate "CDR0_TESTN" input line)
					(alternate "COMP3N" input line)
					(alternate "PCLKC5_1" input line)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PB2A")
					(number "K15")
					(alternate "ADC_CP0" input line)
					(alternate "CDR_RXP0" input line)
					(alternate "COMP1P" input line)
					(alternate "LLC_GPLL0T_IN" input line)
					(alternate "VREF5_1" input line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PB6A")
					(number "K16")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PB12B")
					(number "L11")
					(alternate "CDR1_TESTN" input line)
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PB4A")
					(number "L12")
					(alternate "ADC_CP1" input line)
					(alternate "CDR_RXP1" input line)
					(alternate "COMP2P" input line)
					(alternate "LLC_GPLL0T_MFGOUT1" output line)
					(alternate "PCLKT5_0" input line)
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PB8B")
					(number "L13")
					(alternate "ADC_CN3" input line)
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PB10A")
					(number "L14")
					(alternate "ADC_CP2" input line)
					(alternate "CDR0_TESTP" input line)
					(alternate "COMP3P" input line)
					(alternate "PCLKT5_1" input line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PB2B")
					(number "L15")
					(alternate "ADC_CN0" input line)
					(alternate "CDR_RXN0" input line)
					(alternate "COMP1N" input line)
					(alternate "LLC_GPLL0C_IN" input line)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PB6B")
					(number "L16")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "PB48B")
					(number "M11")
					(alternate "VREF5_2" input line)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PB36B")
					(number "M12")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PB36A")
					(number "M13")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PB28A")
					(number "M14")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PB26B")
					(number "M15")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PB26A")
					(number "M16")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "PB48A")
					(number "N11")
				)
				(pin bidirectional line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PB44A")
					(number "N12")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PB34B")
					(number "N13")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PB34A")
					(number "N14")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PB28B")
					(number "N15")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PB30A")
					(number "N16")
				)
				(pin bidirectional line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PB44B")
					(number "P12")
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PB38B")
					(number "P13")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PB38A")
					(number "P14")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PB32A")
					(number "P15")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PB30B")
					(number "P16")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "PB46A")
					(number "R12")
					(alternate "PCLKT5_3" input line)
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PB40B")
					(number "R13")
					(alternate "PCLKC5_2" input line)
				)
				(pin bidirectional line
					(at 0 -66.04 0)
					(length 3.81)
					(name "PB40A")
					(number "R14")
					(alternate "PCLKT5_2" input line)
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PB32B")
					(number "R15")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 3.81)
					(name "VCCIO5")
					(number "R16")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "PB46B")
					(number "T12")
					(alternate "PCLKC5_3" input line)
				)
				(pin bidirectional line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PB42B")
					(number "T13")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PB42A")
					(number "T14")
				)
				(pin passive line
					(at 27.94 0 180)
					(length 3.81)
					(hide yes)
					(name "VCCIO5")
					(number "T15")
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_7_1"
				(text "BANK 6"
					(at 10.16 1.524 0)
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PL46B")
					(number "J8")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PL46A")
					(number "J9")
					(alternate "PCLKT6_2" input line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PL44B")
					(number "J10")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PL44A")
					(number "J11")
					(alternate "PCLKT6_1" input line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PL42B")
					(number "J12")
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PL42A")
					(number "J13")
					(alternate "PCLKT6_0" input line)
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 3.81)
					(name "VCCIO6")
					(number "J16")
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_8_1"
				(text "BANK 7"
					(at 10.16 1.524 0)
				)
				(pin bidirectional line
					(at 0 0 0)
					(length 3.81)
					(name "PL3A")
					(number "D15")
					(alternate "EIO" bidirectional line)
					(alternate "ULC_GPLL0_IN" input line)
				)
				(pin bidirectional line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PL3B")
					(number "D16")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PL4A")
					(number "E12")
					(alternate "ULC_GPLL0T_MFGOUT1" output line)
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PL4B")
					(number "E13")
					(alternate "ULC_GPLL0T_MFGOUT2" output line)
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PL6A")
					(number "E14")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PL6B")
					(number "E15")
				)
				(pin bidirectional line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PL11A")
					(number "E16")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PL8A")
					(number "F11")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PL8B")
					(number "F12")
				)
				(pin bidirectional line
					(at 0 -20.32 0)
					(length 3.81)
					(name "PL10A")
					(number "F13")
				)
				(pin bidirectional line
					(at 0 -22.86 0)
					(length 3.81)
					(name "PL10B")
					(number "F14")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PL19A")
					(number "F15")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PL11B")
					(number "F16")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PL13A")
					(number "G9")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PL13B")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PL15A")
					(number "G11")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PL15B")
					(number "G12")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PL17A")
					(number "G13")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PL17B")
					(number "G14")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PL19B")
					(number "G15")
				)
				(pin power_in line
					(at 27.94 0 180)
					(length 3.81)
					(name "VCCIO7")
					(number "G16")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PL28A")
					(number "H9")
					(alternate "PCLKT7_2" input line)
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PL28B")
					(number "H10")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PL29A")
					(number "H11")
					(alternate "PCLKT7_1" input line)
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PL29B")
					(number "H12")
				)
				(pin bidirectional line
					(at 0 -60.96 0)
					(length 3.81)
					(name "PL31A")
					(number "H13")
					(alternate "PCLKT7_0" input line)
				)
				(pin bidirectional line
					(at 0 -63.5 0)
					(length 3.81)
					(name "PL31B")
					(number "H14")
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_9_1"
				(text "ADC"
					(at 14.224 1.524 0)
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "ADC_REFP1")
					(number "K5")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "ADC_DP1")
					(number "K6")
				)
				(pin input line
					(at 0 -5.08 0)
					(length 3.81)
					(name "ADC_DP0")
					(number "K7")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "ADC_DN0")
					(number "K8")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "ADC_REFP0")
					(number "L5")
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "ADC_DN1")
					(number "L6")
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_10_1"
				(text "SERDES QUAD 0"
					(at 13.97 1.524 0)
				)
				(pin input line
					(at 0 -12.7 0)
					(length 3.81)
					(name "SD_EXT1_REFCLKP")
					(number "A2")
				)
				(pin output line
					(at 44.45 -45.72 180)
					(length 3.81)
					(name "SD3_TXDN")
					(number "A5")
				)
				(pin output line
					(at 44.45 -43.18 180)
					(length 3.81)
					(name "SD3_TXDP")
					(number "A6")
				)
				(pin output line
					(at 44.45 -38.1 180)
					(length 3.81)
					(name "SD2_TXDN")
					(number "A8")
				)
				(pin output line
					(at 44.45 -35.56 180)
					(length 3.81)
					(name "SD2_TXDP")
					(number "A9")
				)
				(pin output line
					(at 44.45 -30.48 180)
					(length 3.81)
					(name "SD1_TXDN")
					(number "A11")
				)
				(pin output line
					(at 44.45 -27.94 180)
					(length 3.81)
					(name "SD1_TXDP")
					(number "A12")
				)
				(pin output line
					(at 44.45 -22.86 180)
					(length 3.81)
					(name "SD0_TXDN")
					(number "A14")
				)
				(pin output line
					(at 44.45 -20.32 180)
					(length 3.81)
					(name "SD0_TXDP")
					(number "A15")
				)
				(pin input line
					(at 0 -15.24 0)
					(length 3.81)
					(name "SD_EXT1_REFCLKN")
					(number "B1")
				)
				(pin input line
					(at 0 -7.62 0)
					(length 3.81)
					(name "SD_EXT0_REFCLKP")
					(number "B2")
				)
				(pin input line
					(at 0 -10.16 0)
					(length 3.81)
					(name "SD_EXT0_REFCLKN")
					(number "B3")
				)
				(pin input line
					(at 0 -38.1 0)
					(length 3.81)
					(name "SD2_RXDN")
					(number "B7")
				)
				(pin input line
					(at 0 -30.48 0)
					(length 3.81)
					(name "SD1_RXDN")
					(number "B10")
				)
				(pin input line
					(at 0 -22.86 0)
					(length 3.81)
					(name "SD0_RXDN")
					(number "B13")
				)
				(pin input line
					(at 0 -43.18 0)
					(length 3.81)
					(name "SD3_RXDP")
					(number "C5")
				)
				(pin input line
					(at 0 -45.72 0)
					(length 3.81)
					(name "SD3_RXDN")
					(number "C6")
				)
				(pin input line
					(at 0 -35.56 0)
					(length 3.81)
					(name "SD2_RXDP")
					(number "C8")
				)
				(pin input line
					(at 0 -27.94 0)
					(length 3.81)
					(name "SD1_RXDP")
					(number "C11")
				)
				(pin input line
					(at 0 -20.32 0)
					(length 3.81)
					(name "SD0_RXDP")
					(number "C14")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "SDQ0_REFCLKP")
					(number "D10")
				)
				(pin input line
					(at 0 -2.54 0)
					(length 3.81)
					(name "SDQ0_REFCLKN")
					(number "E10")
				)
			)
			(symbol "LFMXO5-55TD-8BBG256C_11_1"
				(pin power_in line
					(at 0 -44.45 0)
					(length 3.81)
					(name "VSSSDQ")
					(number "A1")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "A3")
				)
				(pin power_in line
					(at 34.29 0 180)
					(length 3.81)
					(name "VCCAUXSDQ0")
					(number "A4")
				)
				(pin power_in line
					(at 34.29 -41.91 180)
					(length 3.81)
					(name "VCCSD3")
					(number "A7")
				)
				(pin power_in line
					(at 34.29 -30.48 180)
					(length 3.81)
					(name "VCCSD2")
					(number "A10")
				)
				(pin power_in line
					(at 34.29 -19.05 180)
					(length 3.81)
					(name "VCCSD1")
					(number "A13")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "A16")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "B4")
				)
				(pin power_in line
					(at 34.29 -44.45 180)
					(length 3.81)
					(name "VCCPLLSD3")
					(number "B5")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "B6")
				)
				(pin power_in line
					(at 34.29 -33.02 180)
					(length 3.81)
					(name "VCCPLLSD2")
					(number "B8")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "B9")
				)
				(pin power_in line
					(at 34.29 -21.59 180)
					(length 3.81)
					(name "VCCPLLSD1")
					(number "B11")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "B12")
				)
				(pin power_in line
					(at 34.29 -10.16 180)
					(length 3.81)
					(name "VCCPLLSD0")
					(number "B14")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "B15")
				)
				(pin power_in line
					(at 34.29 -7.62 180)
					(length 3.81)
					(name "VCCSD0")
					(number "B16")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "C7")
				)
				(pin input line
					(at 34.29 -38.1 180)
					(length 3.81)
					(name "SD2_REFRET")
					(number "C9")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "C10")
				)
				(pin input line
					(at 34.29 -26.67 180)
					(length 3.81)
					(name "SD1_REFRET")
					(number "C12")
				)
				(pin input line
					(at 34.29 -24.13 180)
					(length 3.81)
					(name "SD1_REXT")
					(number "C13")
				)
				(pin input line
					(at 34.29 -15.24 180)
					(length 3.81)
					(name "SD0_REFRET")
					(number "C15")
				)
				(pin input line
					(at 34.29 -12.7 180)
					(length 3.81)
					(name "SD0_REXT")
					(number "C16")
				)
				(pin input line
					(at 34.29 -49.53 180)
					(length 3.81)
					(name "SD3_REFRET")
					(number "D8")
				)
				(pin input line
					(at 34.29 -35.56 180)
					(length 3.81)
					(name "SD2_REXT")
					(number "D9")
				)
				(pin power_in line
					(at 34.29 -3.81 180)
					(length 3.81)
					(name "VCCSDCK")
					(number "D11")
				)
				(pin power_in line
					(at 0 -49.53 0)
					(length 3.81)
					(name "VSS")
					(number "D12")
				)
				(pin power_in line
					(at 0 -10.16 0)
					(length 3.81)
					(name "VCCAUXA")
					(number "D13")
					(alternate "VCCAUX" power_in line)
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "D14")
				)
				(pin input line
					(at 34.29 -46.99 180)
					(length 3.81)
					(name "SD3_REXT")
					(number "E8")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "E9")
				)
				(pin passive line
					(at 0 -44.45 0)
					(length 3.81)
					(hide yes)
					(name "VSSSDQ")
					(number "E11")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "F1")
				)
				(pin power_in line
					(at 0 0 0)
					(length 3.81)
					(name "VCC")
					(number "F8")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "G8")
				)
				(pin power_in line
					(at 0 -7.62 0)
					(length 3.81)
					(name "VCCAUX")
					(number "H8")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "H15")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "H16")
				)
				(pin passive line
					(at 0 -7.62 0)
					(length 3.81)
					(hide yes)
					(name "VCCAUX")
					(number "J14")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "J15")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "K1")
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "K2")
				)
				(pin power_in line
					(at 0 -46.99 0)
					(length 3.81)
					(name "VSSADC")
					(number "K3")
				)
				(pin power_in line
					(at 0 -30.48 0)
					(length 3.81)
					(name "VCCADC18")
					(number "K4")
				)
				(pin power_in line
					(at 0 -12.7 0)
					(length 3.81)
					(name "VCCAUXH3")
					(number "L1")
					(alternate "VCCAUX" power_in line)
				)
				(pin passive line
					(at 0 0 0)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "L8")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M8")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "M10")
				)
				(pin power_in line
					(at 0 -15.24 0)
					(length 3.81)
					(name "VCCAUXH4")
					(number "N7")
					(alternate "VCCAUX" power_in line)
				)
				(pin passive line
					(at 0 -3.81 0)
					(length 3.81)
					(hide yes)
					(name "VCCECLK")
					(number "N8")
					(alternate "VCC" power_in line)
				)
				(pin power_in line
					(at 0 -3.81 0)
					(length 3.81)
					(name "VCCECLK")
					(number "N10")
					(alternate "VCC" power_in line)
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "P7")
				)
				(pin power_in line
					(at 0 -17.78 0)
					(length 3.81)
					(name "VCCAUXH5")
					(number "P11")
					(alternate "VCCAUX" power_in line)
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "R11")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "T1")
				)
				(pin passive line
					(at 0 -49.53 0)
					(length 3.81)
					(hide yes)
					(name "VSS")
					(number "T16")
				)
			)
			(embedded_fonts no)
		)
)
