(kicad_symbol_lib
	(version 20260206)
	(generator "partreel-import")
		(symbol "CrossLink_LIF-MD6000-6JMG80I"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(in_pos_files yes)
			(duplicate_pin_numbers_are_jumpers no)
			(property "Reference" "U"
				(at 78.74 -6.35 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Value" "CrossLink_LIF-MD6000-6JMG80I"
				(at 78.74 -11.43 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Footprint" "CrossLink_LIF-MD6000-6JMG80I"
				(at 78.74 -13.97 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Datasheet" "https://www.latticesemi.com/view_document?document_id=51662"
				(at 78.74 -16.51 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Description" "FPGA, CrossLink, PLL37 I/O, 400 MHz, 5936 Cells, 1.14 V to 1.26 V, CTFBGA-80"
				(at 78.74 -26.67 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "MPN" "LIF-MD6000-6JMG80I"
				(at 78.74 -8.89 0)
				(show_name no)
				(do_not_autoplace no)
			)
			(property "Manufacturer" "Lattice Semiconductor"
				(at 78.74 -19.05 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "Author" "Antmicro"
				(at 78.74 -21.59 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "License" "Apache-2.0"
				(at 78.74 -24.13 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(property "ki_keywords" "SMT, FPGA, IC, RoHS"
				(at 0 0 0)
				(show_name no)
				(do_not_autoplace no)
				(hide yes)
			)
			(symbol "CrossLink_LIF-MD6000-6JMG80I_1_1"
				(text "Bank_1"
					(at 27.94 -30.48 900)
				)
				(text "Bank_2"
					(at 27.94 -73.66 900)
				)
				(text "Bank_0"
					(at 34.29 -5.08 900)
				)
				(text "DPHY0"
					(at 44.45 -46.99 900)
				)
				(text "DPHY1"
					(at 44.45 -85.09 900)
				)
				(pin bidirectional line
					(at 63.5 -71.12 180)
					(length 3.81)
					(name "DPHY1_DN2")
					(number "A1")
				)
				(pin bidirectional line
					(at 63.5 -60.96 180)
					(length 3.81)
					(name "DPHY1_DN0")
					(number "A2")
				)
				(pin bidirectional line
					(at 63.5 -55.88 180)
					(length 3.81)
					(name "DPHY1_CKN")
					(number "A3")
				)
				(pin bidirectional line
					(at 63.5 -66.04 180)
					(length 3.81)
					(name "DPHY1_DN1")
					(number "A4")
				)
				(pin bidirectional line
					(at 63.5 -76.2 180)
					(length 3.81)
					(name "DPHY1_DN3")
					(number "A5")
				)
				(pin bidirectional line
					(at 63.5 -33.02 180)
					(length 3.81)
					(name "DPHY0_DN2")
					(number "A6")
				)
				(pin bidirectional line
					(at 63.5 -22.86 180)
					(length 3.81)
					(name "DPHY0_DN0")
					(number "A7")
				)
				(pin bidirectional line
					(at 63.5 -17.78 180)
					(length 3.81)
					(name "DPHY0_CKN")
					(number "A8")
				)
				(pin bidirectional line
					(at 63.5 -27.94 180)
					(length 3.81)
					(name "DPHY0_DN1")
					(number "A9")
				)
				(pin bidirectional line
					(at 63.5 -38.1 180)
					(length 3.81)
					(name "DPHY0_DN3")
					(number "A10")
				)
				(pin bidirectional line
					(at 63.5 -68.58 180)
					(length 3.81)
					(name "DPHY1_DP2")
					(number "B1")
				)
				(pin bidirectional line
					(at 63.5 -58.42 180)
					(length 3.81)
					(name "DPHY1_DP0")
					(number "B2")
				)
				(pin bidirectional line
					(at 63.5 -53.34 180)
					(length 3.81)
					(name "DPHY1_CKP")
					(number "B3")
				)
				(pin bidirectional line
					(at 63.5 -63.5 180)
					(length 3.81)
					(name "DPHY1_DP1")
					(number "B4")
				)
				(pin bidirectional line
					(at 63.5 -73.66 180)
					(length 3.81)
					(name "DPHY1_DP3")
					(number "B5")
				)
				(pin bidirectional line
					(at 63.5 -30.48 180)
					(length 3.81)
					(name "DPHY0_DP2")
					(number "B6")
				)
				(pin bidirectional line
					(at 63.5 -20.32 180)
					(length 3.81)
					(name "DPHY0_DP0")
					(number "B7")
				)
				(pin bidirectional line
					(at 63.5 -15.24 180)
					(length 3.81)
					(name "DPHY0_CKP")
					(number "B8")
				)
				(pin bidirectional line
					(at 63.5 -25.4 180)
					(length 3.81)
					(name "DPHY0_DP1")
					(number "B9")
				)
				(pin bidirectional line
					(at 63.5 -35.56 180)
					(length 3.81)
					(name "DPHY0_DP3")
					(number "B10")
				)
				(pin power_in line
					(at 63.5 -106.68 180)
					(length 3.81)
					(name "GND")
					(number "C1")
				)
				(pin power_in line
					(at 63.5 -78.74 180)
					(length 3.81)
					(name "GNDA_DPHY1")
					(number "C2")
				)
				(pin power_in line
					(at 63.5 -40.64 180)
					(length 3.81)
					(name "GNDA_DPHY0")
					(number "C9")
				)
				(pin passive line
					(at 63.5 -106.68 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "C10")
				)
				(pin bidirectional line
					(at 0 -5.08 0)
					(length 3.81)
					(name "PB48/PCLKT0_1/USER_SCL")
					(number "D1")
				)
				(pin power_in line
					(at 63.5 -83.82 180)
					(length 3.81)
					(name "VCCPLL_DPHY1")
					(number "D2")
				)
				(pin power_in line
					(at 63.5 -81.28 180)
					(length 3.81)
					(name "VCCA_DPHY1")
					(number "D4")
				)
				(pin power_in line
					(at 63.5 -5.08 180)
					(length 3.81)
					(name "VCCAUX")
					(number "D5")
				)
				(pin power_in line
					(at 63.5 -101.6 180)
					(length 3.81)
					(name "GNDPLL_DPHY_X")
					(number "D6")
				)
				(pin bidirectional line
					(at 63.5 -45.72 180)
					(length 3.81)
					(name "VCCPLL_DPHY0")
					(number "D7")
				)
				(pin bidirectional line
					(at 0 -68.58 0)
					(length 3.81)
					(name "PB16A/PCLKT2_0")
					(number "D9")
				)
				(pin bidirectional line
					(at 0 -71.12 0)
					(length 3.81)
					(name "PB16B/PCLKC2_0")
					(number "D10")
				)
				(pin input line
					(at 0 -25.4 0)
					(length 3.81)
					(name "PB34A/GR_PCLK1_0")
					(number "E1")
				)
				(pin bidirectional line
					(at 0 -27.94 0)
					(length 3.81)
					(name "PB34B")
					(number "E2")
				)
				(pin power_in line
					(at 63.5 0 180)
					(length 3.81)
					(name "VCC")
					(number "E4")
				)
				(pin passive line
					(at 63.5 -106.68 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "E5")
				)
				(pin passive line
					(at 63.5 0 180)
					(length 3.81)
					(hide yes)
					(name "VCC")
					(number "E6")
				)
				(pin power_in line
					(at 63.5 -43.18 180)
					(length 3.81)
					(name "VCCA_DPHY0")
					(number "E7")
				)
				(pin input line
					(at 0 -73.66 0)
					(length 3.81)
					(name "PB12A/GPLLT2_0")
					(number "E9")
				)
				(pin input line
					(at 0 -76.2 0)
					(length 3.81)
					(name "PB12B/GPLLC2_0")
					(number "E10")
				)
				(pin bidirectional line
					(at 0 -30.48 0)
					(length 3.81)
					(name "PB38A")
					(number "F1")
				)
				(pin bidirectional line
					(at 0 -33.02 0)
					(length 3.81)
					(name "PB38B")
					(number "F2")
				)
				(pin power_in line
					(at 0 -20.32 0)
					(length 3.81)
					(name "VCCIO0")
					(number "F4")
				)
				(pin power_in line
					(at 0 -60.96 0)
					(length 3.81)
					(name "VCCIO1")
					(number "F5")
				)
				(pin power_in line
					(at 0 -109.22 0)
					(length 3.81)
					(name "VCCIO2")
					(number "F6")
				)
				(pin passive line
					(at 0 -109.22 0)
					(length 3.81)
					(hide yes)
					(name "VCCIO2")
					(number "F7")
				)
				(pin input line
					(at 0 -78.74 0)
					(length 3.81)
					(name "PB6A/GR_PCLK2_0")
					(number "F9")
				)
				(pin bidirectional line
					(at 0 -81.28 0)
					(length 3.81)
					(name "PB6B")
					(number "F10")
				)
				(pin bidirectional line
					(at 0 -10.16 0)
					(length 3.81)
					(name "PB50/MOSI")
					(number "G1")
				)
				(pin passive line
					(at 63.5 -106.68 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G2")
				)
				(pin passive line
					(at 0 -60.96 0)
					(length 3.81)
					(hide yes)
					(name "VCCIO1")
					(number "G4")
				)
				(pin passive line
					(at 63.5 -106.68 180)
					(length 3.81)
					(hide yes)
					(name "GND")
					(number "G5")
				)
				(pin power_in line
					(at 63.5 -10.16 180)
					(length 3.81)
					(name "VCCGPLL")
					(number "G6")
				)
				(pin power_in line
					(at 63.5 -104.14 180)
					(length 3.81)
					(name "GNDGPLL")
					(number "G7")
				)
				(pin bidirectional line
					(at 0 -83.82 0)
					(length 3.81)
					(name "PB2A")
					(number "G9")
				)
				(pin bidirectional line
					(at 0 -86.36 0)
					(length 3.81)
					(name "PB2B")
					(number "G10")
				)
				(pin bidirectional line
					(at 0 -12.7 0)
					(length 3.81)
					(name "PB52/SPI_SS/CSN/SCL")
					(number "H1")
				)
				(pin input line
					(at 0 0 0)
					(length 3.81)
					(name "CRESET_B")
					(number "H2")
				)
				(pin bidirectional line
					(at 0 -88.9 0)
					(length 3.81)
					(name "PB2D/MIPI_CLKC2_0")
					(number "H9")
				)
				(pin bidirectional line
					(at 0 -91.44 0)
					(length 3.81)
					(name "PB2C/MIPI_CLKT2_0")
					(number "H10")
				)
				(pin bidirectional line
					(at 0 -15.24 0)
					(length 3.81)
					(name "PB53/SPI_SCK/MCK/SDA")
					(number "J1")
				)
				(pin passive line
					(at 0 -2.54 0)
					(length 3.81)
					(name "PB49/PMU_WKUPN/CDONE")
					(number "J2")
				)
				(pin bidirectional line
					(at 0 -45.72 0)
					(length 3.81)
					(name "PB43D")
					(number "J3")
				)
				(pin bidirectional line
					(at 0 -43.18 0)
					(length 3.81)
					(name "PB38D")
					(number "J4")
				)
				(pin bidirectional line
					(at 0 -40.64 0)
					(length 3.81)
					(name "PB34D/MIPI_CLKC1_0")
					(number "J5")
				)
				(pin bidirectional line
					(at 0 -38.1 0)
					(length 3.81)
					(name "PB29D/PCLKC1_1")
					(number "J6")
				)
				(pin bidirectional line
					(at 0 -35.56 0)
					(length 3.81)
					(name "PB29A/PCLKT1_0")
					(number "J7")
				)
				(pin bidirectional line
					(at 0 -93.98 0)
					(length 3.81)
					(name "PB16D/PCLKC2_1")
					(number "J8")
				)
				(pin bidirectional line
					(at 0 -96.52 0)
					(length 3.81)
					(name "PB6D")
					(number "J9")
				)
				(pin bidirectional line
					(at 0 -99.06 0)
					(length 3.81)
					(name "PB6C")
					(number "J10")
				)
				(pin bidirectional line
					(at 0 -17.78 0)
					(length 3.81)
					(name "PB51/MISO")
					(number "K1")
				)
				(pin bidirectional line
					(at 0 -7.62 0)
					(length 3.81)
					(name "PB47/PCLKT0_0/USER_SDA")
					(number "K2")
				)
				(pin bidirectional line
					(at 0 -58.42 0)
					(length 3.81)
					(name "PB43C")
					(number "K3")
				)
				(pin bidirectional line
					(at 0 -55.88 0)
					(length 3.81)
					(name "PB38C")
					(number "K4")
				)
				(pin bidirectional line
					(at 0 -53.34 0)
					(length 3.81)
					(name "PB34C/MIPI_CLKT1_0")
					(number "K5")
				)
				(pin bidirectional line
					(at 0 -50.8 0)
					(length 3.81)
					(name "PB29C/PCLKT1_1")
					(number "K6")
				)
				(pin bidirectional line
					(at 0 -48.26 0)
					(length 3.81)
					(name "PB29B/PCLKC1_0")
					(number "K7")
				)
				(pin bidirectional line
					(at 0 -101.6 0)
					(length 3.81)
					(name "PB16C/PCLKT2_1")
					(number "K8")
				)
				(pin bidirectional line
					(at 0 -104.14 0)
					(length 3.81)
					(name "PB12D")
					(number "K9")
				)
				(pin bidirectional line
					(at 0 -106.68 0)
					(length 3.81)
					(name "PB12C")
					(number "K10")
				)
			)
			(embedded_fonts no)
		)
)
